(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 238)
    (zones 0)
    (modules 9)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu power)
    (3 In3.Cu signal)
    (4 In4.Cu signal)
    (5 In5.Cu signal)
    (6 In6.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.2)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.3048)
    (via_min_drill 0.2)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.6 4.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00000_7fffff82)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../../"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad5)")
  (net 3 "Net-(J2-Pad6)")
  (net 4 "Net-(J2-Pad7)")
  (net 5 "Net-(J2-Pad8)")
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J3-Pad3)")
  (net 9 "Net-(J3-Pad4)")
  (net 10 "Net-(J3-Pad5)")
  (net 11 "Net-(J3-Pad6)")
  (net 12 "Net-(J3-Pad7)")
  (net 13 "Net-(J3-Pad9)")
  (net 14 "Net-(J3-Pad11)")
  (net 15 "Net-(J3-Pad13)")
  (net 16 "Net-(J3-Pad15)")
  (net 17 "Net-(J3-Pad19)")
  (net 18 "Net-(J3-Pad23)")
  (net 19 "Net-(J3-Pad27)")
  (net 20 "Net-(J3-Pad31)")
  (net 21 "Net-(J3-Pad35)")
  (net 22 "Net-(J3-Pad37)")
  (net 23 "Net-(J3-Pad39)")
  (net 24 "Net-(U1-Pad15)")
  (net 25 "Net-(U1-Pad4)")
  (net 26 "Net-(U1-Pad9)")
  (net 27 "Net-(U1-Pad33)")
  (net 28 "Net-(U1-Pad28)")
  (net 29 GND)
  (net 30 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad23)")
    (add_net "Net-(J3-Pad27)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad9)")
    (add_net VCC)
  )
  (net_class New ""
    (clearance 0.1)
    (trace_width 0.1524)
    (via_dia 0.3048)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad31)")
    (add_net "Net-(J3-Pad35)")
    (add_net "Net-(J3-Pad37)")
    (add_net "Net-(J3-Pad39)")
  )
  (module AWMF:AWMF-0108 (layer F.Cu) (tedit 5C250EFD)
    (at 135.580001 107.950001)
    (fp_text reference U1 (at 0.119999 -4.800001) (layer F.SilkS))
    (fp_text value AWMF-0108A- (at 0.219999 5.349999) (layer F.Fab))
    (pad 24 smd oval (at 2.2 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 23 smd oval (at 1.8 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 22 smd oval (at 1.4 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 21 smd oval (at 1 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 20 smd oval (at 0.6 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 19 smd oval (at 0.2 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 18 smd oval (at -0.2 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 17 smd oval (at -0.6 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 16 smd oval (at -1 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 15 smd oval (at -1.4 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad15)"))
    (pad 14 smd oval (at -1.8 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 13 smd oval (at -2.2 2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 25 smd oval (at 2.8 2.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 26 smd oval (at 2.8 1.8 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 27 smd oval (at 2.8 1.4 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 28 smd oval (at 2.8 1 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad28)"))
    (pad 29 smd oval (at 2.8 0.6 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 30 smd oval (at 2.8 0.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 31 smd oval (at 2.8 -0.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 32 smd oval (at 2.8 -0.6 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 33 smd oval (at 2.8 -1 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad33)"))
    (pad 34 smd oval (at 2.8 -1.4 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 35 smd oval (at 2.8 -1.8 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 36 smd oval (at 2.8 -2.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 37- smd oval (at 2.2 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad35)"))
    (pad 38+ smd oval (at 1.8 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad37)"))
    (pad 39- smd oval (at 1.4 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad39)"))
    (pad 40 smd oval (at 1 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad11)"))
    (pad 41 smd oval (at 0.6 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad13)"))
    (pad 42 smd oval (at 0.2 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 43 smd oval (at -0.2 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 44- smd oval (at -0.6 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad27)"))
    (pad 45+ smd oval (at -1 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad23)"))
    (pad 46 smd oval (at -1.4 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad31)"))
    (pad 47 smd oval (at -1.8 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad19)"))
    (pad 48- smd oval (at -2.2 -2.8) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad15)"))
    (pad 12 smd oval (at -2.8 2.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 11 smd oval (at -2.8 1.8 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 10 smd oval (at -2.8 1.4 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 9 smd oval (at -2.8 1 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad9)"))
    (pad 8 smd oval (at -2.8 0.6 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 7 smd oval (at -2.8 0.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 6 smd oval (at -2.8 -0.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 5 smd oval (at -2.8 -0.6 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 4 smd oval (at -2.8 -1 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad4)"))
    (pad 3 smd oval (at -2.8 -1.4 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 2 smd oval (at -2.8 -1.8 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 2 smd oval (at -2.8 -1.8 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 1 smd oval (at -2.8 -2.2 270) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 49 smd rect (at 0 0) (size 4.6 4.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.695 113.03 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value GRM1555C1H102JA01D (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 -0.065413 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 VCC))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.75 113.03 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value GRM1555C1H200JA01D (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tantalum-T491D227K010AT:T491D227K010AT (layer F.Cu) (tedit 5C1F8A51)
    (at 160.06064 118.491 90)
    (descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C3 (at 0 -3.1 90) (layer F.SilkS))
    (fp_text value T491D227K010At (at 0 3.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.1125 0 90) (size 2.075 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 29 GND))
    (pad 2 smd roundrect (at 2.9 -0.025 90) (size 2.075 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 153.67 113.03)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value GRM188R61E106MA73D (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.6475 113.03)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value GRM188R71E104KA01D (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 VCC))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1092-03A-6:SMA END LAUNCH" (layer F.Cu) (tedit 5C22117D)
    (at 135.75284 132.67436 90)
    (fp_text reference J1 (at 0 8.5 90) (layer F.SilkS))
    (fp_text value 1092-03A-6 (at -0.03 -8.2 90) (layer F.Fab))
    (pad 1 smd rect (at 6.5 0 90) (size 6 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 6.5 3.65 90) (size 6 5.694) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 6.49986 -3.7211 90) (size 6 5.694) (layers F.Cu F.Paste F.Mask))
  )
  (module IPL1-104-02-L-D-K-TR:IPL110402LDKTR (layer F.Cu) (tedit 5C1E45E2)
    (at 150.71344 120.69064)
    (descr IPL1-104-02-L-D-K-TR-2)
    (tags Connector)
    (attr smd)
    (fp_text reference J2 (at 0 -0.51) (layer F.SilkS))
    (fp_text value IPL1-104-02-L-D-K-TR (at 0 -0.51) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.81 -3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 2 smd rect (at -1.27 -3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 3 smd rect (at 1.27 -3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 4 smd rect (at 3.81 -3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 5 smd rect (at 3.81 3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at 1.27 3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at -1.27 3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at -3.81 3.11) (size 1.27 3.94) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad8)"))
  )
  (module LSHM-120-02.5-F-DV-A-N-K-TR:LSHM120025FDVANKTR (layer F.Cu) (tedit 5C24BEB6)
    (at 135.2 95.25)
    (descr LSHM-120-02.5-F-DV-A-N-K-TR-1)
    (tags Connector)
    (fp_text reference J3 (at 0 0.25) (layer F.SilkS))
    (fp_text value LSHM-120-02.5-F-DV-A-N-K-TR (at 0 0.25) (layer F.SilkS) hide)
    (pad 1 smd rect (at 4.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 4.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 4.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 4.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 3.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad5)"))
    (pad 6 smd rect (at 3.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad6)"))
    (pad 7 smd rect (at 3.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad7)"))
    (pad 8 smd rect (at 3.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 9 smd rect (at 2.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J3-Pad9)"))
    (pad 10 smd rect (at 2.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 11 smd rect (at 2.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad11)"))
    (pad 12 smd rect (at 2.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 13 smd rect (at 1.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad13)"))
    (pad 14 smd rect (at 1.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 15 smd rect (at 1.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad15)"))
    (pad 16 smd rect (at 1.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 17 smd rect (at 0.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 18 smd rect (at 0.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 19 smd rect (at 0.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad19)"))
    (pad 20 smd rect (at 0.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 21 smd rect (at -0.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 22 smd rect (at -0.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 23 smd rect (at -0.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad23)"))
    (pad 24 smd rect (at -0.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 25 smd rect (at -1.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 26 smd rect (at -1.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 27 smd rect (at -1.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad27)"))
    (pad 28 smd rect (at -1.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 29 smd rect (at -2.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 30 smd rect (at -2.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 31 smd rect (at -2.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad31)"))
    (pad 32 smd rect (at -2.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 33 smd rect (at -3.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 34 smd rect (at -3.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 35 smd rect (at -3.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad35)"))
    (pad 36 smd rect (at -3.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 37 smd rect (at -4.25 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad37)"))
    (pad 38 smd rect (at -4.25 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad 39 smd rect (at -4.75 1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad39)"))
    (pad 40 smd rect (at -4.75 -1.85) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 GND))
    (pad MH1 thru_hole circle (at -6 0.85 90) (size 0.725 0.725) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
    (pad MH2 thru_hole circle (at 6 0.85 90) (size 0.725 0.725) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 107.95 129.54) (end 107.95 90.17) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 129.54) (end 107.95 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 90.17) (end 162.56 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 90.17) (end 162.56 90.17) (layer Edge.Cuts) (width 0.15))
)
