(module "vfedtec:op600-fp-v4" (layer F.Cu) (tedit 5D14D1F6)
  (descr "op600 StepUp generated footprint")
  (fp_text reference "REF**" (at 0 -2.4) (layer F.SilkS))
  (fp_text value "Value " (at 0 2.4) (layer F.SilkS))
  (fp_text user "%R" (at 0 -2.4) (layer F.Fab))
  (pad "1" smd custom (at 1.5 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
    (zone_connect 0)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.818195 0.455568) (xy -0.742419 0.3138) (xy -0.695756 0.159974) (xy -0.68 0) (xy -0.695756 -0.159974)
         (xy -0.742419 -0.3138) (xy -0.818195 -0.455568) (xy -0.920172 -0.579828) (xy -0.5 -1) (xy 0.5 -1)
         (xy 0.5 1) (xy -0.5 1) (xy -0.920172 0.579828)) (width 0))
    ))
  (pad "1" smd custom (at -1.5 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
    (zone_connect 0)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy 0.818195 -0.455568) (xy 0.742419 -0.3138) (xy 0.695756 -0.159974) (xy 0.68 0) (xy 0.695756 0.159974)
         (xy 0.742419 0.3138) (xy 0.818195 0.455568) (xy 0.920172 0.579828) (xy 0.5 1) (xy -0.5 1)
         (xy -0.5 -1) (xy 0.5 -1) (xy 0.920172 -0.579828)) (width 0))
    ))
  (pad "" smd circle (at 0 0) (size 2.9 2.9) (layers "B.Cu" "B.SilkS" "B.Mask"))
  (pad "" np_thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  (model "C:\\Temp\\op600.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
