(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 766)
    (tracks 0)
    (zones 0)
    (modules 3)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.17145)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.177546)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.524 0.889)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 7.2 7.2)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 127)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.508000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Plots/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /Channel_1/PWR-SWITCHED)
  (net 3 /Power/PWR-IN-1)
  (net 4 "Net-(J11-Pad12)")
  (net 5 LINK-ACT-1)
  (net_class Default "This is the default net class."
    (clearance 0.17145)
    (trace_width 0.1778)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Power/PWR-IN-1)
    (add_net GND)
    (add_net LINK-ACT-1)
    (add_net "Net-(J11-Pad12)")
  )
  (net_class AMP2 ""
    (clearance 0.17145)
    (trace_width 2.54)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Channel_1/PWR-SWITCHED)
  )
  (module Capacitors-SI:C_0603 (layer F.Cu) (tedit 5BC5FB65)
    (at 65.913 119.392 90)
    (descr "Resistor SMD 0603")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C94 (at 2.9076 -0.10668 90) (layer F.SilkS))
    (fp_text value C0603_100nf_10%_X7R_100V_CS0603KRX7R0BB104 (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Channel_1/PWR-SWITCHED))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module Diodes-SI:D_SMA (layer F.Cu) (tedit 5BE9BE92)
    (at 215.868 73.279 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D25 (at 0.095 -2.921 180) (layer F.SilkS))
    (fp_text value D_TVS_33V_SMAJ33A-13-F (at 0 2.6 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /Power/PWR-IN-1))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors-SI:R_0603 (layer F.Cu) (tedit 5BC5FB65)
    (at 111.76 84.213 90)
    (descr "Resistor SMD 0603")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R195 (at 3.1884 -0.0508 90) (layer F.SilkS))
    (fp_text value R0603_3K01_1%_0W1_ERJ-3EKF3011V (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LINK-ACT-1))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J11-Pad12)"))
  )
  (gr_line (start 15.7673 134.84225) (end 15.7673 164.64915) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 221.5073 49.24425) (end 223.5393 49.24425) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 15.7673 49.24425) (end 15.7673 130.27025) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 220.9993 130.77825) (end 220.9993 134.33425) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 18.3073 134.33425) (end 18.3073 130.77825) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 15.7673 49.24425) (end 17.7993 49.24425) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 15.7673 134.84225) (end 17.7993 134.84225) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 15.7673 14.43355) (end 15.7673 44.67225) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 223.5393 130.27025) (end 221.5073 130.27025) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 17.7993 48.73625) (end 17.7993 49.24425) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 18.3073 48.73625) (end 18.3073 45.18025) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 17.7993 45.18025) (end 18.3073 45.18025) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 17.7993 44.67225) (end 15.7673 44.67225) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 223.5393 14.43355) (end 15.7673 14.43355) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 223.5393 44.67225) (end 223.5393 14.43355) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 223.5393 44.67225) (end 221.5073 44.67225) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 221.5073 45.18025) (end 221.5073 44.67225) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 223.5393 130.27025) (end 223.5393 49.24425) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 221.5073 134.33425) (end 220.9993 134.33425) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 221.5073 134.84225) (end 223.5393 134.84225) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 221.5073 130.77825) (end 221.5073 130.27025) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 223.5393 164.64915) (end 223.5393 134.84225) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 15.7673 164.64915) (end 223.5393 164.64915) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 17.7993 134.33425) (end 17.7993 134.84225) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 17.7993 130.77825) (end 18.3073 130.77825) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 220.9993 45.18025) (end 220.9993 48.73625) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 221.5073 48.73625) (end 220.9993 48.73625) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 17.80286 130.27152) (end 15.77086 130.27152) (layer Edge.Cuts) (width 0.0254))
)
