(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 31)
    (zones 0)
    (modules 8)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.16)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.59)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.3)
    (via_min_size 0.635)
    (via_min_drill 0.3)
    (user_via 0.635 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.4 4.4)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 100.005001 127.99)
    (grid_origin 100 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00028_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/carlos/tmp/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /SCLK)
  (net 4 "Net-(U1-Pad21)")
  (net 5 "Net-(U1-Pad20)")
  (net 6 "Net-(U1-Pad19)")
  (net 7 "Net-(U1-Pad17)")
  (net 8 "Net-(U1-Pad16)")
  (net 9 "Net-(U1-Pad15)")
  (net 10 "Net-(U1-Pad14)")
  (net 11 "Net-(U1-Pad12)")
  (net 12 "Net-(U1-Pad11)")
  (net 13 /REGOUT)
  (net 14 +1V8)
  (net 15 "Net-(U1-Pad7)")
  (net 16 "Net-(U1-Pad6)")
  (net 17 "Net-(U1-Pad5)")
  (net 18 "Net-(U1-Pad4)")
  (net 19 "Net-(U1-Pad3)")
  (net 20 "Net-(U1-Pad2)")
  (net 21 "Net-(U1-Pad1)")
  (net 22 "/SDA(IN)")
  (net 23 /SDOUT)
  (net 24 /~CS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.635)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3V3)
    (add_net /REGOUT)
    (add_net /SCLK)
    (add_net "/SDA(IN)")
    (add_net /SDOUT)
    (add_net /~CS)
    (add_net GND)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
  )
  (module local:QFN-24_3x3mm_P0.4mm locked (layer F.Cu) (tedit 5BAE9FA5)
    (at 114 104)
    (descr "24-Lead Plastic QFN (3mm x 3mm); Pitch 0.4mm")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U1 (at -3.254999 -1.45) (layer F.SilkS))
    (fp_text value ICM-20948 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.5 -1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.5 -0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(U1-Pad2)"))
    (pad 3 smd roundrect (at -1.5 -0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at -1.5 0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(U1-Pad4)"))
    (pad 5 smd roundrect (at -1.5 0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(U1-Pad5)"))
    (pad 6 smd roundrect (at -1.5 1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(U1-Pad6)"))
    (pad 7 smd roundrect (at -1 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(U1-Pad7)"))
    (pad 8 smd roundrect (at -0.6 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 +1V8))
    (pad 9 smd roundrect (at -0.2 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /SDOUT))
    (pad 10 smd roundrect (at 0.2 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /REGOUT))
    (pad 11 smd roundrect (at 0.6 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(U1-Pad11)"))
    (pad 12 smd roundrect (at 1 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad12)"))
    (pad 13 smd roundrect (at 1.5 1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 14 smd roundrect (at 1.5 0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad14)"))
    (pad 15 smd roundrect (at 1.5 0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad15)"))
    (pad 16 smd roundrect (at 1.5 -0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad16)"))
    (pad 17 smd roundrect (at 1.5 -0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad17)"))
    (pad 18 smd roundrect (at 1.5 -1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 19 smd roundrect (at 1 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad19)"))
    (pad 20 smd roundrect (at 0.6 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U1-Pad20)"))
    (pad 21 smd roundrect (at 0.2 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad21)"))
    (pad 22 smd roundrect (at -0.2 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /~CS))
    (pad 23 smd roundrect (at -0.6 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /SCLK))
    (pad 24 smd roundrect (at -1 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "/SDA(IN)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24_3x3mm_P0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.39 106.98 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.17 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /REGOUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.399999 106.98 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.05 1.09 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.784999 104 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.4 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:MountingHole_3.2mm (layer F.Cu) (tedit 5BA924DF)
    (at 124.2 124.2)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H4 (at 2.385001 2.71) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module local:MountingHole_3.2mm (layer F.Cu) (tedit 5BA924DF)
    (at 103.8 124.2)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H3 (at -2.464999 2.8) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module local:MountingHole_3.2mm (layer F.Cu) (tedit 5BA924DF)
    (at 124.2 103.8)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 2.355001 -2.63) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module local:MountingHole_3.2mm (layer F.Cu) (tedit 5BA924DF)
    (at 103.8 103.8)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at -2.384999 -2.65) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 100 128) (end 100 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128 128) (end 100 128) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128 100) (end 128 128) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 128 100) (layer Edge.Cuts) (width 0.15))
)
