(module C_FEEDTHRU_0603 (layer F.Cu) (tedit 5CD10682)
  (descr "Capacitor  Feed Through 0603 Generic (https://product.tdk.com/info/en/catalog/datasheets/3tf_commercial_power_yff-p_en.pdf)")
  (tags "capacitor 0603 feedthru NFM")
  (attr smd)
  (fp_text reference REF** (at 0.55 -1.8) (layer F.SilkS))
  (fp_text value C_FEEDTHRU_0603 (at 0 2.1) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 3 smd rect (at 0 0) (size 0.4 2) (layers F.Cu))
  (pad 1 smd rect (at -0.8 0) (size 0.8 0.6) (drill (offset -0.1 0)) (layers F.Cu))
  (pad 2 smd rect (at 0.8 0) (size 0.8 0.6) (drill (offset 0.1 0)) (layers F.Cu))
  (model Capacitors_SMD.3dshapes/C_0603.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
