(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 54)
    (zones 0)
    (modules 36)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 167.517648 85.110008)
    (grid_origin 290.74524 121.564376)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "ATsub_Gerber_V2/"))
  )
  (net 0 "")
  (net 1 VDD_3.3V)
  (net 2 Earth)
  (net 3 "Net-(C16-Pad1)")
  (net 4 "Net-(DN21-Pad1)")
  (net 5 "Net-(DN21-Pad2)")
  (net 6 "Net-(DN21-Pad3)")
  (net 7 "Net-(DN22-Pad3)")
  (net 8 "Net-(DN22-Pad2)")
  (net 9 "Net-(DN22-Pad1)")
  (net 10 "Net-(DN23-Pad3)")
  (net 11 "Net-(DN23-Pad2)")
  (net 12 "Net-(DN23-Pad1)")
  (net 13 /LED/blue)
  (net 14 /LED/green)
  (net 15 /LED/red)
  (net 16 "Net-(R11-Pad2)")
  (net 17 "Net-(R12-Pad2)")
  (net 18 "Net-(R15-Pad1)")
  (net 19 "Net-(R18-Pad1)")
  (net 20 "Net-(R19-Pad2)")
  (net 21 "Net-(C14-Pad1)")
  (net 22 "Net-(C15-Pad1)")
  (net 23 Stby_Key)
  (net 24 Fan_Key)
  (net 25 BLUE_LED_PWM)
  (net 26 GREEN_LED_PWM)
  (net 27 RED_LED_PWM)
  (net 28 Cover_key)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LED/blue)
    (add_net /LED/green)
    (add_net /LED/red)
    (add_net BLUE_LED_PWM)
    (add_net Cover_key)
    (add_net Earth)
    (add_net Fan_Key)
    (add_net GREEN_LED_PWM)
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(DN21-Pad1)")
    (add_net "Net-(DN21-Pad2)")
    (add_net "Net-(DN21-Pad3)")
    (add_net "Net-(DN22-Pad1)")
    (add_net "Net-(DN22-Pad2)")
    (add_net "Net-(DN22-Pad3)")
    (add_net "Net-(DN23-Pad1)")
    (add_net "Net-(DN23-Pad2)")
    (add_net "Net-(DN23-Pad3)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net RED_LED_PWM)
    (add_net Stby_Key)
    (add_net VDD_3.3V)
  )
  (module "00_footprint:DTC144EE(SOT-416)" (layer F.Cu) (tedit 5CD27E7C)
    (at 180.858 115.122)
    (descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
    (tags SOT-416)
    (attr smd)
    (fp_text reference Q23 (at 2.292 -1.047) (layer F.SilkS))
    (fp_text value "DTC144EE(EMT3)" (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.65 -0.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 RED_LED_PWM))
    (pad 1 smd rect (at -0.65 0.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 3 smd rect (at 0.65 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /LED/red))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-416.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00_footprint:12505WR-08000 (layer B.Cu) (tedit 5D2D8281)
    (at 172.63524 122.580376 180)
    (fp_text reference J1 (at 1.31064 9.1567) (layer B.SilkS))
    (fp_text value 12505WR-08000 (at 2.75336 7.66318) (layer B.Fab))
    (pad 8 smd rect (at 1.05 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD_3.3V))
    (pad 10 smd rect (at -1.1 1.55 180) (size 2.2 3.1) (layers B.Cu B.Paste B.Mask)
      (net 2 Earth))
    (pad 9 smd rect (at 11.95 1.55 180) (size 2.2 3.1) (layers B.Cu B.Paste B.Mask)
      (net 2 Earth))
    (pad 7 smd rect (at 2.3 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 23 Stby_Key))
    (pad 6 smd rect (at 3.55 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 24 Fan_Key))
    (pad 5 smd rect (at 4.8 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 25 BLUE_LED_PWM))
    (pad 4 smd rect (at 6.05 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 26 GREEN_LED_PWM))
    (pad 3 smd rect (at 7.3 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 27 RED_LED_PWM))
    (pad 2 smd rect (at 8.55 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 28 Cover_key))
    (pad 1 smd rect (at 9.8 4.45 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 Earth))
  )
  (module 00_footprint:Touch_pad (layer F.Cu) (tedit 5D14935B)
    (at 199.05124 68.478376)
    (fp_text reference PAD11 (at -0.1 -2.275) (layer F.SilkS))
    (fp_text value TOUCH_PAD (at 0.3429 -6.604) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C14-Pad1)"))
  )
  (module 00_footprint:Touch_pad (layer F.Cu) (tedit 5D14934E)
    (at 136.31324 68.478376)
    (fp_text reference PAD12 (at -0.075 -2.175) (layer F.SilkS))
    (fp_text value TOUCH_PAD (at 0.3429 -6.604) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C15-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.725 56.075 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 Cover_key))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 142.758 108.56 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 3.35 -0.198 180) (layer F.SilkS))
    (fp_text value 10uF/1608/10V (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 144.282 108.56 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 2.17 -1.722 180) (layer F.SilkS))
    (fp_text value 2.2uF/1608/10V (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.488 109.28 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0.33 -1.078 180) (layer F.SilkS))
    (fp_text value 100nF/1005/50V/C0G (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 144.26 111.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -1.46 0.05) (layer B.SilkS))
    (fp_text value 1pF (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 144.775 113.34 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -1.61 -0.25 180) (layer B.SilkS))
    (fp_text value 1pF (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 145.775 113.34 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -1.61 0.05 180) (layer B.SilkS))
    (fp_text value 1pF (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00_footprint:SP117RGB (layer F.Cu) (tedit 5D1457BD)
    (at 197.664696 100.990376 330)
    (fp_text reference DN21 (at 7.52899 -0.629966 70) (layer F.SilkS))
    (fp_text value "SP117RGB(sideView)" (at -0.0635 -4.1275 330) (layer F.Fab))
    (pad 1 smd rect (at 1.75 -0.25 330) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(DN21-Pad1)"))
    (pad 2 smd rect (at 0.4 -0.8 330) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(DN21-Pad2)"))
    (pad 4 smd rect (at -1.75 -0.25 330) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD_3.3V))
    (pad 3 smd rect (at -0.4 -0.8 330) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(DN21-Pad3)"))
  )
  (module 00_footprint:SP117RGB (layer F.Cu) (tedit 5D1457BD)
    (at 166.29524 50.439376 90)
    (fp_text reference DN22 (at 1.079 1.782 90) (layer F.SilkS))
    (fp_text value "SP117RGB(sideView)" (at -0.0635 -4.1275 90) (layer F.Fab))
    (pad 3 smd rect (at -0.4 -0.8 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(DN22-Pad3)"))
    (pad 4 smd rect (at -1.75 -0.25 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD_3.3V))
    (pad 2 smd rect (at 0.4 -0.8 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(DN22-Pad2)"))
    (pad 1 smd rect (at 1.75 -0.25 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(DN22-Pad1)"))
  )
  (module 00_footprint:SP117RGB (layer F.Cu) (tedit 5D1457BD)
    (at 138.85324 103.276376 210)
    (fp_text reference DN23 (at 4.894905 -3.262575 290) (layer F.SilkS))
    (fp_text value "SP117RGB(sideView)" (at -0.0635 -4.1275 30) (layer F.Fab))
    (pad 3 smd rect (at -0.4 -0.8 210) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(DN23-Pad3)"))
    (pad 4 smd rect (at -1.75 -0.25 210) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD_3.3V))
    (pad 2 smd rect (at 0.4 -0.8 210) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(DN23-Pad2)"))
    (pad 1 smd rect (at 1.75 -0.25 210) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(DN23-Pad1)"))
  )
  (module "00_footprint:DTC144EE(SOT-416)" (layer F.Cu) (tedit 5CD27E7C)
    (at 183.975 118.425)
    (descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
    (tags SOT-416)
    (attr smd)
    (fp_text reference Q21 (at 2.25 -1.5) (layer F.SilkS))
    (fp_text value "DTC144EE(EMT3)" (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.65 -0.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 BLUE_LED_PWM))
    (pad 1 smd rect (at -0.65 0.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 3 smd rect (at 0.65 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /LED/blue))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-416.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "00_footprint:DTC144EE(SOT-416)" (layer F.Cu) (tedit 5CD27E7C)
    (at 180.86 117.5)
    (descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
    (tags SOT-416)
    (attr smd)
    (fp_text reference Q22 (at 3.94 -2.025) (layer F.SilkS))
    (fp_text value "DTC144EE(EMT3)" (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 0.65 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED/green))
    (pad 1 smd rect (at -0.65 0.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 2 smd rect (at -0.65 -0.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 GREEN_LED_PWM))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-416.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 141.785 110.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -1.395 0) (layer F.SilkS))
    (fp_text value 1k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.552 109.28 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0.395 -1.023) (layer F.SilkS))
    (fp_text value 1k (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.385 113.025 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -1.54 -0.15 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 Stby_Key))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 149.31 114)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 1.49 0.025) (layer B.SilkS))
    (fp_text value NC (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 Stby_Key))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.725 113.435 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -0.035 0.925) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C14-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.385 111.95 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -1.49 -0.05 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 Fan_Key))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 146.325 111.9 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -1.435 -0.09 180) (layer B.SilkS))
    (fp_text value NC (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 Fan_Key))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.34 115.1 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -0.61 -0.925 180) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R18-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.845 115.122 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -1.505 -0.198 180) (layer F.SilkS))
    (fp_text value NC (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD_3.3V))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.845 116.392)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0.495 1.158) (layer F.SilkS))
    (fp_text value 0R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Earth))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 198.79724 104.061376 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -1.912 -0.883 180) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(DN21-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /LED/red))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 201.08324 99.720376 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -0.775 1.85 180) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /LED/green))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(DN21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 200.59824 97.942376 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -0.3 2.225 180) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(DN21-Pad3)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /LED/blue))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 168.18024 48.689376 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at -2.463 -0.061 180) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /LED/red))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(DN22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 163.23724 49.682376)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at -1.705 -1.067 -270) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(DN22-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /LED/green))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 163.23724 50.952376)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -1.678 0.988 -270) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /LED/blue))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(DN22-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 135.80524 101.752376 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at -1.846 -0.503) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(DN23-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /LED/red))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.85324 106.832376 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at -0.321 -1.346 90) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /LED/green))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(DN23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 140.12324 106.809376 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at -0.119 2.484 90) (layer F.SilkS))
    (fp_text value 200R (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(DN23-Pad3)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /LED/blue))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00_footprint:GT304L (layer F.Cu) (tedit 5D11ED63)
    (at 145.275 112.4)
    (attr smd)
    (fp_text reference U11 (at 3.8 -4.575) (layer F.SilkS) hide)
    (fp_text value GT304L-QN (at 0 2.95) (layer F.Fab))
    (pad 1 smd oval (at -1.45 -0.75 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd oval (at -1.45 -0.25 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R11-Pad2)"))
    (pad 3 smd oval (at -1.45 0.25 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd oval (at -1.45 0.75 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R15-Pad1)"))
    (pad 5 smd oval (at -0.75 1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R18-Pad1)"))
    (pad 6 smd oval (at -0.25 1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at 0.25 1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C16-Pad1)"))
    (pad 8 smd oval (at 0.75 1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R19-Pad2)"))
    (pad 9 smd oval (at 1.45 0.75 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd oval (at 1.45 0.25 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 Stby_Key))
    (pad 11 smd oval (at 1.45 -0.25 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 Fan_Key))
    (pad 12 smd oval (at 1.45 -0.75 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 13 smd oval (at 0.75 -1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at 0.25 -1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd oval (at -0.25 -1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R12-Pad2)"))
    (pad 16 smd oval (at -0.75 -1.45) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD_3.3V))
    (pad 17 smd rect (at -0.61875 -0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.61875 -0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.61875 0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.61875 0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.20625 -0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.20625 -0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.20625 0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at -0.20625 0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.20625 -0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.20625 -0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.20625 0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.20625 0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.61875 -0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.61875 -0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.61875 0.1875) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
    (pad 17 smd rect (at 0.61875 0.5625) (size 0.4125 0.375) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth) (solder_paste_margin -0.75))
  )
  (gr_circle (center 167.5212 85.09) (end 206.5212 85.09) (layer Edge.Cuts) (width 0.2))
  (target plus (at 167.517648 85.110008) (size 5) (width 0.05) (layer Edge.Cuts))
  (gr_circle (center 167.5212 85.09) (end 198.7712 85.09) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 131.5212 85.09) (end 132.9212 85.09) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.3 41.85) (xy 212.7 41.725) (xy 208.45 128) (xy 122.225 128.1)
      )
    )
  )
  (zone (net 2) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.425 125.775) (xy 123.525 130.675) (xy 123.15 44.725) (xy 207.025 44.6)
      )
    )
  )
)
