(kicad_pcb (version 20171130) (host pcbnew 5.1.3-ffb9f22~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 0)
    (zones 0)
    (modules 56)
    (nets 44)
  )
  (page A)
  (title_block
    (title "ESR Meter PCB")
    (date 2019-07-25)
    (rev -)
    (company "Marilla elek, 8440 Marilla Rd, Copemish, MI 49625-9747 USA")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(AR1-Pad7)")
  (net 3 "Net-(AR1-Pad6)")
  (net 4 "Net-(AR1-Pad5)")
  (net 5 -5V)
  (net 6 GNDPWR)
  (net 7 "Net-(AR1-Pad2)")
  (net 8 "Net-(AR1-Pad1)")
  (net 9 "Net-(AR2-Pad1)")
  (net 10 "Net-(AR2-Pad2)")
  (net 11 "Net-(AR2-Pad5)")
  (net 12 "Net-(AR2-Pad6)")
  (net 13 "Net-(AR2-Pad7)")
  (net 14 "Net-(AR3-Pad6)")
  (net 15 "Net-(AR3-Pad2)")
  (net 16 "Net-(AR3-Pad1)")
  (net 17 "Net-(C1-Pad1)")
  (net 18 "Net-(C2-Pad1)")
  (net 19 "Net-(C3-Pad1)")
  (net 20 "Net-(C4-Pad1)")
  (net 21 "Net-(C5-Pad1)")
  (net 22 "Net-(C5-Pad2)")
  (net 23 "Net-(C6-Pad2)")
  (net 24 "Net-(C8-Pad1)")
  (net 25 "Net-(C8-Pad2)")
  (net 26 "Net-(D2-Pad1)")
  (net 27 "Net-(D2-Pad2)")
  (net 28 "Net-(D3-Pad2)")
  (net 29 "Net-(D4-Pad2)")
  (net 30 "Net-(DS1-Pad2)")
  (net 31 "Net-(J2-Pad3)")
  (net 32 "Net-(N1R1-Pad1)")
  (net 33 "Net-(N1R1-Pad2)")
  (net 34 "Net-(N1R2-Pad2)")
  (net 35 "Net-(N1R2-Pad1)")
  (net 36 "Net-(R8-Pad1)")
  (net 37 "Net-(R16-Pad1)")
  (net 38 "Net-(R17-Pad3)")
  (net 39 "Net-(R20-Pad1)")
  (net 40 "Net-(S1-Pad3)")
  (net 41 "Net-(VR1-Pad1)")
  (net 42 "Net-(VR1-Pad6)")
  (net 43 "Net-(VR1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net -5V)
    (add_net GNDPWR)
    (add_net "Net-(AR1-Pad1)")
    (add_net "Net-(AR1-Pad2)")
    (add_net "Net-(AR1-Pad5)")
    (add_net "Net-(AR1-Pad6)")
    (add_net "Net-(AR1-Pad7)")
    (add_net "Net-(AR2-Pad1)")
    (add_net "Net-(AR2-Pad2)")
    (add_net "Net-(AR2-Pad5)")
    (add_net "Net-(AR2-Pad6)")
    (add_net "Net-(AR2-Pad7)")
    (add_net "Net-(AR3-Pad1)")
    (add_net "Net-(AR3-Pad2)")
    (add_net "Net-(AR3-Pad6)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(DS1-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(N1R1-Pad1)")
    (add_net "Net-(N1R1-Pad2)")
    (add_net "Net-(N1R2-Pad1)")
    (add_net "Net-(N1R2-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad3)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(VR1-Pad1)")
    (add_net "Net-(VR1-Pad6)")
    (add_net "Net-(VR1-Pad7)")
  )
  (module Non-plated_holes:MTGNPH300Z400 (layer F.Cu) (tedit 0)
    (at 89 72)
    (descr "Mounting Hole, Non-Plated; 0.00 mm Clearance, 3.00 mm Hole")
    (fp_text reference NPH2 (at 0 -3) (layer F.SilkS))
    (fp_text value Non_plated_hole (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 3) (layers *.Cu *.Mask))
  )
  (module footprints:Meter-DH-670_1_mA locked (layer F.Cu) (tedit 5D3F8BF4)
    (at 135.036938 116.230585)
    (fp_text reference M1 (at -0.036938 -31.230585) (layer F.SilkS))
    (fp_text value "0..1 mA DC" (at -0.036938 4.469415) (layer F.Fab) hide)
    (fp_text user - (at -15.036938 -5.230585) (layer B.SilkS))
    (fp_text user + (at 14.963062 -5.230585) (layer B.SilkS))
    (fp_text user - (at -15 -5.5) (layer F.SilkS))
    (fp_text user + (at 15 -5.5) (layer F.SilkS))
    (pad 1 thru_hole circle (at -15 -7.5) (size 2.92 2.92) (drill 2.15) (layers *.Cu *.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 15 -7.5) (size 2.92 2.92) (drill 2.15) (layers *.Cu *.Mask)
      (net 26 "Net-(D2-Pad1)"))
  )
  (module SamacSys_Parts:PV37W (layer F.Cu) (tedit 0)
    (at 151 84)
    (descr PV37W)
    (tags Resistor)
    (fp_text reference R17 (at 0 -6) (layer F.SilkS))
    (fp_text value "10 kΩ" (at -0.42 -1.474) (layer F.SilkS) hide)
    (fp_text user %R (at -0.42 -1.474) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.54 -1.02) (size 1.1 1.1) (drill 0.69) (layers *.Cu *.Mask)
      (net 38 "Net-(R17-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.56) (size 1.1 1.1) (drill 0.69) (layers *.Cu *.Mask)
      (net 15 "Net-(AR3-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -1.02) (size 1.1 1.1) (drill 0.69) (layers *.Cu *.Mask)
      (net 37 "Net-(R16-Pad1)"))
  )
  (module SamacSys_Parts:PV37W (layer F.Cu) (tedit 0)
    (at 112 48 90)
    (descr PV37W)
    (tags Resistor)
    (fp_text reference R8 (at 5 -2 180) (layer F.SilkS))
    (fp_text value "10 kΩ" (at -0.42 -1.474 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.54 -1.02 90) (size 1.1 1.1) (drill 0.69) (layers *.Cu *.Mask)
      (net 2 "Net-(AR1-Pad7)"))
    (pad 2 thru_hole circle (at 0 -3.56 90) (size 1.1 1.1) (drill 0.69) (layers *.Cu *.Mask)
      (net 3 "Net-(AR1-Pad6)"))
    (pad 1 thru_hole circle (at -2.54 -1.02 90) (size 1.1 1.1) (drill 0.69) (layers *.Cu *.Mask)
      (net 36 "Net-(R8-Pad1)"))
  )
  (module SamacSys_Parts:DIPS762W51P254L1016H419Q8N (layer B.Cu) (tedit 5D1E7298)
    (at 97 51)
    (descr 110-99-308-41-001000)
    (tags Connector)
    (fp_text reference AR1 (at 3 -10) (layer B.SilkS))
    (fp_text value TL082 (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at 4 -3) (layer B.Fab))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 7 thru_hole circle (at 7.62 -2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(AR1-Pad7)"))
    (pad 6 thru_hole circle (at 7.62 -5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(AR1-Pad6)"))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(AR1-Pad5)"))
    (pad 4 thru_hole circle (at 0 -7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 -5V))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(AR1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(AR1-Pad1)"))
  )
  (module SamacSys_Parts:DIPS762W51P254L1016H419Q8N (layer B.Cu) (tedit 5D1E7298)
    (at 137 66)
    (descr 110-99-308-41-001000)
    (tags Connector)
    (fp_text reference AR2 (at 4 -10) (layer B.SilkS))
    (fp_text value TL082 (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at 4 -3) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(AR2-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(AR2-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(AR1-Pad7)"))
    (pad 4 thru_hole circle (at 0 -7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 -5V))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(AR2-Pad5)"))
    (pad 6 thru_hole circle (at 7.62 -5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(AR2-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 -2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(AR2-Pad7)"))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +5V))
  )
  (module SamacSys_Parts:DIPS762W51P254L1016H419Q8N (layer B.Cu) (tedit 5D1E7298)
    (at 132 96)
    (descr 110-99-308-41-001000)
    (tags Connector)
    (fp_text reference AR3 (at 4 -10) (layer B.SilkS))
    (fp_text value TL082 (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at 4 -3) (layer B.Fab))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 7 thru_hole circle (at 7.62 -2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(AR3-Pad6)"))
    (pad 6 thru_hole circle (at 7.62 -5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(AR3-Pad6)"))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 4 thru_hole circle (at 0 -7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 -5V))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(AR2-Pad7)"))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(AR3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(AR3-Pad1)"))
  )
  (module footprints:CAP_AVX_SR21 (layer B.Cu) (tedit 5BEC3D0C)
    (at 98 55)
    (descr "Capacitor, Radial (Dipped, Rectangular); 5.08 mm C X 0.508 mm W 5.08 mm L X 3.175 mm T X 5.08 mm H body")
    (fp_text reference C1 (at 0 0) (layer B.Fab))
    (fp_text value "1 nF" (at 0 0) (layer B.Fab))
    (fp_text user %R (at 1 2) (layer B.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 17 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 6 GNDPWR))
  )
  (module footprints:CAP_AVX_SR21 (layer B.Cu) (tedit 5BEC3D0C)
    (at 100 62 90)
    (descr "Capacitor, Radial (Dipped, Rectangular); 5.08 mm C X 0.508 mm W 5.08 mm L X 3.175 mm T X 5.08 mm H body")
    (fp_text reference C2 (at 0 0 270) (layer B.Fab))
    (fp_text value "1 nF" (at 0 0 270) (layer B.Fab))
    (fp_text user %R (at -5 0 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 6 GNDPWR))
  )
  (module footprints:CAP_AVX_SR21 (layer B.Cu) (tedit 5BEC3D0C)
    (at 105 55)
    (descr "Capacitor, Radial (Dipped, Rectangular); 5.08 mm C X 0.508 mm W 5.08 mm L X 3.175 mm T X 5.08 mm H body")
    (fp_text reference C3 (at 0 0) (layer B.Fab))
    (fp_text value "1 nF" (at 0 0) (layer B.Fab))
    (fp_text user %R (at 2 3) (layer B.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 6 GNDPWR))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 19 "Net-(C3-Pad1)"))
  )
  (module footprints:CAP_AVX_SR21 (layer B.Cu) (tedit 5BEC3D0C)
    (at 125 44 90)
    (descr "Capacitor, Radial (Dipped, Rectangular); 5.08 mm C X 0.508 mm W 5.08 mm L X 3.175 mm T X 5.08 mm H body")
    (fp_text reference C4 (at -5 0 180) (layer B.Fab))
    (fp_text value "100 nF" (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -5 0 180) (layer B.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 4 "Net-(AR1-Pad5)"))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 20 "Net-(C4-Pad1)"))
  )
  (module footprints:CAP_AVX_SR21 (layer B.Cu) (tedit 5BEC3D0C)
    (at 121 72)
    (descr "Capacitor, Radial (Dipped, Rectangular); 5.08 mm C X 0.508 mm W 5.08 mm L X 3.175 mm T X 5.08 mm H body")
    (fp_text reference C5 (at 0 -3) (layer B.Fab))
    (fp_text value "100 nF" (at 0 0) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 21 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 22 "Net-(C5-Pad2)"))
  )
  (module footprints:CAP_AVX_SR21 (layer B.Cu) (tedit 5BEC3D0C)
    (at 121 81)
    (descr "Capacitor, Radial (Dipped, Rectangular); 5.08 mm C X 0.508 mm W 5.08 mm L X 3.175 mm T X 5.08 mm H body")
    (fp_text reference C6 (at 0 -3) (layer B.Fab))
    (fp_text value "100 nF" (at 0 0) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 23 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.16 1.16) (drill 0.76) (layers *.Cu *.Mask B.Paste)
      (net 10 "Net-(AR2-Pad2)"))
  )
  (module SamacSys_Parts:T350F226K016AS (layer B.Cu) (tedit 0)
    (at 146 50 270)
    (descr T350F226K016AS_1)
    (tags "Capacitor Polarised")
    (fp_text reference C7 (at -4 0) (layer B.SilkS))
    (fp_text value "22 µF" (at 1.27 0 270) (layer B.SilkS) hide)
    (fp_text user %R (at 1.27 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 -5V))
    (model T350F226K016AS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:T350G106K035AT (layer B.Cu) (tedit 0)
    (at 166 48 270)
    (descr T350G106K035AT-2)
    (tags "Capacitor Polarised")
    (fp_text reference C8 (at -4 0 180) (layer B.SilkS))
    (fp_text value "10 µF" (at 1.27 0 90) (layer B.SilkS) hide)
    (fp_text user %R (at 1.27 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad2)"))
    (model T350G106K035AT.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE50CD5)
    (at 128 80.62 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at -2 0 180) (layer B.SilkS))
    (fp_text value 1N4148 (at 3.81 -2.12 90) (layer B.Fab))
    (fp_text user K (at 0 1.8 90) (layer B.SilkS))
    (fp_text user K (at 0 1.8 90) (layer B.Fab))
    (fp_text user %R (at 4.11 0 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C5-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(AR2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE50CD5)
    (at 144.5 111 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 3.81 2.12) (layer B.SilkS))
    (fp_text value 1N5711 (at 3.81 -2.12) (layer B.Fab))
    (fp_text user %R (at 4.11 0) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE50CD5)
    (at 144.5 106 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 3.81 2.12) (layer B.SilkS))
    (fp_text value 1N5711 (at 3.81 -2.12) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.SilkS))
    (fp_text user K (at 0 1.8) (layer B.Fab))
    (fp_text user %R (at 4.11 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE50CD5)
    (at 132.5 111 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D4 (at 3.81 2.12) (layer B.SilkS))
    (fp_text value 1N5711 (at 3.81 -2.12) (layer B.Fab))
    (fp_text user %R (at 4.11 0) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE50CD5)
    (at 132.5 106 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 3.81 2.12) (layer B.SilkS))
    (fp_text value 1N5711 (at 3.81 -2.12) (layer B.Fab))
    (fp_text user %R (at 4.11 0) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.Fab))
    (fp_text user K (at 0 1.8) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:INL5AR30 (layer F.Cu) (tedit 0)
    (at 179 67 270)
    (descr INL-5AR30-2)
    (tags LED)
    (fp_text reference DS1 (at -5 0 180) (layer F.SilkS))
    (fp_text value RED (at 0.798 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.798 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.397 1.397) (drill 0.91) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.91) (layers *.Cu *.Mask)
      (net 30 "Net-(DS1-Pad2)"))
  )
  (module SamacSys_Parts:MJ3502N (layer F.Cu) (tedit 0)
    (at 118 47 270)
    (descr MJ-3502N-1)
    (tags Connector)
    (fp_text reference J1 (at -4 -6 180) (layer F.SilkS))
    (fp_text value "AUX FREQ INPUT" (at 3.498 0.3 90) (layer F.SilkS) hide)
    (fp_text user %R (at 3.498 0.3 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 4.193 4.193) (drill 2.7951) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole circle (at 5.4 0 270) (size 4.193 4.193) (drill 2.7951) (layers *.Cu *.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 3 thru_hole circle (at 11.1 0 270) (size 4.193 4.193) (drill 2.7951) (layers *.Cu *.Mask)
      (net 19 "Net-(C3-Pad1)"))
    (model MJ-3502N.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:CONSOCJ2155 (layer F.Cu) (tedit 0)
    (at 176 56 270)
    (descr CON-SOCJ-2155-1)
    (tags Connector)
    (fp_text reference J2 (at -14 7 180) (layer F.SilkS))
    (fp_text value "+5 V DC" (at -5.925 -1.425 90) (layer F.SilkS) hide)
    (fp_text user %R (at -5.925 -1.425 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 5.3 5.3) (drill 3.6401) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -6 0 270) (size 5 5) (drill 3.1623) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 3 thru_hole circle (at -3 -4.7 270) (size 5.3 5.3) (drill 3.6401) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad3)"))
    (pad 4 np_thru_hole circle (at -10.5 0 270) (size 2.2 0) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module SamacSys_Parts:RESAD1653W69L737D229 (layer B.Cu) (tedit 0)
    (at 95 111 90)
    (descr CMF55-111)
    (tags Resistor)
    (fp_text reference N1R1 (at 9 -4) (layer B.SilkS))
    (fp_text value "5 Ω/1 %" (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(N1R1-Pad1)"))
    (pad 2 thru_hole circle (at 16.5 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(N1R1-Pad2)"))
    (model RN55D1R00FRE6.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:RESAD1653W69L737D229 (layer B.Cu) (tedit 0)
    (at 95 134 90)
    (descr CMF55-111)
    (tags Resistor)
    (fp_text reference N1R2 (at 9 -4) (layer B.SilkS))
    (fp_text value "1 Ω/1 %" (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(N1R2-Pad1)"))
    (pad 2 thru_hole circle (at 16.5 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(N1R2-Pad2)"))
    (model RN55D1R00FRE6.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Non-plated_holes:MTGNPH300Z400 (layer F.Cu) (tedit 0)
    (at 102 72)
    (descr "Mounting Hole, Non-Plated; 0.00 mm Clearance, 3.00 mm Hole")
    (fp_text reference NPH1 (at 0 -3) (layer F.SilkS))
    (fp_text value Non_plated_hole (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 3) (layers *.Cu *.Mask))
  )
  (module Non-plated_holes:MTGNPH300Z400 (layer F.Cu) (tedit 0)
    (at 102 81)
    (descr "Mounting Hole, Non-Plated; 0.00 mm Clearance, 3.00 mm Hole")
    (fp_text reference NPH3 (at 0 -3) (layer F.SilkS))
    (fp_text value Non_plated_hole (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 3) (layers *.Cu *.Mask))
  )
  (module Non-plated_holes:MTGNPH300Z400 (layer F.Cu) (tedit 0)
    (at 89 81)
    (descr "Mounting Hole, Non-Plated; 0.00 mm Clearance, 3.00 mm Hole")
    (fp_text reference NPH4 (at 0 -3) (layer F.SilkS))
    (fp_text value Non_plated_hole (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 3) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 92 43 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -2 0) (layer B.SilkS))
    (fp_text value "22 kΩ" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(AR1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 88 53 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 10 0 180) (layer B.SilkS))
    (fp_text value "1 MΩ" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(AR1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(AR1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 92 61 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3 -3 180) (layer B.SilkS))
    (fp_text value "2.2 kΩ" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(AR1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 96 67 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 2 -3 180) (layer B.SilkS))
    (fp_text value "2.2 kΩ" (at 3.81 -2.37 90) (layer B.Fab))
    (fp_text user %R (at 3.81 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 104 58 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5 -3 180) (layer B.SilkS))
    (fp_text value "2.2 kΩ" (at 3.81 -2.37 90) (layer B.Fab))
    (fp_text user %R (at 3.81 0 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 129 50 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 2.37 180) (layer B.SilkS))
    (fp_text value "100 kΩ" (at 3.81 -2.37 90) (layer B.Fab))
    (fp_text user %R (at 3.81 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(AR1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 125 51 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 0 -3 90) (layer B.SilkS))
    (fp_text value "820 kΩ" (at 3.81 -2.37 90) (layer B.Fab))
    (fp_text user %R (at 3.81 0 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(AR1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 110 61 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 3.81 2.37) (layer B.SilkS))
    (fp_text value "10 kΩ" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 133 73 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 10 0 180) (layer B.SilkS))
    (fp_text value "47 Ω" (at 3.81 -2.37 90) (layer B.Fab))
    (fp_text user %R (at 3.81 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(AR2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 140 80 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 3.81 2.37) (layer B.SilkS))
    (fp_text value "270 Ω" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(AR2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 144 70 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 3 -3) (layer B.SilkS))
    (fp_text value "1 kΩ" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(AR2-Pad6)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 149 61 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 10 0) (layer B.SilkS))
    (fp_text value "1 kΩ" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(AR2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 154 69 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 6 3) (layer B.SilkS))
    (fp_text value "22 kΩ" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(AR2-Pad7)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(AR2-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 156 58 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 3.81 2.37) (layer B.SilkS))
    (fp_text value "22 kΩ" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(AR2-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 153 89 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at 3.81 2.37) (layer B.SilkS))
    (fp_text value "1.5 kΩ" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 158 93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R18 (at 4 3 180) (layer B.SilkS))
    (fp_text value "10 kΩ" (at 3.81 -2.37 90) (layer B.Fab))
    (fp_text user %R (at 3.81 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R17-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 166 99 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R19 (at 3.81 2.37) (layer B.SilkS))
    (fp_text value "680 Ω" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 170 93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R20 (at 3.81 2.37) (layer B.SilkS))
    (fp_text value "180 Ω" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 134 101 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R21 (at 11 0) (layer B.SilkS))
    (fp_text value "560 Ω" (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(AR3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 172 71 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R22 (at 10 0) (layer B.SilkS))
    (fp_text value "330 Ω" (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(DS1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:100SP1T1B4M2QE (layer F.Cu) (tedit 0)
    (at 179 98 270)
    (descr 100SP1T1B4M2QE)
    (tags Switch)
    (fp_text reference S1 (at -9 3 180) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -4.7 0 270) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask)
      (net 39 "Net-(R20-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 3 thru_hole circle (at 4.7 0 270) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask)
      (net 40 "Net-(S1-Pad3)"))
    (model 100SP1T1B1M2QEH.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Plated_holes:MTGP305H205 (layer F.Cu) (tedit 0)
    (at 91 95 90)
    (descr "Mounting Hole, Plated; 3.05 mm Pad, 2.05 mm Hole")
    (fp_text reference TP1 (at -3 0) (layer F.SilkS))
    (fp_text value Plated_thru_hole (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.05 3.05) (drill 2.05) (layers *.Cu *.Mask)
      (net 33 "Net-(N1R1-Pad2)"))
  )
  (module Plated_holes:MTGP305H205 (layer F.Cu) (tedit 0)
    (at 91 111 90)
    (descr "Mounting Hole, Plated; 3.05 mm Pad, 2.05 mm Hole")
    (fp_text reference TP2 (at 3 0) (layer F.SilkS))
    (fp_text value Plated_thru_hole (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.05 3.05) (drill 2.05) (layers *.Cu *.Mask)
      (net 32 "Net-(N1R1-Pad1)"))
  )
  (module Plated_holes:MTGP305H205 (layer F.Cu) (tedit 0)
    (at 91 118 90)
    (descr "Mounting Hole, Plated; 3.05 mm Pad, 2.05 mm Hole")
    (fp_text reference TP3 (at -3 0) (layer F.SilkS))
    (fp_text value Plated_thru_hole (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.05 3.05) (drill 2.05) (layers *.Cu *.Mask)
      (net 34 "Net-(N1R2-Pad2)"))
  )
  (module Plated_holes:MTGP305H205 (layer F.Cu) (tedit 0)
    (at 91 134 90)
    (descr "Mounting Hole, Plated; 3.05 mm Pad, 2.05 mm Hole")
    (fp_text reference TP4 (at 3 0) (layer F.SilkS))
    (fp_text value Plated_thru_hole (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.05 3.05) (drill 2.05) (layers *.Cu *.Mask)
      (net 35 "Net-(N1R2-Pad1)"))
  )
  (module SamacSys_Parts:DIPS762W51P254L1016H419Q8N (layer B.Cu) (tedit 5D1E7298)
    (at 160 45 180)
    (descr 110-99-308-41-001000)
    (tags Connector)
    (fp_text reference VR1 (at 4 3) (layer B.SilkS))
    (fp_text value TL7660CP (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at 4 -3) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 41 "Net-(VR1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 GNDPWR))
    (pad 4 thru_hole circle (at 0 -7.62 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad2)"))
    (pad 5 thru_hole circle (at 7.62 -7.62 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 -5V))
    (pad 6 thru_hole circle (at 7.62 -5.08 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 "Net-(VR1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 -2.54 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 "Net-(VR1-Pad7)"))
    (pad 8 thru_hole circle (at 7.62 0 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +5V))
  )
  (module Plated_holes:MTGPH50 (layer F.Cu) (tedit 0)
    (at 115 72)
    (descr "Mounting Hole, Plated; 1.20 mm Pad, 0.50 mm Hole")
    (fp_text reference WT1 (at 0 -2) (layer F.SilkS))
    (fp_text value Plated_thru_hole (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.5) (layers *.Cu *.Mask)
      (net 21 "Net-(C5-Pad1)"))
  )
  (module Plated_holes:MTGPH50 (layer F.Cu) (tedit 0)
    (at 115 81)
    (descr "Mounting Hole, Plated; 1.20 mm Pad, 0.50 mm Hole")
    (fp_text reference WT2 (at 0 -2) (layer F.SilkS))
    (fp_text value Plated_thru_hole (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(AR2-Pad2)"))
  )
  (gr_line (start 185 138) (end 185 42) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87 140) (end 183 140) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85 42) (end 85 138) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87 40) (end 183 40) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 87 138) (end 85 138) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 183 138) (end 183 140) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 183 42) (end 185 42) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 87 42) (end 87 40) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text X1 (at 179 106) (layer F.SilkS))
  (gr_text X5 (at 179 90) (layer F.SilkS))
  (zone (net 6) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185 140) (xy 85 140) (xy 85 40) (xy 185 40)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185 140) (xy 85 140) (xy 85 40) (xy 185 40)
      )
    )
  )
)
