(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")

  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 0)
    (zones 0)
    (modules 0)
    (nets 1)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 181.9 122)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (gr_line (start 185.39 62.03) (end 185.39 57.02) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.41 81.27) (end 184.66 81.27) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.68 63.49) (end 168.68 80.54) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 184.66 62.76) (end 169.41 62.76) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183.89 125.52) (end 173.12 125.52) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.4 117.13) (end 172.39 124.79) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.13 116.4) (end 171.67 116.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.4 124.79) (end 132.4 117.13) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.39 124.02) (end 97.39 79.02) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.39 57.02) (end 97.39 61.44) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.93 78.29) (end 98.12 78.29) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.66 62.89) (end 114.66 77.56) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98.12 62.17) (end 113.93 62.16) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.67 125.52) (end 98.89 125.52) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98.89 55.52) (end 183.89 55.52) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 185.39 82) (end 185.39 124.02) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 98.12 79.02) (end 98.12 78.29) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.93 77.56) (end 113.93 78.29) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 98.12 61.44) (end 97.39 61.44) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.93 62.89) (end 114.66 62.89) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169.41 80.54) (end 168.68 80.54) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 184.66 82) (end 185.39 82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 184.66 62.03) (end 184.66 62.76) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169.41 63.49) (end 169.41 62.76) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171.67 117.13) (end 172.4 117.13) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 133.13 117.13) (end 133.13 116.4) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 173.12 124.79) (end 172.39 124.79) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.67 124.79) (end 131.67 125.52) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 98.89 124.02) (end 97.39 124.02) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 98.89 57.02) (end 98.89 55.52) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 183.89 57.02) (end 185.39 57.02) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 183.89 124.02) (end 183.89 125.52) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 100.89 59.02) (end 99.24 59.02) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 181.89 59.02) (end 180.24 59.02) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 100.89 122.02) (end 99.24 122.02) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 181.89 122.02) (end 183.54 122.02) (layer Edge.Cuts) (width 0.05))

)
