(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6002)
    (drawings 10)
    (tracks 1813)
    (zones 0)
    (modules 161)
    (nets 115)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (trace_clearance 0.126746)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.635 0.254)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.508 0.508)
    (pad_drill 0.254)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 3V3)
  (net 2 1V8)
  (net 3 1V0)
  (net 4 12V0)
  (net 5 3V3_MICRO)
  (net 6 /xilinx_configuration/DTR)
  (net 7 "Net-(C3-Pad2)")
  (net 8 "Net-(C4-Pad1)")
  (net 9 "Net-(C9-Pad1)")
  (net 10 5V0)
  (net 11 2V8)
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D2-Pad2)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad2)")
  (net 16 "Net-(D5-Pad2)")
  (net 17 "Net-(D6-Pad1)")
  (net 18 "Net-(D6-Pad2)")
  (net 19 "Net-(D7-Pad1)")
  (net 20 "Net-(D7-Pad2)")
  (net 21 /xilinx_configuration/FTDI_3V3)
  (net 22 /xilinx_configuration/TXO)
  (net 23 /xilinx_configuration/RXI)
  (net 24 /xilinx_configuration/TMS)
  (net 25 /xilinx_configuration/TDI)
  (net 26 /xilinx_configuration/TDO)
  (net 27 /xilinx_configuration/TCK)
  (net 28 /ToF_sensors/TOF_TOP_FINGER_SDA)
  (net 29 /ToF_sensors/TOF_TOP_FINGER_SCL)
  (net 30 /ToF_sensors/TOF_TOP_FINGER_INT)
  (net 31 WHL_MOT_DIR)
  (net 32 /xilinx_configuration/INIT_B)
  (net 33 "Net-(Q1-Pad3)")
  (net 34 "Net-(Q3-Pad3)")
  (net 35 /xilinx_configuration/CD)
  (net 36 /xilinx_configuration/M0)
  (net 37 "Net-(R6-Pad1)")
  (net 38 "Net-(R7-Pad1)")
  (net 39 "Net-(R8-Pad1)")
  (net 40 /xilinx_configuration/M2)
  (net 41 /xilinx_configuration/M1)
  (net 42 /xilinx_configuration/STATUS_0)
  (net 43 /xilinx_configuration/STATUS_1)
  (net 44 /xilinx_configuration/CLEAR_EEPROM)
  (net 45 /xilinx_configuration/DEBUG_PROD_B)
  (net 46 /xilinx_configuration/SCLK)
  (net 47 /xilinx_configuration/DONE)
  (net 48 /xilinx_configuration/PROGRAM_B)
  (net 49 FPGA_PGOOD)
  (net 50 /xilinx_configuration/MCLK)
  (net 51 /xilinx_configuration/MISO)
  (net 52 WHL_MOT_FAULT_B)
  (net 53 GRP_MOT_ENABLE_B)
  (net 54 GRP_MOT_SLEEP_B)
  (net 55 GRP_MOT_STEP)
  (net 56 GRP_MOT_DIR)
  (net 57 GRP_MOT_FAULT_B)
  (net 58 WHL_MOT_ENABLE_B)
  (net 59 WHL_MOT_STEP)
  (net 60 WHL_MOT_SLEEP_B)
  (net 61 "Net-(L1-Pad1)")
  (net 62 /xilinx_configuration/CS_B)
  (net 63 /xilinx_configuration/MOSI)
  (net 64 "Net-(L2-Pad1)")
  (net 65 "Net-(L3-Pad1)")
  (net 66 "Net-(L4-Pad1)")
  (net 67 "Net-(R51-Pad1)")
  (net 68 "Net-(J3-Pad7)")
  (net 69 /xilinx_configuration/OUT_EN)
  (net 70 IR_LED_EN_B)
  (net 71 WHL_MOT_M1)
  (net 72 GRP_MOT_M1)
  (net 73 WHL_MOT_M0)
  (net 74 GRP_MOT_M0)
  (net 75 SCL_FPGA)
  (net 76 SDA_FPGA)
  (net 77 VP0)
  (net 78 CLD_ES_SIG)
  (net 79 OPN_ES_SIG)
  (net 80 "Net-(R9-Pad1)")
  (net 81 "Net-(R15-Pad2)")
  (net 82 "Net-(R16-Pad2)")
  (net 83 "Net-(R22-Pad1)")
  (net 84 /xilinx_configuration/NVRAM_SDA)
  (net 85 /xilinx_configuration/NVRAM_SCL)
  (net 86 DGND)
  (net 87 /ADC/VP)
  (net 88 /ADC/VN)
  (net 89 /ADC/VREFP)
  (net 90 FPGA_5V_EN)
  (net 91 /ADC/VREFN)
  (net 92 /ADC/VCCADC)
  (net 93 FPGA_BUCK_EN)
  (net 94 /power_generation_1/PG)
  (net 95 /power_generation_2/PWR_IN)
  (net 96 /power_generation_1/5V0)
  (net 97 /power_generation_2/EN3)
  (net 98 /power_generation_2/EN2)
  (net 99 /power_generation_2/EN1)
  (net 100 /power_generation_2/FB1)
  (net 101 /power_generation_2/FB2)
  (net 102 /power_generation_2/FB3)
  (net 103 /xilinx_configuration/D02)
  (net 104 /xilinx_configuration/D03)
  (net 105 /xilinx_configuration/CCLK)
  (net 106 /ToF_sensors/TOF_LEFT_FINGER_SDA)
  (net 107 /ToF_sensors/TOF_LEFT_FINGER_SCL)
  (net 108 /ToF_sensors/TOF_LEFT_FINGER_INT)
  (net 109 /ToF_sensors/TOF_RIGHT_FINGER_SDA)
  (net 110 /ToF_sensors/TOP_RIGHT_FINGER_SCL)
  (net 111 /ToF_sensors/TOF_RIGHT_FINGER_INT)
  (net 112 /ToF_sensors/TOP_FRONT_FACING_SDA)
  (net 113 /ToF_sensors/TOF_FRONT_FACING_SCL)
  (net 114 /ToF_sensors/TOF_FRONT_FACING_INT)
  (net_class Default "This is the default net class."
    (clearance 0.126746)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (add_net /ADC/VCCADC)
    (add_net /ADC/VN)
    (add_net /ADC/VP)
    (add_net /ADC/VREFN)
    (add_net /ADC/VREFP)
    (add_net /ToF_sensors/TOF_FRONT_FACING_INT)
    (add_net /ToF_sensors/TOF_FRONT_FACING_SCL)
    (add_net /ToF_sensors/TOF_LEFT_FINGER_INT)
    (add_net /ToF_sensors/TOF_LEFT_FINGER_SCL)
    (add_net /ToF_sensors/TOF_LEFT_FINGER_SDA)
    (add_net /ToF_sensors/TOF_RIGHT_FINGER_INT)
    (add_net /ToF_sensors/TOF_RIGHT_FINGER_SDA)
    (add_net /ToF_sensors/TOF_TOP_FINGER_INT)
    (add_net /ToF_sensors/TOF_TOP_FINGER_SCL)
    (add_net /ToF_sensors/TOF_TOP_FINGER_SDA)
    (add_net /ToF_sensors/TOP_FRONT_FACING_SDA)
    (add_net /ToF_sensors/TOP_RIGHT_FINGER_SCL)
    (add_net /power_generation_1/5V0)
    (add_net /power_generation_1/PG)
    (add_net /power_generation_2/EN1)
    (add_net /power_generation_2/EN2)
    (add_net /power_generation_2/EN3)
    (add_net /power_generation_2/FB1)
    (add_net /power_generation_2/FB2)
    (add_net /power_generation_2/FB3)
    (add_net /power_generation_2/PWR_IN)
    (add_net /xilinx_configuration/CCLK)
    (add_net /xilinx_configuration/CD)
    (add_net /xilinx_configuration/CLEAR_EEPROM)
    (add_net /xilinx_configuration/CS_B)
    (add_net /xilinx_configuration/D02)
    (add_net /xilinx_configuration/D03)
    (add_net /xilinx_configuration/DEBUG_PROD_B)
    (add_net /xilinx_configuration/DONE)
    (add_net /xilinx_configuration/DTR)
    (add_net /xilinx_configuration/FTDI_3V3)
    (add_net /xilinx_configuration/INIT_B)
    (add_net /xilinx_configuration/M0)
    (add_net /xilinx_configuration/M1)
    (add_net /xilinx_configuration/M2)
    (add_net /xilinx_configuration/MCLK)
    (add_net /xilinx_configuration/MISO)
    (add_net /xilinx_configuration/MOSI)
    (add_net /xilinx_configuration/NVRAM_SCL)
    (add_net /xilinx_configuration/NVRAM_SDA)
    (add_net /xilinx_configuration/OUT_EN)
    (add_net /xilinx_configuration/PROGRAM_B)
    (add_net /xilinx_configuration/RXI)
    (add_net /xilinx_configuration/SCLK)
    (add_net /xilinx_configuration/STATUS_0)
    (add_net /xilinx_configuration/STATUS_1)
    (add_net /xilinx_configuration/TCK)
    (add_net /xilinx_configuration/TDI)
    (add_net /xilinx_configuration/TDO)
    (add_net /xilinx_configuration/TMS)
    (add_net /xilinx_configuration/TXO)
    (add_net 12V0)
    (add_net 1V0)
    (add_net 1V8)
    (add_net 2V8)
    (add_net 3V3)
    (add_net 3V3_MICRO)
    (add_net 5V0)
    (add_net CLD_ES_SIG)
    (add_net DGND)
    (add_net FPGA_5V_EN)
    (add_net FPGA_BUCK_EN)
    (add_net FPGA_PGOOD)
    (add_net GRP_MOT_DIR)
    (add_net GRP_MOT_ENABLE_B)
    (add_net GRP_MOT_FAULT_B)
    (add_net GRP_MOT_M0)
    (add_net GRP_MOT_M1)
    (add_net GRP_MOT_SLEEP_B)
    (add_net GRP_MOT_STEP)
    (add_net IR_LED_EN_B)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(L3-Pad1)")
    (add_net "Net-(L4-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R51-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net OPN_ES_SIG)
    (add_net SCL_FPGA)
    (add_net SDA_FPGA)
    (add_net VP0)
    (add_net WHL_MOT_DIR)
    (add_net WHL_MOT_ENABLE_B)
    (add_net WHL_MOT_FAULT_B)
    (add_net WHL_MOT_M0)
    (add_net WHL_MOT_M1)
    (add_net WHL_MOT_SLEEP_B)
    (add_net WHL_MOT_STEP)
  )
  (module footprint:LTC3569EUD#TRPBF (layer F.Cu) (tedit 5C229686)
    (at 142.2019 120.34012 270)
    (descr "20-Lead Ultra Thin Plastic Quad Flat, No Lead Package (JP) - 3x3x0.50 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U11 (at 1.88468 3.1115 180) (layer F.SilkS))
    (fp_text value ﻿LTC3569EUD#PBF (at -5.53212 -55.0037 270) (layer F.Fab))
    (pad 21 thru_hole circle (at 0.3302 0.3429 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 21 thru_hole circle (at -0.3429 0.3429 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 21 thru_hole circle (at 0.3302 -0.3302 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 21 thru_hole circle (at -0.3429 -0.3302 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 21 smd circle (at 0 0 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at 0 0.6731 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at 0.6731 0 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at -0.6731 0 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at 0 -0.6731 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at -0.6731 0.6731 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at 0.6731 0.6731 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at 0.6731 -0.6731 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 21 smd circle (at -0.6731 -0.6731 270) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 1 smd oval (at -1.5 -0.8 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(L3-Pad1)"))
    (pad 2 smd oval (at -1.5 -0.4 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (pad 3 smd oval (at -1.5 0 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 49 FPGA_PGOOD))
    (pad 4 smd oval (at -1.5 0.4 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 5 smd oval (at -1.5 0.8 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (pad 6 smd oval (at -0.8 1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 101 /power_generation_2/FB2))
    (pad 7 smd oval (at -0.4 1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 100 /power_generation_2/FB1))
    (pad 8 smd oval (at 0 1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 102 /power_generation_2/FB3))
    (pad 9 smd oval (at 0.4 1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (pad 10 smd oval (at 0.8 1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (zone_connect 2))
    (pad 11 smd oval (at 1.5 0.8 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 97 /power_generation_2/EN3))
    (pad 12 smd oval (at 1.5 0.4 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 98 /power_generation_2/EN2))
    (pad 13 smd oval (at 1.5 0 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 99 /power_generation_2/EN1))
    (pad 14 smd oval (at 1.5 -0.4 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 15 smd oval (at 1.5 -0.8 270) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(L4-Pad1)"))
    (pad 16 smd oval (at 0.8 -1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (pad 17 smd oval (at 0.4 -1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (pad 18 smd oval (at 0 -1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(L2-Pad1)"))
    (pad 19 smd oval (at -0.4 -1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 20 smd oval (at -0.8 -1.5) (size 0.75 0.2) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:ATSHA204A-MAHCZ-T (layer F.Cu) (tedit 5C181AD9)
    (at 110.3376 138.0236 180)
    (fp_text reference U13 (at 0.7366 -4.7117 180) (layer F.SilkS))
    (fp_text value ﻿ATSHA204A-MAHCZ-T (at -19.7485 -20.31238 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 1.06 -1.45 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND) (zone_connect 2))
    (pad 4 thru_hole circle (at 0.43 -1.45 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND) (zone_connect 2))
    (pad 1 smd rect (at 0 0 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.5 0 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1 0 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.5 0 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 5 smd rect (at 1.5 -2.9 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1 -2.9 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0.5 -2.9 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 -2.9 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 4 smd circle (at 0.12 -1.76 180) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 4 smd circle (at 0.12332 -1.1384 180) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 4 smd circle (at 0.7466 -1.7584 180) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 4 smd circle (at 0.7466 -1.1384 180) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 4 smd circle (at 1.38 -1.14 180) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 4 smd circle (at 1.3816 -1.7584 180) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
  )
  (module footprint:DSC1033CI1-008.0000 (layer F.Cu) (tedit 5B671854)
    (at 91.8972 129.4638)
    (fp_text reference U1 (at -1.4732 0.9652 90) (layer F.SilkS))
    (fp_text value ﻿DSC1033CI1-008.0000 (at -35.4965 44.2722 -90) (layer F.Fab))
    (pad 4 smd rect (at 0 0) (size 0.889 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 3 smd rect (at 2.1082 0) (size 0.889 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 50 /xilinx_configuration/MCLK))
    (pad 2 smd rect (at 2.1082 1.8796) (size 0.889 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at 0 1.8796) (size 0.889 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 91.5028 126.8222 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.5788 -0.0762 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 41.2616 -7.1882 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 99.9109 122.7843 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.012 -1.3716 90) (layer B.SilkS))
    (fp_text value 0.1uF (at -32.4619 -15.1892 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 3V3_MICRO))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 104.5845 109.2207 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.5 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 16.3075 3.3401 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 /xilinx_configuration/DTR))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 102.8065 123.2542 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.3716 90) (layer B.SilkS))
    (fp_text value 0.1uF (at -9.1941 77.2414 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 110.0956 109.1946)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.5) (layer B.SilkS))
    (fp_text value 0.1uF (at -0.2152 11.7856) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 90.678 140.2468 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.4264 0.0762 90) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.7486 -23.0378 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 127.0508 119.7356 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.397 90) (layer B.SilkS))
    (fp_text value 0.1uF (at -21.9202 -54.3306 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 153.0604 147.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.7211 -0.0508 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.2032 -22.5044 270) (layer F.Fab))
    (fp_text user %R (at 1.254 -22.1488 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 148.2478 149.479 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.55848 -0.01524 180) (layer F.SilkS))
    (fp_text value 3.3nF (at -26.658 1.4478 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 152.84888 140.49248 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 2.92538 0.00508 180) (layer F.SilkS))
    (fp_text value 1uF (at -22.81104 -6.36016 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 153.0604 143.1892 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 22uF (at -10.7442 -26.8986 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 96 /power_generation_1/5V0))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 152.85396 138.79068 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 2.93046 -0.02032 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -27.8758 3.59664 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 /power_generation_1/5V0))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 142.1384 143.60836 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 1uF (at -5.3333 35.0266 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 152.85212 133.2484 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3.163 -0.0254 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -28.11456 -2.26568 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5C229669)
    (at 138.4427 119.7196 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0.1618 1.6891 270) (layer F.SilkS))
    (fp_text value 22uF (at -7.1468 -58.6613 270) (layer F.Fab))
    (fp_text user %R (at -0.6698 -58.6613 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (zone_connect 2))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 146.9042 124.1552 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0.0033 -1.7526 180) (layer F.SilkS))
    (fp_text value 22uF (at -50.1998 5.5626 270) (layer F.Fab))
    (fp_text user %R (at -50.1998 5.207 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 143.8275 115.93652 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at -2.44932 -0.0127) (layer F.SilkS))
    (fp_text value 10uF (at -1.48412 -53.3019 270) (layer F.Fab))
    (fp_text user %R (at -2.52552 -53.2765 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 143.764 124.97232 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at -2.6576 0.01016 180) (layer F.SilkS))
    (fp_text value 10uF (at 13.92352 53.5178 90) (layer F.Fab))
    (fp_text user %R (at 14.38072 53.5178 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 149.004901 91.076901)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 47uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 144.954901 91.246901)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C24 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 144.454901 93.236901)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 47uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 146.954901 97.051901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 147.654901 93.001901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 153.354901 92.191901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 150.504901 95.361901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 150.504901 94.011901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5C28BB93)
    (at 80.6997 86.7283)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C31 (at 2.1248 0.0508) (layer B.SilkS))
    (fp_text value 0.47uF (at 98.7298 -15.24) (layer B.Fab))
    (fp_text user %R (at 100.1014 -14.9352) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 1V0))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 144.104901 96.641901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 159.893 102.9462 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C33 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 157.504901 90.696901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C34 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5C28BB9E)
    (at 83.1684 85.598 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C35 (at 2.1756 -0.0254 180) (layer B.SilkS))
    (fp_text value 0.47uF (at 94.0728 -13.0302 180) (layer B.Fab))
    (fp_text user %R (at 95.2666 -12.827 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 1V0))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 155.235701 99.335501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C36 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5C28BB81)
    (at 80.7427 87.8586 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C37 (at -2.1932 -0.0254 180) (layer B.SilkS))
    (fp_text value 0.47uF (at 79.6456 -40.8432 180) (layer B.Fab))
    (fp_text user %R (at 79.6456 -40.005 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 1V0))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 160.685701 99.345501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C38 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5C28C5FB)
    (at 82.5881 103.6447 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C39 (at 0 -0.9398 180) (layer F.SilkS))
    (fp_text value 0.47uF (at -134.1667 14.1224 180) (layer F.Fab))
    (fp_text user %R (at -90.255 -11.5316 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 156.585701 100.395501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C40 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5C28C4A5)
    (at 85.1408 89.7089 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C41 (at 2.1297 0.0254 90) (layer B.SilkS))
    (fp_text value 0.47uF (at 101.769 2.8702 90) (layer B.Fab))
    (fp_text user %R (at 90.3136 -15.2654 90) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 155.054901 90.841901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C42 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 147.654901 95.701901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C43 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 157.054901 93.876901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C44 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 150.504901 92.661901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 158.635701 100.395501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C46 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 147.654901 94.351901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C47 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 157.854901 92.816901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C48 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 154.204901 95.516901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C49 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 157.854901 91.756901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C50 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 155.004901 94.456901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C51 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 155.785701 101.455501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C52 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 146.554901 98.256901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C53 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 144.104901 97.991901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C54 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 144.454901 95.056901)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C55 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 47uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 152.204901 90.841901)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C56 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 157.285701 99.335501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C57 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 155.804901 92.046901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C58 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 148.604901 98.686901)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C59 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 154.535701 100.395501)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C60 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 110.4552 119.9236 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.4544 -0.0152 270) (layer B.SilkS))
    (fp_text value FDV302P (at -42.2054 14.605 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 32 /xilinx_configuration/INIT_B))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 151.8818 128.1778 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.5146 0.0508 180) (layer F.SilkS))
    (fp_text value FDV301N (at 16.018 -21.397 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 94 /power_generation_1/PG))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 142.9512 137.0076 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 2.5 270) (layer B.SilkS))
    (fp_text value MMBT3904 (at 27.6192 -5.2832 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 90 FPGA_5V_EN))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 144.2974 136.9318 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q4 (at 5.2836 0.0254 180) (layer F.SilkS))
    (fp_text value BSP250 (at 2.3118 45.7454) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q3-Pad3)"))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 5V0))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (pad 4 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 95 /power_generation_2/PWR_IN))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 132.0546 121.2883 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at -2.4417 0) (layer B.SilkS))
    (fp_text value FDV301N (at -7.1153 64.9224 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 49 FPGA_PGOOD))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 104.3933 116.0145)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45) (layer B.SilkS))
    (fp_text value 750R (at -32.5762 -4.9403) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 /xilinx_configuration/FTDI_3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 99.5807 109.1946 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 10k (at 4.2171 30.9118 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.1308 136.5003 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 10k (at -3.6583 -47.3964 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 36 /xilinx_configuration/M0))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 97.4598 139.9166 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.401 0 270) (layer F.SilkS))
    (fp_text value 100R (at 0.8248 30.0228 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /xilinx_configuration/TCK))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 101.4476 139.9166 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.401 0 270) (layer F.SilkS))
    (fp_text value 100R (at 0.9772 33.909 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /xilinx_configuration/TDI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 95.4532 139.9166 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.401 0 270) (layer F.SilkS))
    (fp_text value 100R (at 0.8248 28.1178 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /xilinx_configuration/TMS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 99.441 139.9152 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -2.3996 0 270) (layer F.SilkS))
    (fp_text value 100R (at 0.8008 32.0802 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /xilinx_configuration/TDO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 95.7319 116.1161)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.4758 0.0508) (layer F.SilkS))
    (fp_text value 10k (at -25.6787 1.905) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /xilinx_configuration/M1))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 95.7319 114.2492)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.4758 0.0762) (layer F.SilkS))
    (fp_text value 10k (at -25.7168 3.7846) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /xilinx_configuration/M2))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.6955 136.8044)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -0.0127 1.5748) (layer F.SilkS))
    (fp_text value 750R (at -36.2832 -1.0541) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 /xilinx_configuration/STATUS_0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 113.8421 108.6104 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -2.8963 -0.0381 180) (layer F.SilkS))
    (fp_text value 10k (at -36.7404 -0.9779 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /xilinx_configuration/NVRAM_SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 113.8294 110.3503 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -2.909 -0.0381 180) (layer F.SilkS))
    (fp_text value 10k (at 14.2487 16.7005 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 /xilinx_configuration/NVRAM_SDA))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 98.4003 130.302 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.9711 -0.0762 180) (layer F.SilkS))
    (fp_text value 750R (at 48.375 -3.6322 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /xilinx_configuration/STATUS_1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 133.6929 133.9208 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 2.8582 -0.0254 270) (layer B.SilkS))
    (fp_text value 1k (at -9.5878 -39.2938 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 113.931 143.4846)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 1.45) (layer B.SilkS))
    (fp_text value 1k (at -41.4902 -10.0076) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 122.555 120.4842 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 2.6804 -0.0254 270) (layer F.SilkS))
    (fp_text value 22R (at 74.156 -7.0358 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /xilinx_configuration/CCLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 96.012 127.4826)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 1.45) (layer B.SilkS))
    (fp_text value 200R (at -23.6855 5.4991) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 /xilinx_configuration/DONE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 109.486 142.8877)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -0.0127 1.5494) (layer B.SilkS))
    (fp_text value 4k7 (at 42.5711 8.0645) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 /xilinx_configuration/PROGRAM_B))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 107.3016 117.9576)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 4k7 (at -7.4923 -24.3967) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /xilinx_configuration/INIT_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 106.438 136.8044)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 2.8328 0.0254) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 /xilinx_configuration/CS_B))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 109.4486 116.1676 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at -0.012 -1.4986 90) (layer B.SilkS))
    (fp_text value 750R (at -46.3042 11.2776 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 112.1911 123.1773)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 2.8074 0.0635) (layer B.SilkS))
    (fp_text value 4k7 (at -44.6913 -12.7635) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 103 /xilinx_configuration/D02))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 127 122.5423 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at -0.0127 1.4478 90) (layer B.SilkS))
    (fp_text value 4k7 (at 52.4771 -2.6543 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 104 /xilinx_configuration/D03))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.3802 147.14544 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0.02356 1.53924 270) (layer F.SilkS))
    (fp_text value 100k (at 1.4231 -30.3403 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 /power_generation_1/PG))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 146.9136 136.9942 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at -2.7806 -0.0254 270) (layer B.SilkS))
    (fp_text value 10k (at -8.648 -58.42 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 5V0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.9136 118.80272 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at 2.8328 0.0254 90) (layer F.SilkS))
    (fp_text value 33k2 (at 6.00132 50.0634 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /power_generation_2/FB1))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.7087 115.59032 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at 2.9203 -0.0254 180) (layer F.SilkS))
    (fp_text value 150k (at -58.2683 1.13792 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /power_generation_2/FB2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.5069 125.83922 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R41 (at 2.782 -0.10668 180) (layer F.SilkS))
    (fp_text value 180k (at -58.4955 6.05282 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /power_generation_2/FB3))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 148.6408 118.81542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R42 (at 2.8568 0.0381 90) (layer F.SilkS))
    (fp_text value 133k (at -0.81858 48.4632 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /power_generation_2/FB1))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.696 113.87582 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R43 (at 2.8836 -0.0762 180) (layer F.SilkS))
    (fp_text value 120k (at -58.4334 3.28422 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /power_generation_2/FB2))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.5069 127.59182 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R44 (at 2.782 -0.08128 180) (layer F.SilkS))
    (fp_text value 57.6k (at -58.7495 8.21182 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /power_generation_2/FB3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 132.461 121.043 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R45 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 100k (at -21.2845 36.4363 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 FPGA_PGOOD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.2827 111.2259 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R49 (at -2.9344 0.0254 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 CLD_ES_SIG))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 126.492 111.2259 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R50 (at -2.9598 0.0254 90) (layer F.SilkS))
    (fp_text value 10k (at -3.6075 48.9204 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 OPN_ES_SIG))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E)
    (at 110.1496 110.2946 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U3 (at 2.624 -0.9804 180) (layer F.SilkS))
    (fp_text value ﻿24LC014T-IOT (at -45.2452 -22.418 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 84 /xilinx_configuration/NVRAM_SDA))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 85 /xilinx_configuration/NVRAM_SCL))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E)
    (at 145.0086 143.56588 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U9 (at 2.1717 -2.38252 180) (layer F.SilkS))
    (fp_text value ﻿MIC5504-2.8YM5-TR (at -30.3911 -4.2672 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:5025700893 (layer B.Cu) (tedit 5BD7806A)
    (at 90.043 134.112 270)
    (fp_text reference J3 (at -1.905 -14.4018) (layer B.SilkS))
    (fp_text value ﻿5025700893 (at 25.019 -12.5476) (layer B.Fab))
    (pad 11 smd trapezoid (at 0 0 270) (size 1.397 1.7018) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 11 smd trapezoid (at 12.9032 0 270) (size 1.397 1.7018) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 11 smd trapezoid (at 3.5433 -14.4526 270) (size 1.4986 1.143) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 11 smd trapezoid (at 12.8524 -14.4526 270) (size 1.4986 1.143) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd trapezoid (at 11.43 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd trapezoid (at 10.33018 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 62 /xilinx_configuration/CS_B))
    (pad 3 smd trapezoid (at 9.23036 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 63 /xilinx_configuration/MOSI))
    (pad 4 smd trapezoid (at 8.13054 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 5 smd trapezoid (at 7.03072 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 105 /xilinx_configuration/CCLK))
    (pad 6 smd trapezoid (at 5.9309 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 7 smd trapezoid (at 4.83108 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(J3-Pad7)"))
    (pad 8 smd trapezoid (at 3.73126 -2.8956 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd trapezoid (at 5.8547 -14.4526 270) (size 1.4986 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 10 smd rect (at 13.0302 -9.7536 270) (size 1.143 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 35 /xilinx_configuration/CD))
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 99.048 150.1394 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.8568 -0.0127 180) (layer B.SilkS))
    (fp_text value 10k (at 25.8071 -4.9276 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 /xilinx_configuration/CD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 96.5708 111.8877 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 2.7947 0.0508 90) (layer B.SilkS))
    (fp_text value 10k (at 2.0835 29.2989 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 /xilinx_configuration/CLEAR_EEPROM))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 95.0595 111.9004 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 2.782 0.0381 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /xilinx_configuration/DEBUG_PROD_B))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:NL27WZ126 (layer F.Cu) (tedit 5BD92712)
    (at 106.7689 129.1314 180)
    (fp_text reference U4 (at 2.516 -1.4119 90) (layer F.SilkS))
    (fp_text value ﻿NL27WZ126 (at 2.9224 40.1066 180) (layer F.Fab))
    (pad 8 smd rect (at 0 -2.72 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 7 smd rect (at 0.5 -2.72 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 69 /xilinx_configuration/OUT_EN))
    (pad 6 smd rect (at 1 -2.72 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 105 /xilinx_configuration/CCLK))
    (pad 5 smd rect (at 1.5 -2.72 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J3-Pad7)"))
    (pad 4 smd rect (at 1.5 0 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at 1 0 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 51 /xilinx_configuration/MISO))
    (pad 2 smd rect (at 0.5 -0.00254 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 46 /xilinx_configuration/SCLK))
    (pad 1 smd rect (at 0 0 180) (size 0.3 0.68) (layers F.Cu F.Paste F.Mask)
      (net 69 /xilinx_configuration/OUT_EN))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 131.040136 141.957046)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C61 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 59.6272 4.5212) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 /ADC/VP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 88 /ADC/VN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 118.81288 134.27964)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C63 (at 0 1.5) (layer B.SilkS))
    (fp_text value 100nF (at -46.8496 -3.048) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 92 /ADC/VCCADC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 91 /ADC/VREFN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C2A5DAB)
    (at 121.7048 133.0198)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C65 (at 2.6028 0.0889) (layer B.SilkS))
    (fp_text value 100nF (at 57.4174 -0.508) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 91 /ADC/VREFN))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 89 /ADC/VREFP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 131.040136 143.811246)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R52 (at 0.012 1.524) (layer F.SilkS))
    (fp_text value 100R (at -20.7398 -33.6296 -90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 VP0))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /ADC/VP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 134.189736 141.957046)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R53 (at 0.0134 -1.4986) (layer F.SilkS))
    (fp_text value 100R (at 30.3664 -17.9832) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /ADC/VN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R51-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 134.191136 143.811246 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R51 (at -0.0642 -1.524 180) (layer F.SilkS))
    (fp_text value 698R (at 28.4226 -15.24 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R51-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:0878325623 (layer F.Cu) (tedit 5BEA645A)
    (at 93.4466 147.4552)
    (fp_text reference J2 (at 15.6718 0.6268 -180) (layer F.SilkS))
    (fp_text value Conn_02x07_Odd_Even (at 16.5862 11.3456 -180) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at 0 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 3 smd rect (at 2 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 4 smd rect (at 2 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 24 /xilinx_configuration/TMS))
    (pad 5 smd rect (at 4 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 6 smd rect (at 4 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 27 /xilinx_configuration/TCK))
    (pad 7 smd rect (at 6 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 8 smd rect (at 6 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 26 /xilinx_configuration/TDO))
    (pad 9 smd rect (at 8 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 10 smd rect (at 8 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 25 /xilinx_configuration/TDI))
    (pad 11 smd rect (at 10 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 12 smd rect (at 10 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 12 0) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 14 smd rect (at 12 -4.25) (size 1 2.75) (layers F.Cu F.Paste F.Mask))
    (pad "" thru_hole circle (at 1 -2.13) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 11 -2.13) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer B.Cu) (tedit 58CC8F64)
    (at 121.285 121.2342)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at -3.9116 -3.048) (layer B.SilkS))
    (fp_text value ﻿S25FL127SABMFI101 (at 36.4693 -0.4826 90) (layer B.Fab))
    (fp_text user %R (at 1.778 -36.7538) (layer B.Fab))
    (pad 8 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 7 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 104 /xilinx_configuration/D03))
    (pad 6 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(R22-Pad1)"))
    (pad 5 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 63 /xilinx_configuration/MOSI))
    (pad 4 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 103 /xilinx_configuration/D02))
    (pad 2 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 51 /xilinx_configuration/MISO))
    (pad 1 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 62 /xilinx_configuration/CS_B))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 58CE4E7F)
    (at 98.5164 134.732 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U5 (at 0.0152 2.0043) (layer F.SilkS))
    (fp_text value ﻿CM1213A-04S7 (at -13.31468 -29.16682 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 /xilinx_configuration/TMS))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 /xilinx_configuration/TCK))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 /xilinx_configuration/TDO))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 /xilinx_configuration/TDI))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:M2_hole_for_socket_cap (layer F.Cu) (tedit 5BFB33FD)
    (at 91.948 154.432)
    (fp_text reference MH1 (at 6.985 4.5085) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 9.9822 4.4323) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module footprint:M2_hole_for_socket_cap (layer F.Cu) (tedit 5BFB3410)
    (at 151.892 154.432)
    (fp_text reference MH2 (at -47.0408 4.4577) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -49.5554 4.4069) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module footprint:M2_hole_for_socket_cap (layer F.Cu) (tedit 5BFB344B)
    (at 151.892 109.728)
    (fp_text reference MH3 (at -49.9618 48.9966) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -49.8602 48.8823) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module footprint:M2_hole_for_socket_cap (layer F.Cu) (tedit 5BFB342C)
    (at 91.948 109.728)
    (fp_text reference MH4 (at 9.6139 48.9585) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 9.779 48.9077) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module footprint:M2_hole_for_socket_cap (layer F.Cu) (tedit 5BFB396D)
    (at 91.948 122.3772)
    (fp_text reference MH5 (at 18.0086 36.7284) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 22.9108 36.4236) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module footprint:M2_hole_for_socket_cap (layer F.Cu) (tedit 5BFB3979)
    (at 151.892 122.3772)
    (fp_text reference MH6 (at -32.258 36.6776) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -35.2044 36.576) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module footprint:218-2LPSTR (layer B.Cu) (tedit 5BFB74E1)
    (at 90.805 116.078 90)
    (fp_text reference SW1 (at -2.3114 5.334) (layer B.SilkS))
    (fp_text value SW_DIP_x02 (at -42.72026 11.41984) (layer B.Fab))
    (pad 1 smd rect (at -0.01 0 90) (size 0.762 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 1.27 0 90) (size 0.762 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 3V3))
    (pad 3 smd rect (at 1.27 7.62 90) (size 0.762 1.27) (layers B.Cu B.Paste B.Mask)
      (net 44 /xilinx_configuration/CLEAR_EEPROM))
    (pad 4 smd rect (at 0 7.62 90) (size 0.762 1.27) (layers B.Cu B.Paste B.Mask)
      (net 45 /xilinx_configuration/DEBUG_PROD_B))
  )
  (module "footprint:S4B-PH-SM4-TB(LF)(SN)" (layer F.Cu) (tedit 5C01B486)
    (at 133.458 155.4596 180)
    (fp_text reference J4 (at -0.273 6.5902 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 18.4468 -3.4428 180) (layer F.Fab))
    (pad "" smd rect (at -0.4 -0.09 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1.95 5.22 180) (size 1.1 4) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (pad 2 smd rect (at 3.95 5.22 180) (size 1.1 4) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 3 smd rect (at 5.95 5.21 180) (size 1.1 4) (layers F.Cu F.Paste F.Mask)
      (net 75 SCL_FPGA))
    (pad 4 smd rect (at 7.95 5.22 180) (size 1.1 4) (layers F.Cu F.Paste F.Mask)
      (net 76 SDA_FPGA))
    (pad "" smd rect (at 10.3 -0.09 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
  )
  (module footprint:0533071871 (layer F.Cu) (tedit 5C0C3DBD)
    (at 119.5123 109.6772 270)
    (fp_text reference J9 (at -1.3208 -5.4684) (layer F.SilkS))
    (fp_text value Conn_02x09_Counter_Clockwise (at -4.3815 8.4889) (layer F.Fab))
    (pad 18 smd rect (at 0 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (pad 17 smd rect (at 0.8 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 16 smd rect (at 1.6 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 78 CLD_ES_SIG))
    (pad 15 smd rect (at 2.4 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 79 OPN_ES_SIG))
    (pad 14 smd rect (at 3.2 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 72 GRP_MOT_M1))
    (pad 13 smd rect (at 4 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 74 GRP_MOT_M0))
    (pad 12 smd rect (at 4.8 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 57 GRP_MOT_FAULT_B))
    (pad 11 smd rect (at 5.6 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 53 GRP_MOT_ENABLE_B))
    (pad 10 smd rect (at 6.4 -4.3 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 55 GRP_MOT_STEP))
    (pad 9 smd rect (at 6.4 -0.01 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 56 GRP_MOT_DIR))
    (pad 8 smd rect (at 5.6 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 54 GRP_MOT_SLEEP_B))
    (pad 7 smd rect (at 4.8 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 71 WHL_MOT_M1))
    (pad 6 smd rect (at 4 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 73 WHL_MOT_M0))
    (pad 5 smd rect (at 3.2 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 52 WHL_MOT_FAULT_B))
    (pad 4 smd rect (at 2.4 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 31 WHL_MOT_DIR))
    (pad 3 smd rect (at 1.6 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 59 WHL_MOT_STEP))
    (pad 2 smd rect (at 0.8 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 58 WHL_MOT_ENABLE_B))
    (pad 1 smd rect (at 0 0 270) (size 0.55 1.8) (layers F.Cu F.Paste F.Mask)
      (net 60 WHL_MOT_SLEEP_B))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 107.3531 139.4086 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C66 (at -0.0501 -1.3843 90) (layer F.SilkS))
    (fp_text value 0.1uF (at -38.6835 4.826 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:XC7AxxT-1FTG256C (layer F.Cu) (tedit 5C197238)
    (at 112.7196 141.0208 90)
    (fp_text reference U6 (at 16.9672 15.1694 180) (layer F.SilkS))
    (fp_text value ﻿xc7aXXtftg256 (at 19.70532 -25.01646 90) (layer F.Fab))
    (pad A1 smd circle (at 0 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad A2 smd circle (at 1 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 108 /ToF_sensors/TOF_LEFT_FINGER_INT))
    (pad A3 smd circle (at 2 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 107 /ToF_sensors/TOF_LEFT_FINGER_SCL))
    (pad A4 smd circle (at 3 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 106 /ToF_sensors/TOF_LEFT_FINGER_SDA))
    (pad A5 smd circle (at 4 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 30 /ToF_sensors/TOF_TOP_FINGER_INT))
    (pad A6 smd circle (at 5 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad A7 smd circle (at 6 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 28 /ToF_sensors/TOF_TOP_FINGER_SDA))
    (pad A8 smd circle (at 7 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad A9 smd circle (at 8 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad A10 smd circle (at 9 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd circle (at 10 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad A12 smd circle (at 11 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad A13 smd circle (at 12 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 85 /xilinx_configuration/NVRAM_SCL))
    (pad A14 smd circle (at 13 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 84 /xilinx_configuration/NVRAM_SDA))
    (pad A15 smd circle (at 14 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 60 WHL_MOT_SLEEP_B))
    (pad A16 smd circle (at 15 0 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad B1 smd circle (at 0 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 112 /ToF_sensors/TOP_FRONT_FACING_SDA))
    (pad B2 smd circle (at 1 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at 2 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad B4 smd circle (at 3 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd circle (at 4 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd circle (at 5 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 29 /ToF_sensors/TOF_TOP_FINGER_SCL))
    (pad B7 smd circle (at 6 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B8 smd circle (at 7 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad B9 smd circle (at 8 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B10 smd circle (at 9 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B11 smd circle (at 10 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B12 smd circle (at 11 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B13 smd circle (at 12 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad B14 smd circle (at 13 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B15 smd circle (at 14 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad B16 smd circle (at 15 1 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 58 WHL_MOT_ENABLE_B))
    (pad C1 smd circle (at 0 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 113 /ToF_sensors/TOF_FRONT_FACING_SCL))
    (pad C2 smd circle (at 1 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at 2 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C4 smd circle (at 3 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C5 smd circle (at 4 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad C6 smd circle (at 5 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C7 smd circle (at 6 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C8 smd circle (at 7 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C9 smd circle (at 8 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C10 smd circle (at 9 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad C11 smd circle (at 10 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C12 smd circle (at 11 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd circle (at 12 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd circle (at 13 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad C15 smd circle (at 14 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad C16 smd circle (at 15 2 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 59 WHL_MOT_STEP))
    (pad D1 smd circle (at 0 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 114 /ToF_sensors/TOF_FRONT_FACING_INT))
    (pad D2 smd circle (at 1 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad D3 smd circle (at 2 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D4 smd circle (at 3 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D5 smd circle (at 4 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D6 smd circle (at 5 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D7 smd circle (at 6 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad D8 smd circle (at 7 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D9 smd circle (at 8 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D10 smd circle (at 9 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D11 smd circle (at 10 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D12 smd circle (at 11 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad D13 smd circle (at 12 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D14 smd circle (at 13 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad D15 smd circle (at 14 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 78 CLD_ES_SIG))
    (pad D16 smd circle (at 15 3 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 31 WHL_MOT_DIR))
    (pad E1 smd circle (at 0 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 76 SDA_FPGA))
    (pad E2 smd circle (at 1 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E3 smd circle (at 2 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E4 smd circle (at 3 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad E5 smd circle (at 4 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E6 smd circle (at 5 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E7 smd circle (at 6 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R16-Pad2)"))
    (pad E8 smd circle (at 7 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 105 /xilinx_configuration/CCLK))
    (pad E9 smd circle (at 8 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad E10 smd circle (at 9 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad E11 smd circle (at 10 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E12 smd circle (at 11 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E13 smd circle (at 12 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad E14 smd circle (at 13 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad E15 smd circle (at 14 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 79 OPN_ES_SIG))
    (pad E16 smd circle (at 15 4 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 52 WHL_MOT_FAULT_B))
    (pad F1 smd circle (at 0 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad F2 smd circle (at 1 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F3 smd circle (at 2 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F4 smd circle (at 3 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F5 smd circle (at 4 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F6 smd circle (at 5 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad F7 smd circle (at 6 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad F8 smd circle (at 7 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad F9 smd circle (at 8 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad F10 smd circle (at 9 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad F11 smd circle (at 10 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad F12 smd circle (at 11 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F13 smd circle (at 12 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F14 smd circle (at 13 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F15 smd circle (at 14 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad F16 smd circle (at 15 5 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad G1 smd circle (at 0 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 75 SCL_FPGA))
    (pad G2 smd circle (at 1 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad G3 smd circle (at 2 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad G4 smd circle (at 3 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad G5 smd circle (at 4 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad G6 smd circle (at 5 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad G7 smd circle (at 6 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad G8 smd circle (at 7 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 92 /ADC/VCCADC))
    (pad G9 smd circle (at 8 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad G10 smd circle (at 9 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad G11 smd circle (at 10 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 70 IR_LED_EN_B))
    (pad G12 smd circle (at 11 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad G13 smd circle (at 12 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad G14 smd circle (at 13 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad G15 smd circle (at 14 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad G16 smd circle (at 15 6 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 73 WHL_MOT_M0))
    (pad H1 smd circle (at 0 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 109 /ToF_sensors/TOF_RIGHT_FINGER_SDA))
    (pad H2 smd circle (at 1 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H3 smd circle (at 2 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H4 smd circle (at 3 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H5 smd circle (at 4 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H6 smd circle (at 5 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad H7 smd circle (at 6 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad H8 smd circle (at 7 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 87 /ADC/VP))
    (pad H9 smd circle (at 8 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad H10 smd circle (at 9 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 47 /xilinx_configuration/DONE))
    (pad H11 smd circle (at 10 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H12 smd circle (at 11 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H13 smd circle (at 12 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H14 smd circle (at 13 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad H15 smd circle (at 14 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad H16 smd circle (at 15 7 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 71 WHL_MOT_M1))
    (pad J1 smd circle (at 0 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 110 /ToF_sensors/TOP_RIGHT_FINGER_SCL))
    (pad J2 smd circle (at 1 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad J3 smd circle (at 2 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad J4 smd circle (at 3 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad J5 smd circle (at 4 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad J6 smd circle (at 5 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad J7 smd circle (at 6 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 88 /ADC/VN))
    (pad J8 smd circle (at 7 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 89 /ADC/VREFP))
    (pad J9 smd circle (at 8 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad J10 smd circle (at 9 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad J11 smd circle (at 10 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad J12 smd circle (at 11 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad J13 smd circle (at 12 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 63 /xilinx_configuration/MOSI))
    (pad J14 smd circle (at 13 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 51 /xilinx_configuration/MISO))
    (pad J15 smd circle (at 14 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad J16 smd circle (at 15 8 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 54 GRP_MOT_SLEEP_B))
    (pad K1 smd circle (at 0 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 111 /ToF_sensors/TOF_RIGHT_FINGER_INT))
    (pad K2 smd circle (at 1 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad K3 smd circle (at 2 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad K4 smd circle (at 3 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad K5 smd circle (at 4 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad K6 smd circle (at 5 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad K7 smd circle (at 6 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad K8 smd circle (at 7 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad K9 smd circle (at 8 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad K10 smd circle (at 9 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 32 /xilinx_configuration/INIT_B))
    (pad K11 smd circle (at 10 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad K12 smd circle (at 11 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad K13 smd circle (at 12 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad K14 smd circle (at 13 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad K15 smd circle (at 14 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 103 /xilinx_configuration/D02))
    (pad K16 smd circle (at 15 9 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 104 /xilinx_configuration/D03))
    (pad L1 smd circle (at 0 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad L2 smd circle (at 1 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad L3 smd circle (at 2 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad L4 smd circle (at 3 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad L5 smd circle (at 4 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad L6 smd circle (at 5 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad L7 smd circle (at 6 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R6-Pad1)"))
    (pad L8 smd circle (at 7 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad L9 smd circle (at 8 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 48 /xilinx_configuration/PROGRAM_B))
    (pad L10 smd circle (at 9 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad L11 smd circle (at 10 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad L12 smd circle (at 11 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 62 /xilinx_configuration/CS_B))
    (pad L13 smd circle (at 12 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad L14 smd circle (at 13 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad L15 smd circle (at 14 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(R15-Pad2)"))
    (pad L16 smd circle (at 15 10 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad M1 smd circle (at 0 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd circle (at 1 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd circle (at 2 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad M4 smd circle (at 3 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M5 smd circle (at 4 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M6 smd circle (at 5 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M7 smd circle (at 6 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R8-Pad1)"))
    (pad M8 smd circle (at 7 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad M9 smd circle (at 8 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 36 /xilinx_configuration/M0))
    (pad M10 smd circle (at 9 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 41 /xilinx_configuration/M1))
    (pad M11 smd circle (at 10 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 40 /xilinx_configuration/M2))
    (pad M12 smd circle (at 11 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M13 smd circle (at 12 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad M14 smd circle (at 13 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M15 smd circle (at 14 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad M16 smd circle (at 15 11 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 56 GRP_MOT_DIR))
    (pad N1 smd circle (at 0 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N2 smd circle (at 1 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N3 smd circle (at 2 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N4 smd circle (at 3 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N5 smd circle (at 4 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad N6 smd circle (at 5 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N7 smd circle (at 6 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad1)"))
    (pad N8 smd circle (at 7 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R9-Pad1)"))
    (pad N9 smd circle (at 8 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N10 smd circle (at 9 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad N11 smd circle (at 10 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N12 smd circle (at 11 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N13 smd circle (at 12 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad N14 smd circle (at 13 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 50 /xilinx_configuration/MCLK))
    (pad N15 smd circle (at 14 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad N16 smd circle (at 15 12 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 72 GRP_MOT_M1))
    (pad P1 smd circle (at 0 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P2 smd circle (at 1 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad P3 smd circle (at 2 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P4 smd circle (at 3 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P5 smd circle (at 4 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P6 smd circle (at 5 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P7 smd circle (at 6 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad P8 smd circle (at 7 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P9 smd circle (at 8 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P10 smd circle (at 9 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P11 smd circle (at 10 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P12 smd circle (at 11 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad P13 smd circle (at 12 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P14 smd circle (at 13 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P15 smd circle (at 14 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad P16 smd circle (at 15 13 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 74 GRP_MOT_M0))
    (pad R1 smd circle (at 0 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R2 smd circle (at 1 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R3 smd circle (at 2 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R4 smd circle (at 3 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad R5 smd circle (at 4 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R6 smd circle (at 5 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R7 smd circle (at 6 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R8 smd circle (at 7 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R9 smd circle (at 8 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad R10 smd circle (at 9 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R11 smd circle (at 10 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R12 smd circle (at 11 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R13 smd circle (at 12 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R14 smd circle (at 13 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad R15 smd circle (at 14 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad R16 smd circle (at 15 14 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 57 GRP_MOT_FAULT_B))
    (pad T1 smd circle (at 0 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad T2 smd circle (at 1 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T3 smd circle (at 2 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T4 smd circle (at 3 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T5 smd circle (at 4 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T6 smd circle (at 5 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad T7 smd circle (at 6 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T8 smd circle (at 7 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T9 smd circle (at 8 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T10 smd circle (at 9 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T11 smd circle (at 10 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad T12 smd circle (at 11 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T13 smd circle (at 12 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask))
    (pad T14 smd circle (at 13 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 53 GRP_MOT_ENABLE_B))
    (pad T15 smd circle (at 14 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 55 GRP_MOT_STEP))
    (pad T16 smd circle (at 15 15 90) (size 0.39 0.39) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 120.9414 146.9898 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C64 (at 2.9457 -0.0508 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -53.86 8.1026 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 89 /ADC/VREFP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 120.1547 144.256 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U12 (at -0.0475 2.6924 270) (layer F.SilkS))
    (fp_text value ﻿REF3012AIDBZR (at 58.7756 -10.922 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 89 /ADC/VREFP))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 117.4496 144.3094 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C67 (at -0.0374 1.3716 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 64.3262 -10.1854 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:smt_wire_pad_single_side_8pos (layer F.Cu) (tedit 5C1D10DC)
    (at 133.8214 108.922)
    (fp_text reference J5 (at 14.2606 0.044) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 5.08 -3.302) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 70 IR_LED_EN_B))
    (pad 2 smd rect (at 1.778 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 3 smd rect (at 3.556 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (pad 4 smd rect (at 5.334 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 30 /ToF_sensors/TOF_TOP_FINGER_INT))
    (pad 5 smd rect (at 7.112 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 29 /ToF_sensors/TOF_TOP_FINGER_SCL))
    (pad 6 smd rect (at 8.89 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 28 /ToF_sensors/TOF_TOP_FINGER_SDA))
    (pad 7 smd rect (at 10.668 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 8 smd rect (at 12.446 0) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 77 VP0))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 127.7366 144.5856 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C62 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.47uF (at -0.1358 -46.0502 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 91 /ADC/VREFN))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 92 /ADC/VCCADC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "footprint:S5B-ZR-SM4A-TF(LF)(SN)" (layer F.Cu) (tedit 5BF1FC96)
    (at 96.6246 108.9374)
    (fp_text reference J1 (at 11.3254 3.2798) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 3.7 -4.1) (layer F.Fab))
    (pad "" smd rect (at 10.04 -0.2) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 6.45 3.5) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /xilinx_configuration/RXI))
    (pad 3 smd rect (at 4.95 3.5) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /xilinx_configuration/TXO))
    (pad 2 smd rect (at 3.45 3.5) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /xilinx_configuration/FTDI_3V3))
    (pad 1 smd rect (at 1.95 3.5) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad "" smd rect (at -0.14 -0.2) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 7.95 3.5) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /xilinx_configuration/DTR))
  )
  (module "footprint:S5B-ZR-SM4A-TF(LF)(SN)" (layer F.Cu) (tedit 5BF1FC96)
    (at 107.2004 155.2226 180)
    (fp_text reference J6 (at 0.4442 4.7276 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 3.7 -4.1 180) (layer F.Fab))
    (pad "" smd rect (at 10.04 -0.2 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 6.45 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 106 /ToF_sensors/TOF_LEFT_FINGER_SDA))
    (pad 3 smd rect (at 4.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 107 /ToF_sensors/TOF_LEFT_FINGER_SCL))
    (pad 2 smd rect (at 3.45 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 108 /ToF_sensors/TOF_LEFT_FINGER_INT))
    (pad 1 smd rect (at 1.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (pad "" smd rect (at -0.14 -0.2 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 7.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
  )
  (module "footprint:S5B-ZR-SM4A-TF(LF)(SN)" (layer F.Cu) (tedit 5BF1FC96)
    (at 120.0404 155.2194 180)
    (fp_text reference J8 (at 0.4318 4.6736 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 3.7 -4.1 180) (layer F.Fab))
    (pad "" smd rect (at 10.04 -0.2 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 6.45 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 112 /ToF_sensors/TOP_FRONT_FACING_SDA))
    (pad 3 smd rect (at 4.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /ToF_sensors/TOF_FRONT_FACING_SCL))
    (pad 2 smd rect (at 3.45 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 114 /ToF_sensors/TOF_FRONT_FACING_INT))
    (pad 1 smd rect (at 1.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (pad "" smd rect (at -0.14 -0.2 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 7.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
  )
  (module "footprint:S5B-ZR-SM4A-TF(LF)(SN)" (layer F.Cu) (tedit 5BF1FC96)
    (at 147.4216 155.2194 180)
    (fp_text reference J7 (at -1.27 3.175 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 3.7 -4.1 180) (layer F.Fab))
    (pad "" smd rect (at 10.04 -0.2 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 6.45 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 109 /ToF_sensors/TOF_RIGHT_FINGER_SDA))
    (pad 3 smd rect (at 4.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /ToF_sensors/TOP_RIGHT_FINGER_SCL))
    (pad 2 smd rect (at 3.45 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /ToF_sensors/TOF_RIGHT_FINGER_INT))
    (pad 1 smd rect (at 1.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 11 2V8))
    (pad "" smd rect (at -0.14 -0.2 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 7.95 3.5 180) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 132.092 127.3556)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C68 (at 0.0134 -0.8128) (layer B.SilkS))
    (fp_text value 0.1uF (at 17.91532 4.39928) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 5V0))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.7976 136.779)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R54 (at -2.7806 0.0635) (layer F.SilkS))
    (fp_text value 100k (at 44.8698 5.461) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /power_generation_2/EN3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 5V0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.7976 135.001)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R55 (at -2.7679 0.0254) (layer F.SilkS))
    (fp_text value 100k (at 43.4474 3.2004) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 5V0))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /power_generation_2/EN2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.7976 133.223)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R56 (at -2.7679 0.0508) (layer F.SilkS))
    (fp_text value 100k (at 42.7362 21.6408) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 5V0))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /power_generation_2/EN1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48)
    (at 101.159201 123.231801)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -6.05) (layer F.SilkS))
    (fp_text value ﻿atmega328p (at -33.392001 13.801199) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /xilinx_configuration/CD))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /xilinx_configuration/RXI))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /xilinx_configuration/TXO))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 85 /xilinx_configuration/NVRAM_SCL))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 84 /xilinx_configuration/NVRAM_SDA))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 FPGA_5V_EN))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /xilinx_configuration/INIT_B))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 69 /xilinx_configuration/OUT_EN))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 /xilinx_configuration/CLEAR_EEPROM))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 93 FPGA_BUCK_EN))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 FPGA_PGOOD))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /xilinx_configuration/SCLK))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 /xilinx_configuration/MISO))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 63 /xilinx_configuration/MOSI))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 62 /xilinx_configuration/CS_B))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /xilinx_configuration/DEBUG_PROD_B))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 /xilinx_configuration/STATUS_0))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 /xilinx_configuration/PROGRAM_B))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 /xilinx_configuration/STATUS_1))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /xilinx_configuration/DONE))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 /xilinx_configuration/MCLK))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /xilinx_configuration/M1))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /xilinx_configuration/M2))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 152.60752 136.00684 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U10 (at 2.40462 0.00254 270) (layer F.SilkS))
    (fp_text value ﻿AP7333 (at -28.39288 0.54864 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3_MICRO))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 96 /power_generation_1/5V0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer B.Cu) (tedit 58CE4E7E)
    (at 132.0976 129.9972)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U14 (at -0.7542 2.6924 -180) (layer B.SilkS))
    (fp_text value ﻿LM3880MF-1AxNOPB (at 4.8084 49.1744) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 98 /power_generation_2/EN2))
    (pad 6 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 99 /power_generation_2/EN1))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 97 /power_generation_2/EN3))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 93 FPGA_BUCK_EN))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 5V0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 132.042 125.1839)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at 49.4284 13.1191) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 104.3814 116.0145)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at -32.0168 5.9817) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5C2B9E43)
    (at 101.7398 135.1407)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.4129 0.0508) (layer F.SilkS))
    (fp_text value LED (at -33.9218 1.9939) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 101.7398 133.5405 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -2.4256 -0.0508 180) (layer F.SilkS))
    (fp_text value LED (at -52.0066 0.762 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 109.0296 123.1646)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at -0.3049 24.9174) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 109.4486 116.1668 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 2.4383 0.0381 90) (layer F.SilkS))
    (fp_text value LED (at 31.4832 -19.304 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 151.5746 131.0386 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 2.6796 -0.0508 180) (layer F.SilkS))
    (fp_text value LED (at -18.7326 -4.6482 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 109.0288 123.1646)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 1.45) (layer B.SilkS))
    (fp_text value 750R (at -42.2268 -13.97) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 /xilinx_configuration/DONE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 151.5618 131.0386 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 3.048 -0.0381 180) (layer B.SilkS))
    (fp_text value 750R (at -53.9369 3.0099 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 3V3_MICRO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.0285 125.1839)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R48 (at 0 -1.3589) (layer B.SilkS))
    (fp_text value 750R (at -20.32 43.0784) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 3V3_MICRO))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:TPS62142RGTR (layer F.Cu) (tedit 5C181DFC)
    (at 149.5806 146.304)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U8 (at 2.8321 -1.7907) (layer F.SilkS))
    (fp_text value ﻿TPS6214x (at -55.0617 17.1124) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 /power_generation_1/5V0))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 12V0))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /power_generation_1/PG))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(L1-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(L1-Pad1)"))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(L1-Pad1)"))
    (pad 17 smd circle (at -0.6477 -0.6477) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at -0.6477 0.6477) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at 0.6477 -0.6477) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at 0.6477 0.6477) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at 0 -0.6477) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at -0.6477 0) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at 0 0.6477) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at 0 0) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 smd circle (at 0.6477 0) (size 0.508 0.508) (layers F.Cu F.Paste F.Mask)
      (net 86 DGND) (solder_mask_margin 0.0254))
    (pad 17 thru_hole circle (at -0.3175 -0.3175) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 17 thru_hole circle (at 0.3302 -0.3175) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 17 thru_hole circle (at 0.3302 0.3175) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (pad 17 thru_hole circle (at -0.3175 0.3175) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 86 DGND))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 138.6974 117.221 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 2.8836 -0.0508 180) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 101 /power_generation_2/FB2))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 145.45056 118.95192 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 2.97552 -0.01016 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 100 /power_generation_2/FB1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 138.0142 123.8758 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 3.2926 -0.0635 180) (layer F.SilkS))
    (fp_text value 33pF (at -58.9882 3.9624 270) (layer F.Fab))
    (fp_text user %R (at -42.1607 -0.508 180) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 102 /power_generation_2/FB3))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:1239AS-H-1R5M=P2 (layer F.Cu) (tedit 5C267061)
    (at 141.4526 123.952 270)
    (fp_text reference L4 (at 3.4544 0.381) (layer F.SilkS))
    (fp_text value 2.2uH (at -9.144 -55.3974 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(L4-Pad1)"))
    (pad 2 smd rect (at 2.00152 0.02032 270) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
  )
  (module footprint:1239AS-H-1R5M=P2 (layer F.Cu) (tedit 5C267061)
    (at 145.4912 121.54662)
    (fp_text reference L2 (at 3.2512 0.01778 90) (layer F.SilkS))
    (fp_text value 1.5uH (at 0 -2.3368) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 2.00152 0.02032) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 1V0))
  )
  (module footprint:1239AS-H-1R5M=P2 (layer F.Cu) (tedit 5C267061)
    (at 141.5161 116.7638 90)
    (fp_text reference L3 (at 3.2258 -0.3937 180) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 -2.3368 90) (layer F.Fab))
    (pad 2 smd rect (at 2.00152 0.02032 90) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 1V8))
    (pad 1 smd rect (at 0 0 90) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(L3-Pad1)"))
  )
  (module footprint:1239AS-H-1R5M=P2 (layer F.Cu) (tedit 5C267061)
    (at 148.54428 142.75308)
    (fp_text reference L1 (at 3.42392 0.09652 180) (layer F.SilkS))
    (fp_text value 2.2uH (at 27.70632 4.94792) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 2.00152 0.02032) (size 0.8128 2.032) (layers F.Cu F.Paste F.Mask)
      (net 96 /power_generation_1/5V0))
  )
  (module footprint:1239AS-H-1R5M=P2 (layer B.Cu) (tedit 5C267061)
    (at 124.52858 144.35582)
    (fp_text reference L5 (at 3.5052 0) (layer B.SilkS))
    (fp_text value L (at 50.6349 16.6624) (layer B.Fab))
    (pad 2 smd rect (at 2.00152 -0.02032) (size 0.8128 2.032) (layers B.Cu B.Paste B.Mask)
      (net 92 /ADC/VCCADC))
    (pad 1 smd rect (at 0 0) (size 0.8128 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 1V8))
  )
  (module footprint:1239AS-H-1R5M=P2 (layer B.Cu) (tedit 5C267061)
    (at 120.1928 148.5773 270)
    (fp_text reference L6 (at 3.4036 0.0381) (layer B.SilkS))
    (fp_text value L (at 44.45762 8.19658 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 0.8128 2.032) (layers B.Cu B.Paste B.Mask)
      (net 91 /ADC/VREFN))
    (pad 2 smd rect (at 2.00152 -0.02032 270) (size 0.8128 2.032) (layers B.Cu B.Paste B.Mask)
      (net 86 DGND))
  )
  (gr_text "(FPGA PGOOD)" (at 131.9784 131.5466 90) (layer F.SilkS))
  (gr_text "(DONE)" (at 112.7506 121.8057) (layer F.SilkS))
  (gr_text "(STAT_0)" (at 108.2421 135.1661) (layer F.SilkS))
  (gr_text "(STAT_1)" (at 108.2421 133.5913) (layer F.SilkS))
  (gr_text INT_B (at 111.0742 116.1542 90) (layer F.SilkS))
  (gr_text 5V (at 153.8478 131.1148 90) (layer F.SilkS))
  (gr_line (start 154.94 106.68) (end 154.94 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 106.68) (end 154.94 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 157.48) (end 88.9 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 157.48) (end 154.94 157.48) (layer Edge.Cuts) (width 0.15))
  (zone (net 86) (net_name DGND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.281 107.061) (xy 154.559 107.061) (xy 154.559 157.099) (xy 89.281 157.099)
      )
    )
  )
)
