(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-4-gd25d622-dirty)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 0)
    (zones 0)
    (modules 6)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.7)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 151.25 103.5)
    (grid_origin 151.25 103.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01000_7fffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "DXF/"))
  )
  (net 0 "")
  (net 1 Signal_01)
  (net 2 Signal_02)
  (net 3 Signal_03)
  (net 4 Signal_04)
  (net 5 Signal_05)
  (net 6 Signal_06)
  (net 7 Signal_07)
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J2-Pad8)")
  (net 10 Signal_14)
  (net 11 Signal_13)
  (net 12 Signal_12)
  (net 13 Signal_11)
  (net 14 Signal_10)
  (net 15 Signal_09)
  (net 16 Signal_08)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.7)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad8)")
    (add_net Signal_01)
    (add_net Signal_02)
    (add_net Signal_03)
    (add_net Signal_04)
    (add_net Signal_05)
    (add_net Signal_06)
    (add_net Signal_07)
    (add_net Signal_08)
    (add_net Signal_09)
    (add_net Signal_10)
    (add_net Signal_11)
    (add_net Signal_12)
    (add_net Signal_13)
    (add_net Signal_14)
  )
  (module antenna (layer F.Cu) (tedit 5A74E519)
    (at 151.25 103.5)
    (descr "antenna StepUp generated footprint")
    (fp_text reference REF** (at 0 -2.8) (layer F.SilkS))
    (fp_text value "Value " (at 0 2) (layer F.SilkS))
    (fp_text user %R (at 0 -2.8) (layer F.Fab))
    (pad "#" smd custom (at 0 -15.1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0 15.1) (end 13.5 15.1) (width 1))
      ))
    (pad "#" smd custom (at 0 -15.1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0 15.1) (end 15.1 15.1) (width 1))
      ))
    (pad "#" thru_hole circle (at 14.75 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
    (pad "#" thru_hole circle (at 13.15 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5C8665CF)
    (at 174.5 126.5)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference H3 (at 0 -2.9) (layer F.SilkS))
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5C8665C8)
    (at 128 126.75)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference H2 (at 0 -2.9) (layer F.SilkS))
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module ASYS:522710779_FFC_FPC (layer B.Cu) (tedit 5C8665D8)
    (at 180.75 95 90)
    (fp_text reference J1 (at 0.4 -7.8 90) (layer B.SilkS))
    (fp_text value Conn_01x08 (at 0.5 4.5 90) (layer B.Fab))
    (pad 1 smd rect (at -3 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 1 Signal_01))
    (pad 2 smd rect (at -2 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 Signal_02))
    (pad 3 smd rect (at -1 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 Signal_03))
    (pad 4 smd rect (at 0 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 4 Signal_04))
    (pad 5 smd rect (at 1 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 5 Signal_05))
    (pad 6 smd rect (at 2 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 6 Signal_06))
    (pad 7 smd rect (at 3 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 7 Signal_07))
    (pad 8 smd rect (at 6.15 -0.85 90) (size 2.1 2.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 8 smd rect (at -6.15 -0.85 90) (size 2.1 2.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (model D:/Estrada/KiCad5/packages3D/Connectors_Molex.3dshapes/Molex_EasyOn_522710779_FFC_FPC.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module ASYS:522710779_FFC_FPC (layer B.Cu) (tedit 5C8665DF)
    (at 180.75 112 90)
    (fp_text reference J2 (at 0.4 -7.8 90) (layer B.SilkS))
    (fp_text value Conn_01x08 (at 0.5 4.5 90) (layer B.Fab))
    (pad 8 smd rect (at -6.15 -0.85 90) (size 2.1 2.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 8 smd rect (at 6.15 -0.85 90) (size 2.1 2.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 7 smd rect (at 3 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 10 Signal_14))
    (pad 6 smd rect (at 2 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 11 Signal_13))
    (pad 5 smd rect (at 1 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 12 Signal_12))
    (pad 4 smd rect (at 0 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 13 Signal_11))
    (pad 3 smd rect (at -1 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 14 Signal_10))
    (pad 2 smd rect (at -2 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 15 Signal_09))
    (pad 1 smd rect (at -3 1.5 90) (size 0.6 1.9) (layers B.Cu B.Paste B.Mask)
      (net 16 Signal_08))
    (model D:/Estrada/KiCad5/packages3D/Connectors_Molex.3dshapes/Molex_EasyOn_522710779_FFC_FPC.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5C8665C1)
    (at 151.25 70.75)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 -2.9) (layer F.SilkS))
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_arc (start 151.25 103.5) (end 186.23 102.5) (angle -176.725) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.25 103.5) (end 116.26 104.5) (angle -176.726) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.25 103.5) (end 152.25 113.45) (angle -168.522) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.25 103.5) (end 150.25 93.55) (angle -168.522) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.25 113.5) (end 150.25 113.45) (angle -185.725) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.25 93.5) (end 152.25 93.55) (angle -185.725) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 116.25 103.5) (end 116.26 104.5) (angle -178.281) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 186.25 103.5) (end 186.23 102.5) (angle -178.281) (layer Edge.Cuts) (width 0.1))
)
