(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 96)
    (zones 0)
    (modules 24)
    (nets 2)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber_2/"))
  )
  (net 0 "")
  (net 1 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class 2 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 151.654534 41.149939 180)
    (fp_text reference U1 (at -5.3 3.7 180) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2 180) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1 180) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 95.854534 41.149939 180)
    (fp_text reference U10 (at -5.3 3.7 180) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2 180) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1 180) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 133.054534 41.149939 180)
    (fp_text reference U3 (at -5.3 3.7 180) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2 180) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1 180) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 40.05 41.15)
    (fp_text reference U4 (at -5.3 3.7) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 58.654534 41.149939 180)
    (fp_text reference U5 (at -5.3 3.7 180) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2 180) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1 180) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 95.85 41.15)
    (fp_text reference U6 (at -5.3 3.7) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 114.4 41.35 180)
    (fp_text reference U8 (at -5.3 3.7 180) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2 180) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1 180) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 58.65 41.15)
    (fp_text reference U9 (at -5.3 3.7) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 77.25 41.15)
    (fp_text reference U11 (at -5.3 3.7) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 114.45 41.15)
    (fp_text reference U12 (at -5.3 3.7) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 102.25 37.75)
    (fp_text reference U13 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 102 44.5)
    (fp_text reference U14 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 83.75 37.75)
    (fp_text reference U16 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 120.5 37.75)
    (fp_text reference U17 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 64.75 44.5)
    (fp_text reference U18 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 138.25 37.75)
    (fp_text reference U19 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 83.75 44.5)
    (fp_text reference U20 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 46.75 37.75)
    (fp_text reference U21 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 64.75 37.75)
    (fp_text reference U22 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 120.5 44.25)
    (fp_text reference U23 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 46.75 44.25)
    (fp_text reference U24 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 77.4 41.1 180)
    (fp_text reference U2 (at -5.3 3.7 180) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2 180) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1 180) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:footprint_A (layer F.Cu) (tedit 5C793601)
    (at 132.85 41.4)
    (fp_text reference U7 (at -5.3 3.7) (layer F.SilkS))
    (fp_text value Nickel_Tab (at 4 -2.2) (layer F.Fab))
    (pad 1 smd rect (at 9.4 3.1) (size 8 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Battery_Fuse_Strip_footprint:fuse_3 (layer B.Cu) (tedit 5C7BCB6B)
    (at 138.5 44.5)
    (fp_text reference U15 (at 0.75 -4.5) (layer B.SilkS))
    (fp_text value Fuse_pad (at -1.5 10.75) (layer B.Fab))
    (fp_text user Fuse (at -3.75 0) (layer B.SilkS))
    (pad 1 smd rect (at 3.5 0) (size 5 0.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (gr_line (start 151.65 36.05) (end 40.05 36.05) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.65 46.25) (end 151.65 36.05) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.05 46.25) (end 151.65 46.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.05 36.05) (end 40.05 46.25) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40 39.25) (xy 40 42.5) (xy 151.5 42.5) (xy 151.5 39.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40 39.25) (xy 40 42.5) (xy 151.5 42.5) (xy 151.5 39.25)
      )
    )
  )
)
