(module C_FEEDTHRU_0603_NFM18 (layer F.Cu) (tedit 5CCE24C0)
  (descr "Capacitor  Feed Through 0603 NFM18PC/CC (https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/NFM18PC105R0J3-01.pdf)")
  (tags "capacitor 0603 feedthru NFM")
  (attr smd)
  (fp_text reference REF** (at -0.05 -2.05) (layer F.SilkS))
  (fp_text value C_FEEDTHRU_0603_NFM18 (at 0 2.15) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 2 smd rect (at 0.8 0) (size 0.8 0.6) (drill (offset 0.1 0)) (layers F.Cu))
  (pad 1 smd rect (at -0.8 0) (size 0.8 0.6) (drill (offset -0.1 0)) (layers F.Cu))
  (pad 3 thru_hole rect (at 0 0) (size 0.4 2) (drill 0.2) (layers F.Cu))
  (pad 3 thru_hole rect (at 0 0.8) (size 0.4 0.4) (drill 0.2) (layers F.Cu))
  (pad 3 thru_hole rect (at 0 -0.8) (size 0.4 0.4) (drill 0.2) (layers F.Cu))
  (model Capacitors_SMD.3dshapes/C_0603.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
