(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 937)
    (zones 0)
    (modules 89)
    (nets 90)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 1.27)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 2.5)
    (via_drill 1)
    (via_min_size 2.5)
    (via_min_drill 0.3)
    (uvia_size 0.6)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 1)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_7fffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(ESP32-1-PadD2)")
  (net 2 "Net-(ESP32-1-PadTX2)")
  (net 3 "Net-(ESP32-1-PadD5)")
  (net 4 "Net-(ESP32-1-PadD21)")
  (net 5 "Net-(ESP32-1-PadRX0)")
  (net 6 "Net-(ESP32-1-PadTX0)")
  (net 7 "Net-(ESP32-1-PadD22)")
  (net 8 "Net-(ESP32-1-PadD23)")
  (net 9 "Net-(ESP32-1-PadD13)")
  (net 10 "Net-(ESP32-1-PadD12)")
  (net 11 "Net-(ESP32-1-PadD14)")
  (net 12 "Net-(ESP32-1-PadD27)")
  (net 13 "Net-(ESP32-1-PadD26)")
  (net 14 "Net-(ESP32-1-PadD25)")
  (net 15 "Net-(ESP32-1-PadD33)")
  (net 16 "Net-(ESP32-1-PadD32)")
  (net 17 "Net-(ESP32-1-PadVN)")
  (net 18 "Net-(ESP32-1-PadVP)")
  (net 19 "Net-(ESP32-1-PadEN)")
  (net 20 "Net-(RL1-Pad14)")
  (net 21 "Net-(RL1-Pad24)")
  (net 22 "Net-(RL3-Pad14)")
  (net 23 "Net-(RL3-Pad24)")
  (net 24 "Net-(RL2-Pad14)")
  (net 25 "Net-(RL2-Pad24)")
  (net 26 "Net-(D6-PadA)")
  (net 27 "Net-(RL1-Pad22)")
  (net 28 "Net-(RL1-Pad12)")
  (net 29 "Net-(D8-PadA)")
  (net 30 "Net-(RL2-Pad22)")
  (net 31 "Net-(RL2-Pad21)")
  (net 32 "Net-(RL2-Pad12)")
  (net 33 "Net-(RL2-Pad11)")
  (net 34 "Net-(D7-PadA)")
  (net 35 "Net-(RL3-Pad22)")
  (net 36 "Net-(RL3-Pad21)")
  (net 37 "Net-(RL3-Pad12)")
  (net 38 "Net-(RL3-Pad11)")
  (net 39 "Net-(D4-PadA)")
  (net 40 "Net-(C2-Pad+)")
  (net 41 "Net-(R1-Pad1)")
  (net 42 "Net-(R2-Pad1)")
  (net 43 "Net-(R4-Pad1)")
  (net 44 "Net-(R3-Pad1)")
  (net 45 "Net-(D5-PadA)")
  (net 46 "Net-(C1-Pad+)")
  (net 47 "Net-(R5-Pad1)")
  (net 48 "Net-(ACS1-PadM+)")
  (net 49 "Net-(ACS2-PadM+)")
  (net 50 "Net-(ACS1-PadM-)")
  (net 51 "Net-(ACS1-PadOUT)")
  (net 52 "Net-(ACS2-PadM-)")
  (net 53 "Net-(ACS2-PadOUT)")
  (net 54 "Net-(R8-Pad1)")
  (net 55 "Net-(R9-Pad1)")
  (net 56 "Net-(ALIM1-PadIN)")
  (net 57 "Net-(D1-PadA)")
  (net 58 "Net-(D2-PadA)")
  (net 59 "Net-(D3-PadA)")
  (net 60 "Net-(R16-Pad1)")
  (net 61 "Net-(LUM_EXT1-Pad2)")
  (net 62 "Net-(LUM_EXT1-Pad1)")
  (net 63 "Net-(RL6-PadCOM-CLOSE)")
  (net 64 "Net-(F1-Pad2)")
  (net 65 "Net-(R19-Pad2)")
  (net 66 "Net-(R18-Pad2)")
  (net 67 "Net-(R17-Pad2)")
  (net 68 "Net-(R23-Pad2)")
  (net 69 "Net-(J1-Pad4)")
  (net 70 "Net-(J1-Pad5)")
  (net 71 "Net-(R24-Pad2)")
  (net 72 "Net-(R22-Pad2)")
  (net 73 "Net-(R21-Pad2)")
  (net 74 "Net-(J1-Pad6)")
  (net 75 "Net-(J1-Pad7)")
  (net 76 "Net-(ALIM1-PadOUT)")
  (net 77 "Net-(R9-Pad2)")
  (net 78 "Net-(R8-Pad2)")
  (net 79 "Net-(ACS1-PadVCC)")
  (net 80 "Net-(ACS1-PadGND)")
  (net 81 "Net-(ALIM_12V1-Pad1)")
  (net 82 "Net-(BTN3-Pad1)")
  (net 83 "Net-(BTN5-Pad1)")
  (net 84 "Net-(BTN4-Pad1)")
  (net 85 "Net-(BTN2-Pad1)")
  (net 86 "Net-(BTN1-Pad1)")
  (net 87 "Net-(BTN1-Pad3)")
  (net 88 "Net-(BTN7-Pad3)")
  (net 89 "Net-(BTN6-Pad3)")
  (net_class Default "Ceci est la Netclass par défaut."
    (clearance 0.2)
    (trace_width 1.27)
    (via_dia 2.5)
    (via_drill 1)
    (uvia_dia 0.6)
    (uvia_drill 0.4)
    (diff_pair_gap 0.63)
    (diff_pair_width 0.63)
    (add_net "Net-(ACS1-PadGND)")
    (add_net "Net-(ACS1-PadM+)")
    (add_net "Net-(ACS1-PadM-)")
    (add_net "Net-(ACS1-PadOUT)")
    (add_net "Net-(ACS1-PadVCC)")
    (add_net "Net-(ACS2-PadM+)")
    (add_net "Net-(ACS2-PadM-)")
    (add_net "Net-(ACS2-PadOUT)")
    (add_net "Net-(ALIM1-PadIN)")
    (add_net "Net-(ALIM1-PadOUT)")
    (add_net "Net-(ALIM_12V1-Pad1)")
    (add_net "Net-(BTN1-Pad1)")
    (add_net "Net-(BTN1-Pad3)")
    (add_net "Net-(BTN2-Pad1)")
    (add_net "Net-(BTN3-Pad1)")
    (add_net "Net-(BTN4-Pad1)")
    (add_net "Net-(BTN5-Pad1)")
    (add_net "Net-(BTN6-Pad3)")
    (add_net "Net-(BTN7-Pad3)")
    (add_net "Net-(C1-Pad+)")
    (add_net "Net-(C2-Pad+)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(D3-PadA)")
    (add_net "Net-(D4-PadA)")
    (add_net "Net-(D5-PadA)")
    (add_net "Net-(D6-PadA)")
    (add_net "Net-(D7-PadA)")
    (add_net "Net-(D8-PadA)")
    (add_net "Net-(ESP32-1-PadD12)")
    (add_net "Net-(ESP32-1-PadD13)")
    (add_net "Net-(ESP32-1-PadD14)")
    (add_net "Net-(ESP32-1-PadD2)")
    (add_net "Net-(ESP32-1-PadD21)")
    (add_net "Net-(ESP32-1-PadD22)")
    (add_net "Net-(ESP32-1-PadD23)")
    (add_net "Net-(ESP32-1-PadD25)")
    (add_net "Net-(ESP32-1-PadD26)")
    (add_net "Net-(ESP32-1-PadD27)")
    (add_net "Net-(ESP32-1-PadD32)")
    (add_net "Net-(ESP32-1-PadD33)")
    (add_net "Net-(ESP32-1-PadD5)")
    (add_net "Net-(ESP32-1-PadEN)")
    (add_net "Net-(ESP32-1-PadRX0)")
    (add_net "Net-(ESP32-1-PadTX0)")
    (add_net "Net-(ESP32-1-PadTX2)")
    (add_net "Net-(ESP32-1-PadVN)")
    (add_net "Net-(ESP32-1-PadVP)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(LUM_EXT1-Pad1)")
    (add_net "Net-(LUM_EXT1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(RL1-Pad12)")
    (add_net "Net-(RL1-Pad14)")
    (add_net "Net-(RL1-Pad22)")
    (add_net "Net-(RL1-Pad24)")
    (add_net "Net-(RL2-Pad11)")
    (add_net "Net-(RL2-Pad12)")
    (add_net "Net-(RL2-Pad14)")
    (add_net "Net-(RL2-Pad21)")
    (add_net "Net-(RL2-Pad22)")
    (add_net "Net-(RL2-Pad24)")
    (add_net "Net-(RL3-Pad11)")
    (add_net "Net-(RL3-Pad12)")
    (add_net "Net-(RL3-Pad14)")
    (add_net "Net-(RL3-Pad21)")
    (add_net "Net-(RL3-Pad22)")
    (add_net "Net-(RL3-Pad24)")
    (add_net "Net-(RL6-PadCOM-CLOSE)")
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BD8429D)
    (at 187.96 -65.532)
    (fp_text reference BTN1 (at -2.16001 -4.82249) (layer F.Fab) hide)
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(BTN1-Pad1)"))
    (pad 3 thru_hole circle (at -3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)"))
    (pad 2 thru_hole circle (at 3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(BTN1-Pad1)"))
    (pad 4 thru_hole circle (at 3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)"))
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BD842B7)
    (at 175.26 -65.532 180)
    (fp_text reference BTN6 (at 0 -4.318 180) (layer F.Fab) hide)
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.25 -2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 3 thru_hole circle (at -3.25 2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(BTN6-Pad3)"))
    (pad 2 thru_hole circle (at 3.25 -2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 4 thru_hole circle (at 3.25 2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(BTN6-Pad3)"))
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BD8426A)
    (at 175.26 -47.752 180)
    (fp_text reference BTN7 (at -2.16001 -4.82249 180) (layer F.Fab) hide)
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.25 -2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 3 thru_hole circle (at -3.25 2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(BTN7-Pad3)"))
    (pad 2 thru_hole circle (at 3.25 -2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 4 thru_hole circle (at 3.25 2.25 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(BTN7-Pad3)"))
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BAB7FED)
    (at 157.48 -32.512)
    (fp_text reference BTN5 (at -2.16001 -4.82249) (layer F.SilkS))
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(BTN5-Pad1)"))
    (pad 3 thru_hole circle (at -3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 2 thru_hole circle (at 3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(BTN5-Pad1)"))
    (pad 4 thru_hole circle (at 3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BD84288)
    (at 199.39 -47.752)
    (fp_text reference BTN4 (at -2.16001 -4.82249) (layer F.Fab) hide)
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(BTN4-Pad1)"))
    (pad 3 thru_hole circle (at -3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 2 thru_hole circle (at 3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(BTN4-Pad1)"))
    (pad 4 thru_hole circle (at 3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BD84280)
    (at 187.96 -47.752)
    (fp_text reference BTN3 (at -2.16001 -4.82249) (layer F.Fab) hide)
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(BTN3-Pad1)"))
    (pad 3 thru_hole circle (at -3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 2 thru_hole circle (at 3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(BTN3-Pad1)"))
    (pad 4 thru_hole circle (at 3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module JLN:SW_B3F-1000 (layer Top) (tedit 5BD842A9)
    (at 199.39 -65.532)
    (fp_text reference BTN2 (at -2.16001 -4.82249) (layer F.Fab) hide)
    (fp_text value BTN_POUSSOIR (at -1.47672 4.35595) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(BTN2-Pad1)"))
    (pad 3 thru_hole circle (at -3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)"))
    (pad 2 thru_hole circle (at 3.25 -2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(BTN2-Pad1)"))
    (pad 4 thru_hole circle (at 3.25 2.25) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)"))
  )
  (module JLN:RAD_TO247 (layer Top) (tedit 5B9E1B33)
    (at 171.8945 -132.842)
    (fp_text reference RAD2 (at 0 -2.77) (layer F.SilkS))
    (fp_text value Radiateur_TO247 (at 0 2.77) (layer F.Fab))
    (pad GND thru_hole roundrect (at 12.3 0) (size 5.08 5.08) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad GND thru_hole roundrect (at -12.3 0) (size 5.08 5.08) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module JLN:RAD_TO247 (layer Top) (tedit 5B9E1B33)
    (at 135.255 -132.842)
    (fp_text reference RAD1 (at 0 -2.77) (layer F.SilkS))
    (fp_text value Radiateur_TO247 (at 0 2.77) (layer F.Fab))
    (pad GND thru_hole roundrect (at 12.3 0) (size 5.08 5.08) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad GND thru_hole roundrect (at -12.3 0) (size 5.08 5.08) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module JLN:SIP-1 (layer Top) (tedit 5B9A11F4)
    (at 32.512 -57.2135)
    (fp_text reference TP1 (at 0 -2.77) (layer F.SilkS))
    (fp_text value +5V (at 0 2.77) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)"))
  )
  (module Resistors_THT:R_Array_SIP5 (layer Top) (tedit 57FA3974)
    (at 235.913001 -43.790999)
    (descr "5-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 6.35 -2.4) (layer F.SilkS))
    (fp_text value R_Network04 (at 6.35 2.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad7)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad6)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad5)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module JLN:2SD1287 (layer Top) (tedit 5B9D2582)
    (at 166.37 -128.4605)
    (fp_text reference T8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 2SD1287 (at 0 0) (layer F.SilkS) hide)
    (fp_text user 2SD1287 (at 2.15 -1.1) (layer F.SilkS))
    (fp_text user B (at -0.5 2) (layer F.SilkS))
    (fp_text user C (at 5 2) (layer F.SilkS))
    (fp_text user E (at 10.5 2) (layer F.SilkS))
    (pad E thru_hole oval (at 10.795 0 90) (size 5.08 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(C2-Pad+)") (solder_mask_margin 0.1524))
    (pad C thru_hole oval (at 5.45 0.025 90) (size 5.08 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(ACS2-PadM-)") (solder_mask_margin 0.1524))
    (pad B thru_hole oval (at 0 0 90) (size 5.08 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(R9-Pad1)") (solder_mask_margin 0.1524))
  )
  (module JLN:2SD1287 (layer Top) (tedit 5B9D2582)
    (at 129.921 -128.4605)
    (fp_text reference T7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 2SD1287 (at 0 0) (layer F.SilkS) hide)
    (fp_text user 2SD1287 (at 2.15 -1.1) (layer F.SilkS))
    (fp_text user B (at -0.5 2) (layer F.SilkS))
    (fp_text user C (at 5 2) (layer F.SilkS))
    (fp_text user E (at 10.5 2) (layer F.SilkS))
    (pad E thru_hole oval (at 10.795 0 90) (size 5.08 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(C1-Pad+)") (solder_mask_margin 0.1524))
    (pad C thru_hole oval (at 5.45 0.025 90) (size 5.08 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(ACS1-PadM-)") (solder_mask_margin 0.1524))
    (pad B thru_hole oval (at 0 0 90) (size 5.08 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(R8-Pad1)") (solder_mask_margin 0.1524))
  )
  (module JLN:CA6V (layer Top) (tedit 0)
    (at 196.1515 -116.713)
    (descr "<b>POTENTIOMETER</b><p>\ndistributor Schukat")
    (fp_text reference Trim4 (at -2.54 -4.191) (layer F.SilkS))
    (fp_text value 10k (at -1.5875 6.0325) (layer F.Fab))
    (pad E thru_hole oval (at 2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)") (solder_mask_margin 0.1524))
    (pad A thru_hole oval (at -2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad S thru_hole oval (at 0 -2.54) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(ESP32-1-PadVP)") (solder_mask_margin 0.1524))
  )
  (module JLN:CA6V (layer Top) (tedit 0)
    (at 186.055 -116.6495)
    (descr "<b>POTENTIOMETER</b><p>\ndistributor Schukat")
    (fp_text reference Trim3 (at -2.54 -4.191) (layer F.SilkS))
    (fp_text value 10k (at -1.8415 5.9055) (layer F.Fab))
    (pad E thru_hole oval (at 2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)") (solder_mask_margin 0.1524))
    (pad A thru_hole oval (at -2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad S thru_hole oval (at 0 -2.54) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(ESP32-1-PadVN)") (solder_mask_margin 0.1524))
  )
  (module JLN:CA6V (layer Top) (tedit 0)
    (at 196.342 -101.473)
    (descr "<b>POTENTIOMETER</b><p>\ndistributor Schukat")
    (fp_text reference Trim2 (at -2.54 -4.191) (layer F.SilkS))
    (fp_text value 10k (at -1.4605 5.334) (layer F.Fab))
    (pad E thru_hole oval (at 2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole oval (at -2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad S thru_hole oval (at 0 -2.54) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(R9-Pad2)") (solder_mask_margin 0.1524))
  )
  (module JLN:CA6V (layer Top) (tedit 0)
    (at 186.055 -101.473)
    (descr "<b>POTENTIOMETER</b><p>\ndistributor Schukat")
    (fp_text reference Trim1 (at -2.54 -4.191) (layer F.SilkS))
    (fp_text value 10k (at -1.5875 5.461) (layer F.Fab))
    (pad E thru_hole oval (at 2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole oval (at -2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad S thru_hole oval (at 0 -2.54) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "Net-(R8-Pad2)") (solder_mask_margin 0.1524))
  )
  (module JLN:ESP32_DOIT (layer Top) (tedit 5B9CD79C)
    (at 222.885 -105.537)
    (fp_text reference ESP32-1 (at -0.254 5.969) (layer F.SilkS) hide)
    (fp_text value ESP32_DOIT (at 0 0) (layer F.SilkS) hide)
    (fp_text user ESP32-DOIT (at -5.08 -22.86) (layer F.SilkS))
    (pad 3V3 thru_hole oval (at 12.7 16.51) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)") (solder_mask_margin 0.1524))
    (pad GND2 thru_hole oval (at 12.7 13.97) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad D15 thru_hole oval (at 12.7 11.43) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(BTN4-Pad1)") (solder_mask_margin 0.1524))
    (pad D2 thru_hole oval (at 12.7 8.89) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(ESP32-1-PadD2)") (solder_mask_margin 0.1524))
    (pad D4 thru_hole oval (at 12.7 6.35) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(BTN3-Pad1)") (solder_mask_margin 0.1524))
    (pad RX2 thru_hole oval (at 12.7 3.81) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(BTN5-Pad1)") (solder_mask_margin 0.1524))
    (pad TX2 thru_hole oval (at 12.7 1.27) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(ESP32-1-PadTX2)") (solder_mask_margin 0.1524))
    (pad D5 thru_hole oval (at 12.7 -1.27) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(ESP32-1-PadD5)") (solder_mask_margin 0.1524))
    (pad D18 thru_hole oval (at 12.7 -3.81) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(BTN7-Pad3)") (solder_mask_margin 0.1524))
    (pad D19 thru_hole oval (at 12.7 -6.35) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(BTN6-Pad3)") (solder_mask_margin 0.1524))
    (pad D21 thru_hole oval (at 12.7 -8.89) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(ESP32-1-PadD21)") (solder_mask_margin 0.1524))
    (pad RX0 thru_hole oval (at 12.7 -11.43) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(ESP32-1-PadRX0)") (solder_mask_margin 0.1524))
    (pad TX0 thru_hole oval (at 12.7 -13.97) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(ESP32-1-PadTX0)") (solder_mask_margin 0.1524))
    (pad D22 thru_hole oval (at 12.7 -16.51) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(ESP32-1-PadD22)") (solder_mask_margin 0.1524))
    (pad D23 thru_hole oval (at 12.7 -19.05) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(ESP32-1-PadD23)") (solder_mask_margin 0.1524))
    (pad VIN thru_hole oval (at -12.7 16.51) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)") (solder_mask_margin 0.1524))
    (pad GND1 thru_hole oval (at -12.7 13.97) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad D13 thru_hole oval (at -12.7 11.43) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(ESP32-1-PadD13)") (solder_mask_margin 0.1524))
    (pad D12 thru_hole oval (at -12.7 8.89) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(ESP32-1-PadD12)") (solder_mask_margin 0.1524))
    (pad D14 thru_hole oval (at -12.7 6.35) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(ESP32-1-PadD14)") (solder_mask_margin 0.1524))
    (pad D27 thru_hole oval (at -12.7 3.81) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(ESP32-1-PadD27)") (solder_mask_margin 0.1524))
    (pad D26 thru_hole oval (at -12.7 1.27) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(ESP32-1-PadD26)") (solder_mask_margin 0.1524))
    (pad D25 thru_hole oval (at -12.7 -1.27) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(ESP32-1-PadD25)") (solder_mask_margin 0.1524))
    (pad D33 thru_hole oval (at -12.7 -3.81) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(ESP32-1-PadD33)") (solder_mask_margin 0.1524))
    (pad D32 thru_hole oval (at -12.7 -6.35) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(ESP32-1-PadD32)") (solder_mask_margin 0.1524))
    (pad D35 thru_hole oval (at -12.7 -8.89) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(BTN1-Pad1)") (solder_mask_margin 0.1524))
    (pad D34 thru_hole oval (at -12.7 -11.43) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(BTN2-Pad1)") (solder_mask_margin 0.1524))
    (pad VN thru_hole oval (at -12.7 -13.97) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(ESP32-1-PadVN)") (solder_mask_margin 0.1524))
    (pad VP thru_hole oval (at -12.7 -16.51) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(ESP32-1-PadVP)") (solder_mask_margin 0.1524))
    (pad EN thru_hole oval (at -12.7 -19.05) (size 3.556 1.778) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(ESP32-1-PadEN)") (solder_mask_margin 0.1524))
  )
  (module JLN:DIP-16_W7.62mm_Socket (layer Top) (tedit 59C78D6B)
    (at 224.7265 -43.8785 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 3.81 -2.33 270) (layer F.SilkS))
    (fp_text value ILQ621 (at 3.81 20.11 270) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R21-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(R22-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(R23-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(R24-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JLN:Fusible_5x20mm (layer Top) (tedit 5B9BDF8F)
    (at 45.7835 -103.102 270)
    (descr "Fusible, 5x20, Semi clos, horizontal, Surface 10x25mm,")
    (fp_text reference F1 (at 11.9795 1.27 270) (layer F.SilkS))
    (fp_text value 5A (at 11.916 -1.397 270) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 22 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(F1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(ALIM1-PadIN)"))
  )
  (module JLN:Fusible_5x20mm (layer Top) (tedit 5B9BDF8F)
    (at 58.7375 -103.102 270)
    (descr "Fusible, 5x20, Semi clos, horizontal, Surface 10x25mm,")
    (fp_text reference F2 (at 11.7255 0.889 270) (layer F.SilkS))
    (fp_text value 10A (at 11.3445 -1.3335 270) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 22 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(ALIM_12V1-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(ACS1-PadM+)"))
  )
  (module JLN:Fusible_5x20mm (layer Top) (tedit 5B9BDF8F)
    (at 71.1835 -103.102 270)
    (descr "Fusible, 5x20, Semi clos, horizontal, Surface 10x25mm,")
    (fp_text reference F3 (at 11.789 1.27 270) (layer F.SilkS))
    (fp_text value 10A (at 11.789 -1.524 270) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 22 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(ALIM_12V1-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(ACS2-PadM+)"))
  )
  (module JLN:Fusible_5x20mm (layer Top) (tedit 5B9BDF8F)
    (at 21.0185 -103.102 270)
    (descr "Fusible, 5x20, Semi clos, horizontal, Surface 10x25mm,")
    (fp_text reference F4 (at 11.7255 1.27 270) (layer F.SilkS))
    (fp_text value 5A (at 11.916 -1.4605 270) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 22 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(ALIM_12V1-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(ALIM1-PadIN)"))
  )
  (module JLN:Fusible_5x20mm (layer Top) (tedit 5B9BDF8F)
    (at 33.274 -81.026 90)
    (descr "Fusible, 5x20, Semi clos, horizontal, Surface 10x25mm,")
    (fp_text reference F5 (at 10.3505 -1.4605 90) (layer F.SilkS))
    (fp_text value 3A (at 10.2235 1.2065 90) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 22 0) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(ALIM1-PadOUT)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 4 4) (drill 1.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(ACS1-PadVCC)"))
  )
  (module JLN:PINHEAD1-7 (layer Top) (tedit 5B9CCC2E)
    (at 247.7135 -26.8605 180)
    (fp_text reference J1 (at 6.35 -3.75 180) (layer F.SilkS))
    (fp_text value Conn_01x07 (at 6.35 3.81 180) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad7)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad6)"))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 226.1235 -60.452 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R21 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R21-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(ESP32-1-PadD13)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 222.8215 -60.452 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R22 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(R22-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(ESP32-1-PadD14)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 215.4555 -60.452 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R24 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(R24-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(ESP32-1-PadD26)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 219.2655 -60.452 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R23 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(R23-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(ESP32-1-PadD2)") (solder_mask_margin 0.1524))
  )
  (module JLN:SIP-1 (layer Top) (tedit 5B9A11F4)
    (at 13.0175 -57.3405)
    (fp_text reference TP2 (at 0 -2.77) (layer F.SilkS))
    (fp_text value 12V (at 0 2.77) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(ALIM_12V1-Pad1)"))
  )
  (module JLN:SIP-1 (layer Top) (tedit 5B9A11F4)
    (at 57.15 -57.4675)
    (fp_text reference TP4 (at 0 -2.77) (layer F.SilkS))
    (fp_text value GND (at 0 2.77) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module JLN:SIP-1 (layer Top) (tedit 5B9A11F4)
    (at 172.72 -33.147)
    (fp_text reference TP3 (at 0 -2.77) (layer F.SilkS))
    (fp_text value 3,3V (at 0 2.77) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)"))
  )
  (module JLN:OLED_SSD1306 (layer Top) (tedit 5B9A0543)
    (at 141.9225 -43.942)
    (tags "OLED SSD1306")
    (fp_text reference U1 (at 12.0015 -17.7165) (layer F.SilkS))
    (fp_text value OLED_SSD1306 (at 13.1445 -1.397) (layer F.Fab))
    (pad 1 thru_hole oval (at 11.43 -25.4) (size 1.524 2.54) (drill 0.762) (layers *.Cu *.Mask)
      (net 87 "Net-(BTN1-Pad3)"))
    (pad 2 thru_hole oval (at 13.97 -25.4) (size 1.524 2.54) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(ESP32-1-PadD22)"))
    (pad 3 thru_hole oval (at 16.51 -25.4) (size 1.524 2.54) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(ESP32-1-PadD21)"))
    (pad 0 thru_hole oval (at 8.89 -25.4) (size 1.524 2.54) (drill 0.762) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)"))
  )
  (module Portail:ALIM_12V_5V_5A_H (layer Top) (tedit 0)
    (at 20.2565 -145.923 270)
    (fp_text reference ALIM1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value ALIM_12V_5V_5AHORIZONTAL (at 0 0 270) (layer F.SilkS) hide)
    (pad IN thru_hole oval (at 9.6774 -4.8133) (size 5.08 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad OUT thru_hole oval (at 22.5806 -4.8133) (size 5.08 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(ALIM1-PadOUT)") (solder_mask_margin 0.1524))
    (pad GND thru_hole oval (at 16.129 -4.8133) (size 5.08 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 166.37 -109.347 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R9 (at 1.27 1.27 270) (layer F.SilkS))
    (fp_text value 1k (at 1.27 -0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(R9-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(R9-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 134.62 -109.347 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R8 (at 1.905 1.27 270) (layer F.SilkS))
    (fp_text value 1k (at 1.27 -0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(R8-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(R8-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 107.315 -138.557 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R14 (at 1.905 1.27 180) (layer F.SilkS))
    (fp_text value 2k (at 1.905 -0.635 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(ACS2-PadOUT)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(D2-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 107.315 -133.477)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R13 (at -1.905 -1.524) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(D1-PadA)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 107.315 -128.397 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R12 (at 1.905 1.27 180) (layer F.SilkS))
    (fp_text value 2k (at 1.905 -0.635 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(ACS1-PadOUT)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(D1-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 107.315 -143.637)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R15 (at -1.905 -1.524) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(D2-PadA)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:ACS712-BORNIER (layer Top) (tedit 0)
    (at 68.58 -115.062)
    (fp_text reference ACS1 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value ACS712-G (at 6.985 1.905) (layer F.SilkS) hide)
    (fp_text user >Value (at 1.27 -13.97) (layer F.Fab))
    (fp_text user >Name (at 1.27 -17.78) (layer F.SilkS))
    (fp_text user VCC (at 9.525 -22.86 90) (layer F.Fab))
    (fp_text user OUT (at 6.985 -22.86 90) (layer F.Fab))
    (fp_text user GND (at 4.445 -22.86 90) (layer F.Fab))
    (fp_text user - (at 8.255 0) (layer F.Fab))
    (fp_text user + (at 2.54 0) (layer F.Fab))
    (fp_text user Mesure (at 0.635 -6.35) (layer F.Fab))
    (pad M- thru_hole rect (at 8.89 -3.81) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(ACS1-PadM-)") (solder_mask_margin 0.1524))
    (pad M+ thru_hole rect (at 3.81 -3.81) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(ACS1-PadM+)") (solder_mask_margin 0.1524))
    (pad VCC thru_hole rect (at 8.89 -27.94) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)") (solder_mask_margin 0.1524))
    (pad OUT thru_hole rect (at 6.35 -27.94) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(ACS1-PadOUT)") (solder_mask_margin 0.1524))
    (pad GND thru_hole rect (at 3.81 -27.94) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:ACS712-BORNIER (layer Top) (tedit 0)
    (at 84.455 -115.062)
    (fp_text reference ACS2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value ACS712-D (at 6.35 1.905) (layer F.SilkS) hide)
    (fp_text user >Value (at 1.27 -13.97) (layer F.Fab))
    (fp_text user >Name (at 1.27 -17.78) (layer F.SilkS))
    (fp_text user VCC (at 9.525 -22.86 90) (layer F.Fab))
    (fp_text user OUT (at 6.985 -22.86 90) (layer F.Fab))
    (fp_text user GND (at 4.445 -22.86 90) (layer F.Fab))
    (fp_text user - (at 8.255 0) (layer F.Fab))
    (fp_text user + (at 2.54 0) (layer F.Fab))
    (fp_text user Mesure (at 0.635 -6.35) (layer F.Fab))
    (pad M- thru_hole rect (at 8.89 -3.81) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(ACS2-PadM-)") (solder_mask_margin 0.1524))
    (pad M+ thru_hole rect (at 3.81 -3.81) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(ACS2-PadM+)") (solder_mask_margin 0.1524))
    (pad VCC thru_hole rect (at 8.89 -27.94) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)") (solder_mask_margin 0.1524))
    (pad OUT thru_hole rect (at 6.35 -27.94) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(ACS2-PadOUT)") (solder_mask_margin 0.1524))
    (pad GND thru_hole rect (at 3.81 -27.94) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 40.005 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference ALIM_12V1 (at -5.715 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.715 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 81 "Net-(ALIM_12V1-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 55.245 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference ALIM_5V1 (at -5.08 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.08 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 24.765 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference BAT12V1 (at -4.445 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.08 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 81 "Net-(ALIM_12V1-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:E3,5-8 (layer Top) (tedit 0)
    (at 140.97 -109.347)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 3.5 mm, diameter 8 mm")
    (fp_text reference C1 (at 3.302 -2.794) (layer F.SilkS))
    (fp_text value 250M (at -2.286 3.048) (layer F.SilkS))
    (pad + thru_hole circle (at -1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "Net-(C1-Pad+)") (solder_mask_margin 0.1524))
    (pad - thru_hole circle (at 1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:E3,5-8 (layer Top) (tedit 0)
    (at 172.72 -109.347)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 3.5 mm, diameter 8 mm")
    (fp_text reference C2 (at 3.302 -2.794) (layer F.SilkS))
    (fp_text value 250M (at -2.286 3.048) (layer F.SilkS))
    (pad + thru_hole circle (at -1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 "Net-(C2-Pad+)") (solder_mask_margin 0.1524))
    (pad - thru_hole circle (at 1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:E3,5-8 (layer Top) (tedit 0)
    (at 217.8811 -141.097)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 3.5 mm, diameter 8 mm")
    (fp_text reference C3 (at 3.302 -2.794) (layer F.SilkS))
    (fp_text value 100M (at -2.286 3.048) (layer F.SilkS))
    (pad + thru_hole circle (at -1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 86 "Net-(BTN1-Pad1)") (solder_mask_margin 0.1524))
    (pad - thru_hole circle (at 1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:E3,5-8 (layer Top) (tedit 0)
    (at 228.0411 -141.097)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 3.5 mm, diameter 8 mm")
    (fp_text reference C4 (at 3.302 -2.794) (layer F.SilkS))
    (fp_text value 100M (at -2.286 3.048) (layer F.SilkS))
    (pad + thru_hole circle (at -1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 85 "Net-(BTN2-Pad1)") (solder_mask_margin 0.1524))
    (pad - thru_hole circle (at 1.778 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 140.97 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference CDE_LUM_EXT1 (at -8.89 -6.35) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.715 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 83 "Net-(BTN5-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 191.135 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference CDE_OUV_PORTAIL1 (at -12.065 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.715 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 84 "Net-(BTN4-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 175.895 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference CDE_OUV_VENTAIL1 (at -11.43 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.715 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 82 "Net-(BTN3-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 0)
    (at 202.565 -137.922)
    (fp_text reference D1 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 86 "Net-(BTN1-Pad1)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 57 "Net-(D1-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 0)
    (at 202.565 -143.637)
    (fp_text reference D2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 85 "Net-(BTN2-Pad1)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 58 "Net-(D2-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 0)
    (at 127.635 -52.197)
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 59 "Net-(D3-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 5BD84314)
    (at 109.22 -100.457)
    (fp_text reference D4 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 39 "Net-(D4-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 5BD8433C)
    (at 92.075 -100.457)
    (fp_text reference D5 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.Fab) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 45 "Net-(D5-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 0)
    (at 74.93 -52.197)
    (fp_text reference D6 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 "Net-(D6-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 0)
    (at 92.075 -52.197)
    (fp_text reference D7 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 34 "Net-(D7-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:DIODE_PETITE (layer Top) (tedit 0)
    (at 109.22 -52.197)
    (fp_text reference D8 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.905) (layer F.SilkS) hide)
    (pad C thru_hole circle (at 3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad A thru_hole circle (at -3.175 0) (size 1.778 1.778) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 "Net-(D8-PadA)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 156.21 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference INFO_LUM_EXT1 (at -8.89 -6.35) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.715 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 3 "Net-(ESP32-1-PadD5)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 125.73 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference LUM_EXT1 (at -6.35 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -5.08 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 61 "Net-(LUM_EXT1-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 62 "Net-(LUM_EXT1-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 122.555 -74.422 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R1 (at -3.048 -1.524 90) (layer F.SilkS))
    (fp_text value 1k (at -2.2606 0.635 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(ESP32-1-PadD25)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R1-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 139.7 -74.422 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R16 (at -3.048 -1.524 90) (layer F.SilkS))
    (fp_text value 1k (at -2.2606 0.635 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(ESP32-1-PadTX2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R16-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 225.9965 -21.717 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R17 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(R17-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad4)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 215.8365 -21.717 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R18 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(R18-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad5)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 205.74 -21.717 270)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R19 (at -3.048 -1.524 270) (layer F.SilkS))
    (fp_text value 470 (at -2.2606 0.635 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(R19-Pad2)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad6)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 133.985 -74.422 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R2 (at -3.048 -1.524 90) (layer F.SilkS))
    (fp_text value 1k (at -2.2606 0.635 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(ESP32-1-PadD12)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R2-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 128.27 -74.422 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R3 (at -3.048 -1.524 90) (layer F.SilkS))
    (fp_text value 1k (at -2.2606 0.635 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(ESP32-1-PadD27)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(R3-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 107.315 -117.602)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R4 (at -1.905 -1.524) (layer F.SilkS))
    (fp_text value 1k (at -1.905 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(ESP32-1-PadD26)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(R4-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:0207_10 (layer Top) (tedit 0)
    (at 107.315 -122.682)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R5 (at -1.905 -1.524) (layer F.SilkS))
    (fp_text value 1k (at -1.905 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(ESP32-1-PadD26)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(R5-Pad1)") (solder_mask_margin 0.1524))
  )
  (module Portail:95.15.2 (layer Top) (tedit 0)
    (at 74.93 -33.782 180)
    (fp_text reference RL1 (at 1.905 5.08 180) (layer F.SilkS))
    (fp_text value R_VERROU (at 0 3.81 180) (layer F.SilkS))
    (fp_text user 24 (at 4 -10 180) (layer F.SilkS))
    (fp_text user 21 (at 4.25 -5 180) (layer F.SilkS))
    (fp_text user 22 (at 4.25 0 180) (layer F.SilkS))
    (fp_text user 14 (at -6 -10 180) (layer F.SilkS))
    (fp_text user 11 (at -6 -5 180) (layer F.SilkS))
    (fp_text user 12 (at -6 0 180) (layer F.SilkS))
    (fp_text user A2 (at 4 11.25 180) (layer F.SilkS))
    (fp_text user A1 (at -6 11.25 180) (layer F.SilkS))
    (pad A2 thru_hole oval (at 3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 26 "Net-(D6-PadA)") (solder_mask_margin 0.1524))
    (pad A1 thru_hole oval (at -3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad 22 thru_hole oval (at 3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 27 "Net-(RL1-Pad22)") (solder_mask_margin 0.1524))
    (pad 24 thru_hole oval (at 3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 21 "Net-(RL1-Pad24)") (solder_mask_margin 0.1524))
    (pad 21 thru_hole oval (at 3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 64 "Net-(F1-Pad2)") (solder_mask_margin 0.1524))
    (pad 12 thru_hole oval (at -3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 28 "Net-(RL1-Pad12)") (solder_mask_margin 0.1524))
    (pad 11 thru_hole oval (at -3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 14 thru_hole oval (at -3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 "Net-(RL1-Pad14)") (solder_mask_margin 0.1524))
  )
  (module Portail:95.15.2 (layer Top) (tedit 0)
    (at 109.16 -33.782 180)
    (fp_text reference RL3 (at 1.21 5.08 180) (layer F.SilkS))
    (fp_text value R_DROIT (at -0.06 3.81 180) (layer F.SilkS))
    (fp_text user 24 (at 4 -10 180) (layer F.SilkS))
    (fp_text user 21 (at 4.25 -5 180) (layer F.SilkS))
    (fp_text user 22 (at 4.25 0 180) (layer F.SilkS))
    (fp_text user 14 (at -6 -10 180) (layer F.SilkS))
    (fp_text user 11 (at -6 -5 180) (layer F.SilkS))
    (fp_text user 12 (at -6 0 180) (layer F.SilkS))
    (fp_text user A2 (at 4 11.25 180) (layer F.SilkS))
    (fp_text user A1 (at -6 11.25 180) (layer F.SilkS))
    (pad A2 thru_hole oval (at 3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 29 "Net-(D8-PadA)") (solder_mask_margin 0.1524))
    (pad A1 thru_hole oval (at -3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad 22 thru_hole oval (at 3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(RL3-Pad22)") (solder_mask_margin 0.1524))
    (pad 24 thru_hole oval (at 3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 23 "Net-(RL3-Pad24)") (solder_mask_margin 0.1524))
    (pad 21 thru_hole oval (at 3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 36 "Net-(RL3-Pad21)") (solder_mask_margin 0.1524))
    (pad 12 thru_hole oval (at -3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 37 "Net-(RL3-Pad12)") (solder_mask_margin 0.1524))
    (pad 11 thru_hole oval (at -3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 38 "Net-(RL3-Pad11)") (solder_mask_margin 0.1524))
    (pad 14 thru_hole oval (at -3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 22 "Net-(RL3-Pad14)") (solder_mask_margin 0.1524))
  )
  (module Portail:95.15.2 (layer Top) (tedit 0)
    (at 92.075 -33.782 180)
    (fp_text reference RL2 (at 1.27 5.08 180) (layer F.SilkS))
    (fp_text value R_GAUCHE (at -0.635 3.81 180) (layer F.SilkS))
    (fp_text user 24 (at 4 -10 180) (layer F.SilkS))
    (fp_text user 21 (at 4.25 -5 180) (layer F.SilkS))
    (fp_text user 22 (at 4.25 0 180) (layer F.SilkS))
    (fp_text user 14 (at -6 -10 180) (layer F.SilkS))
    (fp_text user 11 (at -6 -5 180) (layer F.SilkS))
    (fp_text user 12 (at -6 0 180) (layer F.SilkS))
    (fp_text user A2 (at 4 11.25 180) (layer F.SilkS))
    (fp_text user A1 (at -6 11.25 180) (layer F.SilkS))
    (pad A2 thru_hole oval (at 3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 34 "Net-(D7-PadA)") (solder_mask_margin 0.1524))
    (pad A1 thru_hole oval (at -3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad 22 thru_hole oval (at 3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 30 "Net-(RL2-Pad22)") (solder_mask_margin 0.1524))
    (pad 24 thru_hole oval (at 3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 25 "Net-(RL2-Pad24)") (solder_mask_margin 0.1524))
    (pad 21 thru_hole oval (at 3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 31 "Net-(RL2-Pad21)") (solder_mask_margin 0.1524))
    (pad 12 thru_hole oval (at -3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 32 "Net-(RL2-Pad12)") (solder_mask_margin 0.1524))
    (pad 11 thru_hole oval (at -3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(RL2-Pad11)") (solder_mask_margin 0.1524))
    (pad 14 thru_hole oval (at -3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "Net-(RL2-Pad14)") (solder_mask_margin 0.1524))
  )
  (module Portail:95.15.2 (layer Top) (tedit 5BD843DE)
    (at 109.16 -82.042 180)
    (fp_text reference RL5 (at 8.576 16.256 180) (layer F.SilkS))
    (fp_text value INV_D (at -0.695 4.445 180) (layer F.SilkS))
    (fp_text user 24 (at 4 -10 180) (layer F.Fab) hide)
    (fp_text user 21 (at 4.25 -5 180) (layer F.Fab) hide)
    (fp_text user 22 (at 4.25 0 180) (layer F.Fab) hide)
    (fp_text user 14 (at -6 -10 180) (layer F.Fab) hide)
    (fp_text user 11 (at -6 -5 180) (layer F.Fab) hide)
    (fp_text user 12 (at -6 0 180) (layer F.Fab) hide)
    (fp_text user A2 (at 4 11.25 180) (layer F.SilkS))
    (fp_text user A1 (at -6 11.25 180) (layer F.Fab) hide)
    (pad A2 thru_hole oval (at 3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 39 "Net-(D4-PadA)") (solder_mask_margin 0.1524))
    (pad A1 thru_hole oval (at -3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad 22 thru_hole oval (at 3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 38 "Net-(RL3-Pad11)") (solder_mask_margin 0.1524))
    (pad 24 thru_hole oval (at 3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 36 "Net-(RL3-Pad21)") (solder_mask_margin 0.1524))
    (pad 21 thru_hole oval (at 3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 40 "Net-(C2-Pad+)") (solder_mask_margin 0.1524))
    (pad 12 thru_hole oval (at -3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 36 "Net-(RL3-Pad21)") (solder_mask_margin 0.1524))
    (pad 11 thru_hole oval (at -3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 14 thru_hole oval (at -3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 38 "Net-(RL3-Pad11)") (solder_mask_margin 0.1524))
  )
  (module Portail:95.15.2 (layer Top) (tedit 5BD843B1)
    (at 92.075 -82.042 180)
    (fp_text reference RL4 (at 8.509 16.256 180) (layer F.SilkS))
    (fp_text value INV_G (at -0.635 4.445 180) (layer F.Fab) hide)
    (fp_text user 24 (at 4 -10 180) (layer F.Fab) hide)
    (fp_text user 21 (at 4.25 -5 180) (layer F.Fab) hide)
    (fp_text user 22 (at 4.25 0 180) (layer F.Fab) hide)
    (fp_text user 14 (at -6 -10 180) (layer F.Fab) hide)
    (fp_text user 11 (at -6 -5 180) (layer F.Fab) hide)
    (fp_text user 12 (at -6 0 180) (layer F.Fab) hide)
    (fp_text user A2 (at 4 11.25 180) (layer F.SilkS))
    (fp_text user A1 (at -6 11.25 180) (layer F.Fab) hide)
    (pad A2 thru_hole oval (at 3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 45 "Net-(D5-PadA)") (solder_mask_margin 0.1524))
    (pad A1 thru_hole oval (at -3.75 12.5 180) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 56 "Net-(ALIM1-PadIN)") (solder_mask_margin 0.1524))
    (pad 22 thru_hole oval (at 3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(RL2-Pad11)") (solder_mask_margin 0.1524))
    (pad 24 thru_hole oval (at 3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 31 "Net-(RL2-Pad21)") (solder_mask_margin 0.1524))
    (pad 21 thru_hole oval (at 3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 46 "Net-(C1-Pad+)") (solder_mask_margin 0.1524))
    (pad 12 thru_hole oval (at -3.75 -2.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 31 "Net-(RL2-Pad21)") (solder_mask_margin 0.1524))
    (pad 11 thru_hole oval (at -3.75 -7.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad 14 thru_hole oval (at -3.75 -12.5) (size 4.5 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(RL2-Pad11)") (solder_mask_margin 0.1524))
  )
  (module Portail:TO18 (layer Top) (tedit 0)
    (at 74.93 -57.912 90)
    (descr "<b>TO 18</b>")
    (fp_text reference T1 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2N2222A (at -2.54 5.08 90) (layer F.Fab))
    (fp_text user 3 (at 0 -0.635 90) (layer F.Fab))
    (fp_text user 2 (at 0.635 1.27 90) (layer F.Fab))
    (fp_text user 1 (at -1.905 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "Net-(D6-PadA)") (solder_mask_margin 0.1524))
    (pad 2 thru_hole circle (at 1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 "Net-(R1-Pad1)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:TO18 (layer Top) (tedit 0)
    (at 109.22 -57.912 90)
    (descr "<b>TO 18</b>")
    (fp_text reference T3 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2N2222A (at -3.175 5.08 90) (layer F.Fab))
    (fp_text user 3 (at 0 -0.635 90) (layer F.Fab))
    (fp_text user 2 (at 0.635 1.27 90) (layer F.Fab))
    (fp_text user 1 (at -1.905 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(D8-PadA)") (solder_mask_margin 0.1524))
    (pad 2 thru_hole circle (at 1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 42 "Net-(R2-Pad1)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:TO18 (layer Top) (tedit 5BD842FC)
    (at 109.22 -106.807 90)
    (descr "<b>TO 18</b>")
    (fp_text reference T5 (at -1.143 5.08 90) (layer F.SilkS))
    (fp_text value 2N2222A (at -2.54 5.08 90) (layer F.Fab) hide)
    (fp_text user 3 (at 0 -0.635 90) (layer F.Fab))
    (fp_text user 2 (at 0.635 1.27 90) (layer F.Fab))
    (fp_text user 1 (at -1.905 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(D4-PadA)") (solder_mask_margin 0.1524))
    (pad 2 thru_hole circle (at 1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 43 "Net-(R4-Pad1)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:TO18 (layer Top) (tedit 0)
    (at 92.075 -57.912 90)
    (descr "<b>TO 18</b>")
    (fp_text reference T2 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2N2222A (at -2.54 5.08 90) (layer F.Fab))
    (fp_text user 3 (at 0 -0.635 90) (layer F.Fab))
    (fp_text user 2 (at 0.635 1.27 90) (layer F.Fab))
    (fp_text user 1 (at -1.905 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(D7-PadA)") (solder_mask_margin 0.1524))
    (pad 2 thru_hole circle (at 1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 "Net-(R3-Pad1)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:TO18 (layer Top) (tedit 5BD84329)
    (at 92.075 -106.807 90)
    (descr "<b>TO 18</b>")
    (fp_text reference T4 (at -0.889 4.953 90) (layer F.SilkS))
    (fp_text value 2N2222A (at -2.54 5.08 90) (layer F.Fab) hide)
    (fp_text user 3 (at 0 -0.635 90) (layer F.Fab))
    (fp_text user 2 (at 0.635 1.27 90) (layer F.Fab))
    (fp_text user 1 (at -1.905 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "Net-(D5-PadA)") (solder_mask_margin 0.1524))
    (pad 2 thru_hole circle (at 1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 47 "Net-(R5-Pad1)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:TO18 (layer Top) (tedit 0)
    (at 127.635 -57.912 90)
    (descr "<b>TO 18</b>")
    (fp_text reference T6 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2N2222A (at -3.175 5.08 90) (layer F.Fab))
    (fp_text user 3 (at 0 -0.635 90) (layer F.Fab))
    (fp_text user 2 (at 0.635 1.27 90) (layer F.Fab))
    (fp_text user 1 (at -1.905 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 59 "Net-(D3-PadA)") (solder_mask_margin 0.1524))
    (pad 2 thru_hole circle (at 1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 60 "Net-(R16-Pad1)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole circle (at -1.27 1.27 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
  )
  (module Portail:RELAY (layer Top) (tedit 0)
    (at 127.635 -45.212 270)
    (fp_text reference RL6 (at 5.715 -2.54) (layer F.SilkS))
    (fp_text value R_LUM_EXT (at 7.62 0) (layer F.SilkS))
    (fp_text user "" (at 2.54 2.54 270) (layer F.Fab))
    (fp_text user "" (at 2.54 -1.27 270) (layer F.SilkS))
    (pad COM thru_hole circle (at -2 0 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(LUM_EXT1-Pad1)") (solder_mask_margin 0.1524))
    (pad COM-CLOSE thru_hole circle (at 12.2 6 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(RL6-PadCOM-CLOSE)") (solder_mask_margin 0.1524))
    (pad COM_CPEN thru_hole circle (at 12.2 -6 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(LUM_EXT1-Pad2)") (solder_mask_margin 0.1524))
    (pad P$2 thru_hole circle (at 0 6 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(D3-PadA)") (solder_mask_margin 0.1524))
    (pad P$1 thru_hole circle (at 0 -6 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(ACS1-PadVCC)") (solder_mask_margin 0.1524))
  )
  (module Portail:LED_FILS (layer Top) (tedit 5BD83F8D)
    (at 204.47 -9.017)
    (descr "<b>LED Fils</b><br>\nPour connecter une LED avec fils.")
    (fp_text reference U$2 (at 3.175 -4.445) (layer F.SilkS) hide)
    (fp_text value PORTAIL (at 3.81 3.937) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 6.35 -1.27) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad P$1 thru_hole circle (at 1.27 -1.27) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(R19-Pad2)") (solder_mask_margin 0.1524))
  )
  (module Portail:LED_FILS (layer Top) (tedit 5BD83F9E)
    (at 214.63 -9.017)
    (descr "<b>LED Fils</b><br>\nPour connecter une LED avec fils.")
    (fp_text reference U$3 (at 3.81 -4.445) (layer F.SilkS) hide)
    (fp_text value GAUCHE (at 3.81 3.937) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 6.35 -1.27) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad P$1 thru_hole circle (at 1.27 -1.27) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(R18-Pad2)") (solder_mask_margin 0.1524))
  )
  (module Portail:LED_FILS (layer Top) (tedit 5BD83FAF)
    (at 224.79 -9.017)
    (descr "<b>LED Fils</b><br>\nPour connecter une LED avec fils.")
    (fp_text reference U$4 (at 3.175 -4.445) (layer F.SilkS) hide)
    (fp_text value DROIT (at 3.556 3.937) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 6.35 -1.27) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(ACS1-PadGND)") (solder_mask_margin 0.1524))
    (pad P$1 thru_hole circle (at 1.27 -1.27) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(R17-Pad2)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 108.585 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference VENTAILDROIT1 (at -8.89 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -3.81 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 22 "Net-(RL3-Pad14)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 23 "Net-(RL3-Pad24)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 91.44 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference VENTAILGAUCHE1 (at -10.16 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -3.81 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 24 "Net-(RL2-Pad14)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 25 "Net-(RL2-Pad24)") (solder_mask_margin 0.1524))
  )
  (module Portail:GMSTBV2 (layer Top) (tedit 0)
    (at 74.93 -9.652)
    (descr <b>PHOENIX</b>)
    (fp_text reference VERROU1 (at -5.08 -5.715) (layer F.SilkS) hide)
    (fp_text value GMSTBV2 (at -3.81 6.35) (layer F.Fab) hide)
    (fp_text user 2 (at 0.508 0.635) (layer F.SilkS))
    (fp_text user 1 (at -6.858 0.635) (layer F.SilkS))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 20 "Net-(RL1-Pad14)") (solder_mask_margin 0.1524))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 4.191 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (net 21 "Net-(RL1-Pad24)") (solder_mask_margin 0.1524))
  )
  (gr_text + (at 215.9 -146.558) (layer F.SilkS))
  (gr_text - (at 219.456 -146.558) (layer F.SilkS))
  (gr_text - (at 230.124 -146.304) (layer F.SilkS))
  (gr_text + (at 226.314 -146.304) (layer F.SilkS))
  (gr_text 10A (at 71.12 -70.612 90) (layer F.SilkS))
  (gr_text 10A (at 58.928 -70.358 90) (layer F.SilkS))
  (gr_text 5A (at 45.72 -72.136 90) (layer F.SilkS))
  (gr_text 3A (at 33.274 -72.644 90) (layer F.SilkS))
  (gr_text 20A (at 20.828 -70.358 90) (layer F.SilkS))
  (gr_text Portail (at 191.77 -3.302) (layer F.SilkS))
  (gr_text Ventail (at 175.514 -3.302) (layer F.SilkS))
  (gr_text Portail (at 178.816 -18.796) (layer F.SilkS))
  (gr_text Statut (at 156.21 -3.302) (layer F.SilkS))
  (gr_text Cde (at 141.732 -3.302) (layer F.SilkS))
  (gr_text _/_ (at 125.984 -3.302) (layer F.SilkS))
  (gr_text Lumiere (at 148.59 -19.05) (layer F.SilkS))
  (gr_text Gauche (at 109.22 -3.302) (layer F.SilkS))
  (gr_text Droit (at 91.44 -3.302) (layer F.SilkS))
  (gr_text Verrou (at 74.676 -3.302) (layer F.SilkS))
  (gr_text - (at 57.404 -18.034) (layer F.SilkS))
  (gr_text + (at 51.816 -17.78) (layer F.SilkS))
  (gr_text Out5v (at 52.578 -24.638) (layer F.SilkS))
  (gr_text - (at 43.942 -18.034) (layer F.SilkS))
  (gr_text - (at 28.956 -18.034) (layer F.SilkS))
  (gr_text + (at 36.322 -17.78) (layer F.SilkS))
  (gr_text + (at 21.082 -18.034) (layer F.SilkS))
  (gr_text Bat12v (at 30.226 -24.638) (layer F.SilkS))
  (gr_line (start 0.0761 0.0966) (end 253.7461 0.0966) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 253.7461 0.0966) (end 253.7461 -152.2934) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 253.7461 -152.2934) (end 0.0761 -152.2934) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.0761 -152.2934) (end 0.0761 0.0966) (layer Edge.Cuts) (width 0.15))
  (zone (net 80) (net_name "Net-(ACS1-PadGND)") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0.635 -151.892) (xy 253.365 -151.892) (xy 253.365 -0.127) (xy 0.635 -0.127)
      )
    )
  )
  (zone (net 80) (net_name "Net-(ACS1-PadGND)") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0 -152.4) (xy 253.746 -152.4) (xy 253.746 0) (xy 0 0)
      )
    )
  )
)
