(kicad_pcb (version 20171130) (host pcbnew 5.0.2-5.fc29)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 103)
    (zones 0)
    (modules 45)
    (nets 16)
  )
  (page USLetter portrait)
  (title_block
    (title "1-wire Distribution Board")
    (date 2019-01-26)
    (rev 12)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.381)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FEFFF86F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 +5V)
  (net 10 /BUS3)
  (net 11 /BUS2)
  (net 12 /BUS1)
  (net 13 "Net-(U1-Pad8)")
  (net 14 "Net-(U1-Pad10)")
  (net 15 "Net-(U1-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.508)
    (add_net +5V)
    (add_net /BUS1)
    (add_net /BUS2)
    (add_net /BUS3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad8)")
  )
  (module 54602-908LF:AMPHENOL_54602-908LF (layer F.Cu) (tedit 0)
    (at 192.405 63.5 90)
    (fp_text reference J1 (at -4.96784 -11.6463 90) (layer F.SilkS))
    (fp_text value 54602-908LF (at -0.075 4.985 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -4.445 -6.35 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.175 -8.89 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 3 thru_hole circle (at -1.905 -6.35 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -0.635 -8.89 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad 5 thru_hole circle (at 0.635 -6.35 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 1.905 -8.89 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad 7 thru_hole circle (at 3.175 -6.35 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 4.445 -8.89 270) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad Hole np_thru_hole circle (at -5.715 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 5.715 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 187.96 109.855)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D1 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value PWR (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 177.8 59.69 180)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D2 (at 1.27 3.175 180) (layer F.SilkS))
    (fp_text value BUS3ACT (at 1.27 -3.175 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 177.8 97.155 180)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D3 (at 1.27 3.175 180) (layer F.SilkS))
    (fp_text value BUS2ACT (at 1.27 -3.175 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5C8051A9)
    (at 177.8 132.715 180)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D4 (at 1.27 3.175 180) (layer F.SilkS))
    (fp_text value BUS1ACT (at 1.27 -3.175 180) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_5mm (layer F.Cu) (tedit 5C81126F)
    (at 194.31 134.62)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 6) (layer F.Fab) hide)
    (fp_text user %R (at 0.31 -0.65) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_5mm (layer F.Cu) (tedit 5C811262)
    (at 194.31 48.26 180)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -6 180) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 6 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 180) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0 180) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_5mm (layer F.Cu) (tedit 5C811275)
    (at 116.84 134.62)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 6) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_5mm (layer F.Cu) (tedit 5C811269)
    (at 116.84 48.26 180)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -6 180) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 6 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 270) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0 180) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 132.08 122.555 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J2 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value A1-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 127 132.715)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J3 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value A1-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 132.08 86.995 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J4 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value B1-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 127 97.155)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J5 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value B1-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 132.08 50.165 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J6 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value C1-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 127 60.325)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J7 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value C1-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 141.605 122.555 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J8 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value A2-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 136.525 132.715)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J9 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value A2-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 141.605 86.995 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J10 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value B2-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 136.525 97.155)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J11 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value B2-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 141.605 50.165 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J12 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value C2-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 136.525 60.325)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J13 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value C2-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 151.13 122.555 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J14 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value A3-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 146.05 132.715)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J15 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value A3-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 151.13 86.995 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J16 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value B3-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 146.05 97.155)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J17 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value B3-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 151.13 50.165 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J18 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value C3-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 146.05 60.325)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J19 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value C3-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 160.655 122.555 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J20 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value A4-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 155.575 132.715)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J21 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value A4-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 160.655 86.995 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J22 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value B4-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 155.575 97.155)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J23 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value B4-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 160.655 50.165 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J24 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value C4-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 155.575 60.325)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J25 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value C4-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 170.18 122.555 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J26 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value A5-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 165.1 132.715)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J27 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value A5-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 170.18 86.995 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J28 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value B5-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 165.1 97.155)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J29 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value B5-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 170.18 50.165 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J30 (at 2.54 -4.16 180) (layer F.SilkS))
    (fp_text value C5-R (at 2.54 4.16 180) (layer F.Fab))
    (fp_text user %R (at 2.54 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad "" np_thru_hole circle (at 2.54 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 165.1 60.325)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J31 (at 2.54 -4.16) (layer F.SilkS))
    (fp_text value C5-S (at 2.54 4.16) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 189.23 120.65 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value R3k3 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.88 -0.04 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 53.975 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value R3K3 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 91.44 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value R3K3 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 127 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value R3K3 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 185.42 83.82)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HC14 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /BUS3))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /BUS2))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /BUS1))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 193.04 78.74)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 -3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "1-Wire Bus Distribution Board - V2.0\nCopyright 2019 - Kevin P. Fleming\nLicensed under CC-BY-SA 4.0\nhttp://superionic.us" (at 149.225 73.66) (layer F.SilkS))
  (gr_line (start 200.66 41.91) (end 200.66 140.97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 41.91) (end 200.66 41.91) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 140.97) (end 110.49 41.91) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.66 140.97) (end 110.49 140.97) (layer Edge.Cuts) (width 0.1))
  (zone (net 9) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.66 41.91) (xy 200.66 140.97) (xy 110.49 140.97) (xy 110.49 41.91)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.66 41.91) (xy 200.66 140.97) (xy 110.49 140.97) (xy 110.49 41.91)
      )
    )
  )
)
