(module Panasonic_ERJ_3EKF_fp (layer F.Cu) (tedit 5A74E519)
  (attr smd)
  (descr "Panasonic_ERJ_3EKF_ StepUp generated footprint")
  (fp_text reference "FC_" (at 0.0 1.0) (layer F.SilkS))
  (fp_text value "Val_" (at 0.0 -1.0) (layer F.SilkS))
  (fp_text user %R (at 0.0 1.0) (layer F.Fab))
  (fp_text user "EDIT PAD NUMBERS" (at 0.0 -2.0) (layer Cmts.User))
  (pad # smd rect (at -0.7249999999999999 -0.0) (size 0.6499999999999998 0.9)  (layers F.Cu F.Paste F.Mask))
  (pad # smd rect (at 0.7249999999999999 -0.0) (size 0.6499999999999998 0.9)  (layers F.Cu F.Paste F.Mask))
   (model C:\Temp\Panasonic_ERJ_3EKF_.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
