(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0)")
  (general
    (thickness 1.6)
    (drawings 60)
    (tracks 785)
    (zones 0)
    (modules 72)
    (nets 66)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.075)
    (pad_size 1.99898 1.99898)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VBAT)
  (net 2 GND)
  (net 3 /5.0V_OUT)
  (net 4 /5V)
  (net 5 /3.3V)
  (net 6 "Net-(C15-Pad1)")
  (net 7 "Net-(D1-Pad4)")
  (net 8 /LED_DIN)
  (net 9 "Net-(D2-Pad4)")
  (net 10 "Net-(D3-Pad4)")
  (net 11 "Net-(D4-Pad4)")
  (net 12 "Net-(D5-Pad4)")
  (net 13 "Net-(D6-Pad4)")
  (net 14 "Net-(D7-Pad4)")
  (net 15 "Net-(D8-Pad4)")
  (net 16 "Net-(D9-Pad2)")
  (net 17 "Net-(D10-Pad1)")
  (net 18 "Net-(D10-Pad2)")
  (net 19 /BTN_IN)
  (net 20 "Net-(J1-Pad2)")
  (net 21 "Net-(J1-Pad3)")
  (net 22 "Net-(J3-Pad2)")
  (net 23 "Net-(J3-Pad3)")
  (net 24 "Net-(J3-Pad4)")
  (net 25 "Net-(J3-Pad6)")
  (net 26 /MOT1)
  (net 27 /MOT2)
  (net 28 /MOT3)
  (net 29 /MOT4)
  (net 30 /MOT5)
  (net 31 /MOT6)
  (net 32 /MOT7)
  (net 33 /MOT8)
  (net 34 "Net-(Q1-Pad1)")
  (net 35 "Net-(Q2-Pad1)")
  (net 36 "Net-(Q3-Pad1)")
  (net 37 "Net-(Q4-Pad1)")
  (net 38 "Net-(Q5-Pad1)")
  (net 39 "Net-(Q6-Pad1)")
  (net 40 "Net-(Q7-Pad1)")
  (net 41 "Net-(Q8-Pad1)")
  (net 42 /SWDIO)
  (net 43 /SWDCLK)
  (net 44 /MOTOR_CNT1)
  (net 45 "Net-(R5-Pad2)")
  (net 46 "Net-(R7-Pad1)")
  (net 47 /BAT_STAT)
  (net 48 /MOTOR_CNT5)
  (net 49 /MOTOR_CNT2)
  (net 50 /MOTOR_CNT6)
  (net 51 /MOTOR_CNT3)
  (net 52 /MOTOR_CNT7)
  (net 53 /MOTOR_CNT4)
  (net 54 /MOTOR_CNT8)
  (net 55 "Net-(SW1-Pad2)")
  (net 56 "Net-(U1-Pad3)")
  (net 57 "Net-(U1-Pad4)")
  (net 58 "Net-(U1-Pad5)")
  (net 59 "Net-(U1-Pad19)")
  (net 60 "Net-(U1-Pad20)")
  (net 61 "Net-(U1-Pad23)")
  (net 62 "Net-(U2-Pad4)")
  (net 63 "Net-(U4-Pad6)")
  (net 64 "Net-(U1-Pad16)")
  (net 65 "Net-(U1-Pad15)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BAT_STAT)
    (add_net /BTN_IN)
    (add_net /LED_DIN)
    (add_net /MOT1)
    (add_net /MOT2)
    (add_net /MOT3)
    (add_net /MOT4)
    (add_net /MOT5)
    (add_net /MOT6)
    (add_net /MOT7)
    (add_net /MOT8)
    (add_net /MOTOR_CNT1)
    (add_net /MOTOR_CNT2)
    (add_net /MOTOR_CNT3)
    (add_net /MOTOR_CNT4)
    (add_net /MOTOR_CNT5)
    (add_net /MOTOR_CNT6)
    (add_net /MOTOR_CNT7)
    (add_net /MOTOR_CNT8)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /VBAT)
    (add_net GND)
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(D4-Pad4)")
    (add_net "Net-(D5-Pad4)")
    (add_net "Net-(D6-Pad4)")
    (add_net "Net-(D7-Pad4)")
    (add_net "Net-(D8-Pad4)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U4-Pad6)")
  )
  (net_class Power ""
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /5.0V_OUT)
    (add_net /5V)
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill0.8mm (layer F.Cu) (tedit 5D5EBDCA)
    (at 116.4336 98.171 270)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference BT1 (at 1.99898 1.89484 90) (layer F.SilkS))
    (fp_text value "3.7V BAT" (at 1.905 2.54 90) (layer F.Fab))
    (fp_text user %R (at 1.905 0 90) (layer F.Fab))
    (pad 1 connect rect (at 0 0 270) (size 1.99898 1.99898) (layers F.Cu F.Mask)
      (net 1 /VBAT))
    (pad 2 connect circle (at 3.81 0 270) (size 1.99898 1.99898) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.55244 105.12806 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.03302 0.87376 180) (layer F.SilkS))
    (fp_text value 1.0uF (at 1.778 1.016 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 /VBAT))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 134.89432 101.08946 180)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.00762 -0.6858) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 /VBAT))
    (pad 2 smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 128.74752 101.0539)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.04826 0.70866 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.05 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.68 180) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.85064 114.44986)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.05) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 4 /5V))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.99492 112.96396 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.00508 -0.67818 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.05 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 /VBAT))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.36754 104.23652 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -0.04318 -0.5715 270) (layer F.SilkS))
    (fp_text value 1.0uF (at 1.524 -0.762 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 5 /3.3V))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 154.89428 84.4804 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.06604 0.69596 -90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 -90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 -90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 177.97526 85.82152 270)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.00762 -0.81026 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 186.35726 104.56926 180)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.03302 -0.71882 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.68 180) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 2 smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 168.86428 115.8367 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0.01778 -0.75184 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 90) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 145.35404 115.73002 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -0.00762 -0.7874 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 90) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 122.1867 114.11458 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0.01778 -0.8001 -90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 -90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.68 -90) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 113.71072 95.6945)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.03048 -0.70866) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.68 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 131.1656 84.2518 270)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0.06096 -0.72898 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.05 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.00652 110.09884)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.02032 -0.65024) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C15-Pad1)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.1458 104.2543 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -0.07112 -0.69088 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.066 -2.8194 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 5 /3.3V))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 150.5458 84.5566 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D1 (at 4.46278 -0.38608) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 3 smd rect (at -2.45 1.6 180) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (pad 4 smd rect (at -2.45 -1.6 180) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 2.45 1.6 180) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 8 /LED_DIN))
    (pad 1 smd rect (at 2.45 -1.6 180) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 173.5074 84.9884 170)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D2 (at 4.401921 0.098166 350) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4 350) (layer B.Fab))
    (fp_text user %R (at 0 0 350) (layer B.Fab))
    (pad 3 smd rect (at -2.45 1.6 170) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (pad 4 smd rect (at -2.45 -1.6 170) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D2-Pad4)"))
    (pad 2 smd rect (at 2.45 1.6 170) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at 2.45 -1.6 170) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 186.106 99.986 90)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D3 (at 4.80204 -0.0764 270) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at 2.45 -1.6 90) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.45 1.6 90) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D2-Pad4)"))
    (pad 4 smd rect (at -2.45 -1.6 90) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D3-Pad4)"))
    (pad 3 smd rect (at -2.45 1.6 90) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 173.4312 114.9604 10)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D4 (at 4.559063 -0.111724 190) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4 190) (layer B.Fab))
    (fp_text user %R (at 0 0 190) (layer B.Fab))
    (pad 1 smd rect (at 2.45 -1.6 10) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.45 1.6 10) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D3-Pad4)"))
    (pad 4 smd rect (at -2.45 -1.6 10) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D4-Pad4)"))
    (pad 3 smd rect (at -2.45 1.6 10) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 150.3045 115.36934)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D5 (at 4.67868 -0.03556) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.45 -1.6) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.45 1.6) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D4-Pad4)"))
    (pad 4 smd rect (at -2.45 -1.6) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D5-Pad4)"))
    (pad 3 smd rect (at -2.45 1.6) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 126.8603 114.92484 350)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D6 (at 4.78564 0.226524 350) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4 350) (layer B.Fab))
    (fp_text user %R (at 0 0 350) (layer B.Fab))
    (pad 1 smd rect (at 2.45 -1.6 350) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.45 1.6 350) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D5-Pad4)"))
    (pad 4 smd rect (at -2.45 -1.6 350) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D6-Pad4)"))
    (pad 3 smd rect (at -2.45 1.6 350) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 113.91646 100.09632 270)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D7 (at 4.6228 -0.26924 270) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.45 1.6 270) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D6-Pad4)"))
    (pad 4 smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D7-Pad4)"))
    (pad 3 smd rect (at -2.45 1.6 270) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5AA4B263)
    (at 126.79426 84.9757 190)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D8 (at 4.546587 0.105306 190) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4 190) (layer B.Fab))
    (fp_text user %R (at 0 0 190) (layer B.Fab))
    (pad 3 smd rect (at -2.45 1.6 190) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (pad 4 smd rect (at -2.45 -1.6 190) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D8-Pad4)"))
    (pad 2 smd rect (at 2.45 1.6 190) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D7-Pad4)"))
    (pad 1 smd rect (at 2.45 -1.6 190) (size 1.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.4097 114.41176 180)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D10 (at -0.04064 -0.6731) (layer F.SilkS))
    (fp_text value LED (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D10-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 143.98752 100.86086 90)
    (descr "Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D11 (at 0.0127 0.65532 -90) (layer B.SilkS))
    (fp_text value D_TVS (at 0 -1.05 -90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 -90) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 19 /BTN_IN))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x04_P3.175mm_Drill0.8mm (layer F.Cu) (tedit 5AEE5FAE)
    (at 122.1486 105.4862 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J1 (at 5.19938 -1.84658 90) (layer F.SilkS))
    (fp_text value JTAG (at 4.7625 3.175 90) (layer F.Fab) hide)
    (fp_text user %R (at 4.7625 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 /3.3V))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 6.35 0 90) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 9.525 0 90) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 5A1DC0BD)
    (at 150.255 115.1714)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J3 (at 0 -3.3 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 4.6 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 180) (layer Dwgs.User))
    (fp_text user %R (at 0 1.2) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 4 /5V))
    (pad 2 smd rect (at -0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at -2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at -0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module personal:M20-9740646 (layer F.Cu) (tedit 0)
    (at 150.0378 87.376)
    (descr M20-9740646)
    (tags Connector)
    (fp_text reference J5 (at -0.34843 1.32104) (layer F.SilkS))
    (fp_text value M20-9740646 (at -0.34843 1.32104) (layer F.SilkS) hide)
    (fp_text user %R (at -0.34843 1.32104) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.35 6.44) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 26 /MOT1))
    (pad 2 thru_hole circle (at -6.35 3.9) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 3 thru_hole circle (at -3.81 6.44) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 27 /MOT2))
    (pad 4 thru_hole circle (at -3.81 3.9) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 5 thru_hole circle (at -1.27 6.44) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 28 /MOT3))
    (pad 6 thru_hole circle (at -1.27 3.9) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 7 thru_hole circle (at 1.27 6.44) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 29 /MOT4))
    (pad 8 thru_hole circle (at 1.27 3.9) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 9 thru_hole circle (at 3.81 6.44) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 30 /MOT5))
    (pad 10 thru_hole circle (at 3.81 3.9) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 11 thru_hole circle (at 6.35 6.44) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 31 /MOT6))
    (pad 12 thru_hole circle (at 6.35 3.9) (size 1.7 1.7) (drill 1.11) (layers *.Cu *.Mask)
      (net 1 /VBAT))
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill0.8mm (layer F.Cu) (tedit 5D5EBDAE)
    (at 156.53004 106.2609 180)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J6 (at 5.88518 -0.00508) (layer F.SilkS))
    (fp_text value Conn_Mot_7 (at 1.905 2.54) (layer F.Fab))
    (fp_text user %R (at 1.905 0) (layer F.Fab))
    (pad 1 connect rect (at 0 0 180) (size 1.99898 1.99898) (layers F.Cu F.Mask)
      (net 1 /VBAT))
    (pad 2 connect circle (at 3.81 0 180) (size 1.99898 1.99898) (layers F.Cu F.Mask)
      (net 32 /MOT7))
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill0.8mm (layer F.Cu) (tedit 5D5EBD9F)
    (at 146.0754 106.22534 180)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J7 (at 5.87248 -0.06858) (layer F.SilkS))
    (fp_text value Conn_Mot_8 (at 1.905 2.54) (layer F.Fab))
    (fp_text user %R (at 1.905 0) (layer F.Fab))
    (pad 2 connect circle (at 3.81 0 180) (size 1.99898 1.99898) (layers F.Cu F.Mask)
      (net 33 /MOT8))
    (pad 1 connect rect (at 0 0 180) (size 1.99898 1.99898) (layers F.Cu F.Mask)
      (net 1 /VBAT))
  )
  (module Inductor_SMD:L_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 131.79044 99.8601 180)
    (descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at -1.0668 -0.03556) (layer B.SilkS))
    (fp_text value 22uH (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 /VBAT))
    (pad 2 smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 142.78356 97.20326 90)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q1 (at 1.12776 -1.4605 90) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0 90) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0.8 0 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /MOT1))
    (pad 2 smd rect (at -0.8 0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.8 -0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q1-Pad1)"))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 145.79346 97.18294 90)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q2 (at 1.08966 -1.45034 90) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0 90) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0.8 0 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /MOT2))
    (pad 2 smd rect (at -0.8 0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.8 -0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q2-Pad1)"))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 148.94052 97.17024 90)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q3 (at 1.08204 -1.43256 90) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 -0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -0.8 0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.8 0 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /MOT3))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 151.95296 97.15754 90)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q4 (at 1.08712 -1.42748 90) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 -0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -0.8 0.5 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.8 0 180) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MOT4))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 160.08106 89.19934 180)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q5 (at 1.84414 0.66256 90) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0.8 0 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /MOT5))
    (pad 2 smd rect (at -0.8 0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.8 -0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q5-Pad1)"))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 167.40378 89.57818 180)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q6 (at 1.905 0.69088 90) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 -0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at -0.8 0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.8 0 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /MOT6))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 153.6954 108.8009 180)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q7 (at 2.02692 0.55626) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0.8 0 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /MOT7))
    (pad 2 smd rect (at -0.8 0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.8 -0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Q7-Pad1)"))
  )
  (module DMG1012T-7:SOT50P160X80-3N (layer F.Cu) (tedit 5D5543F7)
    (at 143.08582 109.07522 180)
    (descr SOT523)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q8 (at 2.01168 0.81534) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 -0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Q8-Pad1)"))
    (pad 2 smd rect (at -0.8 0.5 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.8 0 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOT8))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.80874 102.31628)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.34544 -0.70866) (layer F.SilkS))
    (fp_text value 33R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J1-Pad2)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 42 /SWDIO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.5903 99.14636)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.31242 -0.67818) (layer F.SilkS))
    (fp_text value 33R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 43 /SWDCLK))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J1-Pad3)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8671 95.91802)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -0.69088) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 44 /MOTOR_CNT1))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q1-Pad1)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.9052 97.05594)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -0.0381 -0.58928) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.53822 101.0539)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -0.01778 0.70866) (layer B.SilkS))
    (fp_text value 7.5k (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 /5.0V_OUT))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.0452 101.09454)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.04064 0.71882) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(R5-Pad2)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 132.7658 111.24692 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.05 90) (layer F.SilkS) hide)
    (fp_text value 2kΩ (at 0 1.05 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R7-Pad1)"))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.89382 115.90528 180)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.00762 -0.68326) (layer F.SilkS))
    (fp_text value 2.2kΩ (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 4 /5V))
    (pad 2 smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.14992 108.54436)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0.00806 -0.69342) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D10-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 47 /BAT_STAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 132.78104 113.04524 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -0.00508 -0.69596 90) (layer F.SilkS))
    (fp_text value 47kΩ (at -2.22 0.0762 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 47 /BAT_STAT))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.76066 89.99982)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0.01524 -0.57658) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(Q5-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 48 /MOTOR_CNT5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.74546 88.69934)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0.0025 -0.71374) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(Q5-Pad1)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.9433 98.49358)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -0.03048 -0.69342) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 49 /MOTOR_CNT2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 170.25878 90.08618)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0.0152 0.70104) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(Q6-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 50 /MOTOR_CNT6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.93314 99.64928)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0.03302 -0.58166) (layer F.SilkS))
    (fp_text value 51K (at 10.4496 -17.8816) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(Q2-Pad1)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 170.23838 89.01938)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0.0356 -0.6731) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(Q6-Pad1)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.96108 100.78974)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.02032 -0.53594) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 51 /MOTOR_CNT3))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q3-Pad1)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 157.24632 109.52734)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 1.39954 0.02794) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(Q7-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 52 /MOTOR_CNT7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.99156 101.93782)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -0.01016 -0.5842) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 157.28696 108.3564)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -1.397 -0.0127) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(Q7-Pad1)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.02966 103.20528)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -0.01524 -0.6477) (layer F.SilkS))
    (fp_text value 270R (at 35.27 -32.7152) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q4-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 53 /MOTOR_CNT4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.59356 109.6264)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0.05588 0.75438) (layer F.SilkS))
    (fp_text value 270R (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(Q8-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 54 /MOTOR_CNT8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.03474 104.24922 180)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 1.40716 -0.03556) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q4-Pad1)"))
    (pad 1 smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.49958 108.59008)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 1.48586 -0.02794) (layer F.SilkS))
    (fp_text value 51K (at 0 1.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(Q8-Pad1)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.21118 110.08868)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0.03512 -0.65786) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 5 /3.3V))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5A02FC95)
    (at 150.114 100.838)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 4.5) (layer B.SilkS))
    (fp_text value Button (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /BTN_IN))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /BTN_IN))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SKB369:SKYLAB_SKB369 (layer F.Cu) (tedit 0)
    (at 169.5196 99.9998 270)
    (attr smd)
    (fp_text reference U1 (at -6.07109 -12.2915 90) (layer F.SilkS))
    (fp_text value SKB369 (at -5.4257 11.7365 90) (layer F.SilkS))
    (pad 1 smd rect (at -6.85 -3.63 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -6.85 -2.36 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /3.3V))
    (pad 3 smd rect (at -6.85 -1.09 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -6.85 0.18 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -6.85 1.45 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -6.85 2.72 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 /MOTOR_CNT6))
    (pad 7 smd rect (at -6.85 3.99 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /MOTOR_CNT5))
    (pad 8 smd rect (at -6.85 5.26 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /BTN_IN))
    (pad 9 smd rect (at -6.85 6.53 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 /BAT_STAT))
    (pad 10 smd rect (at -6.85 7.8 270) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 0 8.7) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 /MOTOR_CNT3))
    (pad 16 smd rect (at 6.85 7.8 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 6.85 6.53 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 /MOTOR_CNT7))
    (pad 18 smd rect (at 6.85 5.26 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 /MOTOR_CNT8))
    (pad 19 smd rect (at 6.85 3.99 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 6.85 2.72 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 6.85 1.45 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_DIN))
    (pad 22 smd rect (at 6.85 0.18 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C15-Pad1)"))
    (pad 23 smd rect (at 6.85 -1.09 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 6.85 -2.36 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /SWDCLK))
    (pad 25 smd rect (at 6.85 -3.63 90) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 /SWDIO))
    (pad 11 smd rect (at -2.55 8.7) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 /MOTOR_CNT1))
    (pad 12 smd rect (at -1.28 8.7) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 /MOTOR_CNT2))
    (pad 14 smd rect (at 1.28 8.7) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 /MOTOR_CNT4))
    (pad 15 smd rect (at 2.55 8.7) (size 3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-Pad15)"))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 129.30886 104.7496 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0.02032 2.12598) (layer F.SilkS))
    (fp_text value AP2127K-3.3 (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /3.3V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBAT))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBAT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 129.72052 111.85656)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -0.01288 -2.1311) (layer F.SilkS))
    (fp_text value MCP73831-2-OT (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBAT))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /5V))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module personal:SDB628 (layer B.Cu) (tedit 5D55C7D2)
    (at 133.25094 97.60712 90)
    (fp_text reference U4 (at 0.03048 2.67208 -90) (layer B.SilkS))
    (fp_text value SDB628 (at 0.03048 3.94208 -90) (layer B.Fab) hide)
    (pad 6 smd rect (at -0.94488 0.8509 90) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(U4-Pad6)"))
    (pad 5 smd rect (at -0.00762 0.8509 90) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBAT))
    (pad 4 smd rect (at 0.96012 0.8509 90) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBAT))
    (pad 1 smd rect (at -0.94488 -0.8509 90) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.00762 -0.8509 90) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.96012 -0.8509 90) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R5-Pad2)"))
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 128.17348 97.42678)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D9 (at 0.00762 1.4859) (layer B.SilkS))
    (fp_text value SS310 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 /5.0V_OUT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 161.998484 106) (end 162.748484 106) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 161.998484 93.999999) (end 162.748484 93.999999) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 176 109) (end 176.75 109) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 176 91.999999) (end 176.75 91.999999) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 138 106) (end 138.75 106) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 138 93.999999) (end 138.75 93.999999) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 123.999999 109) (end 124.749999 109) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 123.999999 91.999999) (end 124.749999 91.999999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.017821 86.499999) (end 135.017821 81.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.017821 86.499999) (end 141.017821 86.499999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.017821 86.499999) (end 141.017821 81.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129 100) (end 129 81.5) (angle -38.05977315) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.017821 81.5) (end 129 81.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171 100) (end 182.33 114.62) (angle 37.77446008) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171 100) (end 186.42 110.23) (angle -66.2629705) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171 100) (end 182.54 85.56) (angle -38.63076342) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129 100) (end 117.460001 114.449999) (angle -38.61142065) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129 100) (end 113.540001 89.850001) (angle -65.94545911) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.758269 106.827503) (end 186.42 110.23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.674826 111.22358) (end 182.33 114.62) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.84362 88.893726) (end 182.54 85.56) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.86014 93.351031) (end 186.571728 90.00247) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.133312 106.638682) (end 113.429859 109.980218) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.163508 111.112144) (end 117.460001 114.449999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.219223 93.21854) (end 113.540001 89.850001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.267846 88.790374) (end 117.594894 85.43348) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.055489 81.5) (end 171 81.515271) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.017821 81.5) (end 159.055489 81.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.055489 86.499999) (end 165.055489 81.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.055489 86.499999) (end 159.055489 81.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.05305 118.5) (end 171 118.496305) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.066462 118.5) (end 159.05305 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.066462 118.491) (end 129 118.491) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.05305 113.5) (end 165.05305 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.05305 113.5) (end 159.05305 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.066462 113.5) (end 141.066462 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.066462 113.5) (end 135.066462 118.491) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.84362 88.893726) (end 182.86014 93.351031) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.758269 106.827503) (end 178.674826 111.22358) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.219223 93.21854) (end 121.267846 88.790374) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.163508 111.112144) (end 117.133312 106.638682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.055489 86.499999) (end 165.055489 86.499999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.066462 113.5) (end 135.066462 113.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.05305 113.5) (end 159.05305 113.5) (layer Edge.Cuts) (width 0.05))
)
