(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 366)
    (zones 0)
    (modules 160)
    (nets 149)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.33)
    (user_trace_width 0.25)
    (user_trace_width 0.33)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin -95 165)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /µC_VCC_SENSE)
  (net 2 GND)
  (net 3 +5V)
  (net 4 µC_PWM1)
  (net 5 µC_PWM2)
  (net 6 µC_PWM3)
  (net 7 µC_PWM4)
  (net 8 µC_PWM5)
  (net 9 µC_PWM6)
  (net 10 "Net-(C13-Pad1)")
  (net 11 "Net-(D8-Pad1)")
  (net 12 µC_FD1)
  (net 13 µC_FD2)
  (net 14 µC_FD3)
  (net 15 µC_FD4)
  (net 16 µC_FD5)
  (net 17 µC_FD6)
  (net 18 "Net-(C14-Pad2)")
  (net 19 "Net-(D15-Pad1)")
  (net 20 µC_DIAG1)
  (net 21 DIAG1)
  (net 22 µC_DIAG3)
  (net 23 DIAG3)
  (net 24 µC_DIAG5)
  (net 25 DIAG5)
  (net 26 µC_DIAG2)
  (net 27 DIAG2)
  (net 28 µC_DIAG4)
  (net 29 DIAG4)
  (net 30 µC_DIAG6)
  (net 31 DIAG6)
  (net 32 "/Output Driver/H_RAIL")
  (net 33 "Net-(Q1-Pad3)")
  (net 34 "Net-(Q1-Pad1)")
  (net 35 /KL30)
  (net 36 "Net-(Q2-Pad1)")
  (net 37 "Net-(Q3-Pad3)")
  (net 38 H_EN)
  (net 39 L_EN)
  (net 40 "/Output Driver/L_RAIL")
  (net 41 "Net-(Q5-Pad3)")
  (net 42 "Net-(Q5-Pad1)")
  (net 43 "Net-(Q10-Pad1)")
  (net 44 "Net-(Q6-Pad1)")
  (net 45 "Net-(Q11-Pad1)")
  (net 46 "Net-(Q7-Pad1)")
  (net 47 "Net-(Q13-Pad1)")
  (net 48 "Net-(Q8-Pad1)")
  (net 49 /PWM1_OUT)
  (net 50 /PWM2_OUT)
  (net 51 "Net-(Q15-Pad3)")
  (net 52 "Net-(Q15-Pad1)")
  (net 53 "Net-(Q16-Pad3)")
  (net 54 "Net-(Q16-Pad1)")
  (net 55 "Net-(Q17-Pad3)")
  (net 56 "Net-(Q17-Pad1)")
  (net 57 LCD_CON)
  (net 58 B4)
  (net 59 B3)
  (net 60 B2)
  (net 61 B1)
  (net 62 B0)
  (net 63 CAN_RX)
  (net 64 CAN_TX)
  (net 65 LCD_EN)
  (net 66 LCD_D6)
  (net 67 LCD_D5)
  (net 68 LCD_D4)
  (net 69 LCD_D3)
  (net 70 LCD_D2)
  (net 71 LCD_D1)
  (net 72 LCD_D0)
  (net 73 USART_RX)
  (net 74 USART_TX)
  (net 75 FAN_REVERSE)
  (net 76 "Net-(U2-Pad7)")
  (net 77 "Net-(U2-Pad6)")
  (net 78 CAN_L)
  (net 79 CAN_H)
  (net 80 "Net-(C2-Pad1)")
  (net 81 "Net-(C4-Pad1)")
  (net 82 "Net-(C6-Pad1)")
  (net 83 "Net-(C18-Pad1)")
  (net 84 "Net-(C20-Pad1)")
  (net 85 "Net-(C21-Pad1)")
  (net 86 VCC)
  (net 87 "Net-(J1-Pad18)")
  (net 88 ~RESET)
  (net 89 "Net-(R2-Pad1)")
  (net 90 IO_0)
  (net 91 IO_1)
  (net 92 IO_2)
  (net 93 IO_3)
  (net 94 B)
  (net 95 A)
  (net 96 MOSI)
  (net 97 SCK)
  (net 98 MISO)
  (net 99 CAN_CS)
  (net 100 CAN_INT)
  (net 101 "Net-(U8-Pad11)")
  (net 102 "Net-(U8-Pad10)")
  (net 103 CAN_CLK)
  (net 104 "Net-(U8-Pad7)")
  (net 105 "Net-(U8-Pad6)")
  (net 106 "Net-(U8-Pad5)")
  (net 107 "Net-(U8-Pad4)")
  (net 108 "Net-(U8-Pad3)")
  (net 109 FD_EN)
  (net 110 DIAG_EN)
  (net 111 "Net-(U10-Pad13)")
  (net 112 RS485_RW)
  (net 113 "Net-(U10-Pad12)")
  (net 114 "Net-(U10-Pad11)")
  (net 115 "Net-(U10-Pad9)")
  (net 116 "Net-(U10-Pad8)")
  (net 117 "Net-(U11-Pad12)")
  (net 118 "Net-(U11-Pad11)")
  (net 119 "Net-(U11-Pad9)")
  (net 120 "Net-(U11-Pad8)")
  (net 121 "Net-(U13-Pad42)")
  (net 122 "Net-(U13-Pad41)")
  (net 123 "Net-(U13-Pad10)")
  (net 124 "Net-(U13-Pad9)")
  (net 125 "Net-(U13-Pad6)")
  (net 126 "Net-(U13-Pad5)")
  (net 127 "Net-(U13-Pad4)")
  (net 128 /SAMC/µC_VCC_SENSE)
  (net 129 "Net-(D28-Pad2)")
  (net 130 /PWM3_OUT)
  (net 131 /PWM5_OUT)
  (net 132 /PWM4_OUT)
  (net 133 /PWM6_OUT)
  (net 134 "Net-(J2-Pad8)")
  (net 135 "Net-(J2-Pad7)")
  (net 136 "Net-(J2-Pad6)")
  (net 137 SWCLK)
  (net 138 SWDIO)
  (net 139 "Net-(C17-Pad1)")
  (net 140 "/Diag inputs/PU_SUPPLY")
  (net 141 "Net-(Q24-Pad1)")
  (net 142 "Net-(R9-Pad1)")
  (net 143 "Net-(R56-Pad1)")
  (net 144 "Net-(R64-Pad1)")
  (net 145 "Net-(R65-Pad2)")
  (net 146 "Net-(R66-Pad2)")
  (net 147 "Net-(R67-Pad2)")
  (net 148 "Net-(R68-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "/Diag inputs/PU_SUPPLY")
    (add_net /KL30)
    (add_net "/Output Driver/H_RAIL")
    (add_net "/Output Driver/L_RAIL")
    (add_net /PWM1_OUT)
    (add_net /PWM2_OUT)
    (add_net /PWM3_OUT)
    (add_net /PWM4_OUT)
    (add_net /PWM5_OUT)
    (add_net /PWM6_OUT)
    (add_net /SAMC/µC_VCC_SENSE)
    (add_net /µC_VCC_SENSE)
    (add_net A)
    (add_net B)
    (add_net B0)
    (add_net B1)
    (add_net B2)
    (add_net B3)
    (add_net B4)
    (add_net CAN_CLK)
    (add_net CAN_CS)
    (add_net CAN_H)
    (add_net CAN_INT)
    (add_net CAN_L)
    (add_net CAN_RX)
    (add_net CAN_TX)
    (add_net DIAG1)
    (add_net DIAG2)
    (add_net DIAG3)
    (add_net DIAG4)
    (add_net DIAG5)
    (add_net DIAG6)
    (add_net DIAG_EN)
    (add_net FAN_REVERSE)
    (add_net FD_EN)
    (add_net GND)
    (add_net H_EN)
    (add_net IO_0)
    (add_net IO_1)
    (add_net IO_2)
    (add_net IO_3)
    (add_net LCD_CON)
    (add_net LCD_D0)
    (add_net LCD_D1)
    (add_net LCD_D2)
    (add_net LCD_D3)
    (add_net LCD_D4)
    (add_net LCD_D5)
    (add_net LCD_D6)
    (add_net LCD_EN)
    (add_net L_EN)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D28-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q11-Pad1)")
    (add_net "Net-(Q13-Pad1)")
    (add_net "Net-(Q15-Pad1)")
    (add_net "Net-(Q15-Pad3)")
    (add_net "Net-(Q16-Pad1)")
    (add_net "Net-(Q16-Pad3)")
    (add_net "Net-(Q17-Pad1)")
    (add_net "Net-(Q17-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q24-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R56-Pad1)")
    (add_net "Net-(R64-Pad1)")
    (add_net "Net-(R65-Pad2)")
    (add_net "Net-(R66-Pad2)")
    (add_net "Net-(R67-Pad2)")
    (add_net "Net-(R68-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U10-Pad11)")
    (add_net "Net-(U10-Pad12)")
    (add_net "Net-(U10-Pad13)")
    (add_net "Net-(U10-Pad8)")
    (add_net "Net-(U10-Pad9)")
    (add_net "Net-(U11-Pad11)")
    (add_net "Net-(U11-Pad12)")
    (add_net "Net-(U11-Pad8)")
    (add_net "Net-(U11-Pad9)")
    (add_net "Net-(U13-Pad10)")
    (add_net "Net-(U13-Pad4)")
    (add_net "Net-(U13-Pad41)")
    (add_net "Net-(U13-Pad42)")
    (add_net "Net-(U13-Pad5)")
    (add_net "Net-(U13-Pad6)")
    (add_net "Net-(U13-Pad9)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U8-Pad10)")
    (add_net "Net-(U8-Pad11)")
    (add_net "Net-(U8-Pad3)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U8-Pad5)")
    (add_net "Net-(U8-Pad6)")
    (add_net "Net-(U8-Pad7)")
    (add_net RS485_RW)
    (add_net SCK)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net USART_RX)
    (add_net USART_TX)
    (add_net VCC)
    (add_net ~RESET)
    (add_net µC_DIAG1)
    (add_net µC_DIAG2)
    (add_net µC_DIAG3)
    (add_net µC_DIAG4)
    (add_net µC_DIAG5)
    (add_net µC_DIAG6)
    (add_net µC_FD1)
    (add_net µC_FD2)
    (add_net µC_FD3)
    (add_net µC_FD4)
    (add_net µC_FD5)
    (add_net µC_FD6)
    (add_net µC_PWM1)
    (add_net µC_PWM2)
    (add_net µC_PWM3)
    (add_net µC_PWM4)
    (add_net µC_PWM5)
    (add_net µC_PWM6)
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 41.2 -38.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R68 (at -3.1 0) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(R68-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 CAN_RX))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 41.2 -36.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R67 (at 3 0) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 "Net-(R67-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 CAN_TX))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 71.2 -46.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R66 (at -0.1 1.6) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 "Net-(R66-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 USART_TX))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 72.5 -54.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R65 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 "Net-(R65-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 USART_RX))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 40.7 -47.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R64 (at 3 -0.1) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 MISO))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 "Net-(R64-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.4 -88.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R63 (at -3 -0.1) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 µC_DIAG6))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.4 -85.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R62 (at -3.1 -0.1) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 µC_DIAG4))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.4 -83 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R61 (at -2.9 0) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 µC_DIAG2))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.4 -87.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R60 (at -2.9 -0.1) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 µC_DIAG5))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.4 -84.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R59 (at -2.87 -0.01) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 µC_DIAG3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.4 -81.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R58 (at -2.9 0) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 µC_DIAG1))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 37.1 -93.7 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R57 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 141 "Net-(Q24-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 B4))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 4.7 -46.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R56 (at 2.7 0) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 SCK))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 "Net-(R56-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 4.7 -44.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.3 -0.1) (layer F.SilkS))
    (fp_text value 33R_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 MOSI))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 142 "Net-(R9-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 32.2 -92.6 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q24 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 140 "/Diag inputs/PU_SUPPLY"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(Q24-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 30.4 -7.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R55 (at 0.03 -1.385) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 SWCLK))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Header_WE:62201021121 (layer F.Cu) (tedit 5DA48D62)
    (at 30.4 -12.5 90)
    (descr "2x5 @ 1.27mm 5H TH")
    (fp_text reference J2 (at -0.212132 -2.05061 90) (layer F.SilkS))
    (fp_text value ARM_SWD_INTERFACE (at -5.08 -6.35 90) (layer F.Fab))
    (pad 10 thru_hole circle (at 2.54 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 ~RESET))
    (pad 9 thru_hole circle (at 2.54 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 1.27 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 134 "Net-(J2-Pad8)"))
    (pad 7 thru_hole circle (at 1.27 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 135 "Net-(J2-Pad7)"))
    (pad 6 thru_hole circle (at 0 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 136 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at 0 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -1.27 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 137 SWCLK))
    (pad 3 thru_hole circle (at -1.27 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 138 SWDIO))
    (pad 1 thru_hole circle (at -2.54 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${SL3DMODEL}/Headers.3dshapes/62201021121.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Header_WE:61302021121 (layer F.Cu) (tedit 5D9F2D91)
    (at 13 -2.9 90)
    (fp_text reference J1 (at -1.4 14 180) (layer F.SilkS))
    (fp_text value 2x10@2.54mm_8.54H_TH (at -8.89 -3.81 90) (layer F.Fab))
    (pad 20 thru_hole circle (at 1.27 11.43 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole circle (at -1.27 11.43 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 18 thru_hole circle (at 1.27 8.89 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at -1.27 8.89 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 B4))
    (pad 16 thru_hole circle (at 1.27 6.35 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 B3))
    (pad 15 thru_hole circle (at -1.27 6.35 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 B2))
    (pad 14 thru_hole circle (at 1.27 3.81 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 B1))
    (pad 13 thru_hole circle (at -1.27 3.81 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 B0))
    (pad 12 thru_hole circle (at 1.27 1.27 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 LCD_EN))
    (pad 11 thru_hole circle (at -1.27 1.27 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 LCD_D5))
    (pad 10 thru_hole circle (at 1.27 -1.27 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 LCD_D0))
    (pad 9 thru_hole circle (at -1.27 -1.27 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 LCD_D1))
    (pad 8 thru_hole circle (at 1.27 -3.81 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 LCD_D2))
    (pad 7 thru_hole circle (at -1.27 -3.81 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 LCD_D3))
    (pad 6 thru_hole circle (at 1.27 -6.35 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 LCD_D6))
    (pad 5 thru_hole circle (at -1.27 -6.35 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 LCD_D6))
    (pad 4 thru_hole circle (at 1.27 -8.89 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 LCD_D5))
    (pad 3 thru_hole circle (at -1.27 -8.89 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 LCD_D4))
    (pad 2 thru_hole circle (at 1.27 -11.43 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.27 -11.43 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${SL3DMODEL}/Headers_WE.3dshapes/61302021121.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_2512 (layer F.Cu) (tedit 5CCCA639)
    (at 69.1 -6.1)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 0 0) (layer F.SilkS))
    (fp_text value 330R_2512_1W_5% (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 129 "Net-(D28-Pad2)"))
    (pad 1 smd roundrect (at -2.9 0) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_2512 (layer F.Cu) (tedit 5CCCA639)
    (at 61.2 -20.1 315)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -0.5 0 135) (layer F.SilkS))
    (fp_text value 1R_2512_1W_5% (at 0 2.62 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 315) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 86 VCC))
    (pad 1 smd roundrect (at -2.9 0 315) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 35 /KL30))
    (model ${SL3DMODEL}/resistor.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 71.4 -1.6 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D28 (at 0 1.5) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(D28-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 5CE6F3D4)
    (at 72.7 -26.5 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C17 (at -0.5 -2 90) (layer F.SilkS))
    (fp_text value 100µ_50_0.16 (at 0 4.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 86 VCC))
    (model ${SL3DMODEL}/capacitor.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-64_10x10mm_P0.5mm (layer F.Cu) (tedit 5B56F227)
    (at 41.1 -10.6 45)
    (descr "TQFP, 64 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_qfp_generator.py")
    (tags "TQFP QFP")
    (attr smd)
    (fp_text reference U13 (at -0.5 0 45) (layer F.SilkS))
    (fp_text value ATSAMC21JA-ANT (at 0 7.35 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 64 smd roundrect (at -3.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 µC_DIAG4))
    (pad 63 smd roundrect (at -3.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 µC_DIAG5))
    (pad 62 smd roundrect (at -2.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 µC_DIAG6))
    (pad 61 smd roundrect (at -2.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 µC_DIAG1))
    (pad 60 smd roundrect (at -1.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 µC_DIAG2))
    (pad 59 smd roundrect (at -1.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 µC_DIAG3))
    (pad 58 smd roundrect (at -0.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 SWDIO))
    (pad 57 smd roundrect (at -0.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 SWCLK))
    (pad 56 smd roundrect (at 0.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 55 smd roundrect (at 0.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(C21-Pad1)"))
    (pad 54 smd roundrect (at 1.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 53 smd roundrect (at 1.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 B4))
    (pad 52 smd roundrect (at 2.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 ~RESET))
    (pad 51 smd roundrect (at 2.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 B2))
    (pad 50 smd roundrect (at 3.25 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 B1))
    (pad 49 smd roundrect (at 3.75 -5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 B0))
    (pad 48 smd roundrect (at 5.6625 -3.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 47 smd roundrect (at 5.6625 -3.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 46 smd roundrect (at 5.6625 -2.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 CAN_RX))
    (pad 45 smd roundrect (at 5.6625 -2.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 CAN_TX))
    (pad 44 smd roundrect (at 5.6625 -1.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 RS485_RW))
    (pad 43 smd roundrect (at 5.6625 -1.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 B3))
    (pad 42 smd roundrect (at 5.6625 -0.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 "Net-(U13-Pad42)"))
    (pad 41 smd roundrect (at 5.6625 -0.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 "Net-(U13-Pad41)"))
    (pad 40 smd roundrect (at 5.6625 0.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 LCD_D5))
    (pad 39 smd roundrect (at 5.6625 0.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 LCD_EN))
    (pad 38 smd roundrect (at 5.6625 1.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 LCD_D6))
    (pad 37 smd roundrect (at 5.6625 1.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 LCD_D6))
    (pad 36 smd roundrect (at 5.6625 2.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 LCD_D5))
    (pad 35 smd roundrect (at 5.6625 2.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 LCD_D4))
    (pad 34 smd roundrect (at 5.6625 3.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 33 smd roundrect (at 5.6625 3.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 32 smd roundrect (at 3.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 LCD_D3))
    (pad 31 smd roundrect (at 3.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 LCD_D2))
    (pad 30 smd roundrect (at 2.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 LCD_D1))
    (pad 29 smd roundrect (at 2.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 LCD_D0))
    (pad 28 smd roundrect (at 1.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 µC_FD3))
    (pad 27 smd roundrect (at 1.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 µC_FD4))
    (pad 26 smd roundrect (at 0.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 µC_FD5))
    (pad 25 smd roundrect (at 0.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 µC_FD6))
    (pad 24 smd roundrect (at -0.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 H_EN))
    (pad 23 smd roundrect (at -0.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 L_EN))
    (pad 22 smd roundrect (at -1.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 21 smd roundrect (at -1.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 20 smd roundrect (at -2.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 µC_PWM6))
    (pad 19 smd roundrect (at -2.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 µC_PWM5))
    (pad 18 smd roundrect (at -3.25 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 µC_PWM4))
    (pad 17 smd roundrect (at -3.75 5.6625 45) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 µC_PWM3))
    (pad 16 smd roundrect (at -5.6625 3.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 µC_PWM2))
    (pad 15 smd roundrect (at -5.6625 3.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 µC_PWM1))
    (pad 14 smd roundrect (at -5.6625 2.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 USART_RX))
    (pad 13 smd roundrect (at -5.6625 2.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 USART_TX))
    (pad 12 smd roundrect (at -5.6625 1.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 µC_FD1))
    (pad 11 smd roundrect (at -5.6625 1.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 µC_FD2))
    (pad 10 smd roundrect (at -5.6625 0.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 "Net-(U13-Pad10)"))
    (pad 9 smd roundrect (at -5.6625 0.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(U13-Pad9)"))
    (pad 8 smd roundrect (at -5.6625 -0.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 7 smd roundrect (at -5.6625 -0.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at -5.6625 -1.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(U13-Pad6)"))
    (pad 5 smd roundrect (at -5.6625 -1.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(U13-Pad5)"))
    (pad 4 smd roundrect (at -5.6625 -2.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(U13-Pad4)"))
    (pad 3 smd roundrect (at -5.6625 -2.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 /SAMC/µC_VCC_SENSE))
    (pad 2 smd roundrect (at -5.6625 -3.25 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 LCD_CON))
    (pad 1 smd roundrect (at -5.6625 -3.75 45) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 FAN_REVERSE))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-64_10x10mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 74.5 -50.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U12 (at 0 -0.1 90) (layer F.SilkS))
    (fp_text value RS485_Transciever (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(C20-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 B))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 A))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 "Net-(R66-Pad2)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 RS485_RW))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 RS485_RW))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 "Net-(R65-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 23.4 -86.4 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U11 (at -0.2 0.3) (layer F.SilkS))
    (fp_text value SN74HC541A (at 0 7.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 19 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 DIAG_EN))
    (pad 18 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 LCD_D4))
    (pad 17 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 LCD_D5))
    (pad 16 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 LCD_D6))
    (pad 15 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 LCD_D6))
    (pad 14 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 LCD_D5))
    (pad 13 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 "Net-(U10-Pad13)"))
    (pad 12 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 "Net-(U11-Pad12)"))
    (pad 11 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 "Net-(U11-Pad11)"))
    (pad 10 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 "Net-(U11-Pad9)"))
    (pad 8 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 "Net-(U11-Pad8)"))
    (pad 7 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 µC_DIAG6))
    (pad 6 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 µC_DIAG5))
    (pad 5 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 µC_DIAG4))
    (pad 4 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 µC_DIAG3))
    (pad 3 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 µC_DIAG2))
    (pad 2 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 µC_DIAG1))
    (pad 1 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 DIAG_EN))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 16.6 -18.2 270)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U10 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value SN74HC541A (at 0 7.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 20 smd roundrect (at 4.65 -5.715 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 19 smd roundrect (at 4.65 -4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 FD_EN))
    (pad 18 smd roundrect (at 4.65 -3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 LCD_D4))
    (pad 17 smd roundrect (at 4.65 -1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 LCD_D5))
    (pad 16 smd roundrect (at 4.65 -0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 LCD_D6))
    (pad 15 smd roundrect (at 4.65 0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 LCD_D6))
    (pad 14 smd roundrect (at 4.65 1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 LCD_D5))
    (pad 13 smd roundrect (at 4.65 3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 "Net-(U10-Pad13)"))
    (pad 12 smd roundrect (at 4.65 4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 "Net-(U10-Pad12)"))
    (pad 11 smd roundrect (at 4.65 5.715 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 "Net-(U10-Pad11)"))
    (pad 10 smd roundrect (at -4.65 5.715 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at -4.65 4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 115 "Net-(U10-Pad9)"))
    (pad 8 smd roundrect (at -4.65 3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 "Net-(U10-Pad8)"))
    (pad 7 smd roundrect (at -4.65 1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 µC_FD6))
    (pad 6 smd roundrect (at -4.65 0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 µC_FD5))
    (pad 5 smd roundrect (at -4.65 -0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 µC_FD4))
    (pad 4 smd roundrect (at -4.65 -1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 µC_FD3))
    (pad 3 smd roundrect (at -4.65 -3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 µC_FD2))
    (pad 2 smd roundrect (at -4.65 -4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 µC_FD1))
    (pad 1 smd roundrect (at -4.65 -5.715 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 FD_EN))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 12 -37.4)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U9 (at 0 0) (layer F.SilkS))
    (fp_text value ATmega644PA-AU (at 0 7.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 µC_PWM6))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 µC_PWM5))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 H_EN))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 103 CAN_CLK))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 75 FAN_REVERSE))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 IO_0))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 91 IO_1))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 92 IO_2))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 93 IO_3))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 B4))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 109 FD_EN))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 110 DIAG_EN))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /µC_VCC_SENSE))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C4-Pad1)"))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 65 LCD_EN))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U10-Pad13)"))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 67 LCD_D5))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 LCD_D6))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 LCD_D6))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 67 LCD_D5))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 68 LCD_D4))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 L_EN))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 µC_PWM4))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 µC_PWM3))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 µC_PWM2))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 µC_PWM1))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 RS485_RW))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 100 CAN_INT))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 74 USART_TX))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 USART_RX))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C6-Pad1)"))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 88 ~RESET))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R56-Pad1)"))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 98 MISO))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 47.8 -42.9 135)
    (descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U8 (at -0.21 0.02 135) (layer F.SilkS))
    (fp_text value MCP2515 (at 0 6.72 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 18 smd roundrect (at 4.65 -5.08 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 17 smd roundrect (at 4.65 -3.81 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(R2-Pad1)"))
    (pad 16 smd roundrect (at 4.65 -2.54 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 CAN_CS))
    (pad 15 smd roundrect (at 4.65 -1.27 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 "Net-(R64-Pad1)"))
    (pad 14 smd roundrect (at 4.65 0 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 MOSI))
    (pad 13 smd roundrect (at 4.65 1.27 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 SCK))
    (pad 12 smd roundrect (at 4.65 2.54 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 CAN_INT))
    (pad 11 smd roundrect (at 4.65 3.81 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(U8-Pad11)"))
    (pad 10 smd roundrect (at 4.65 5.08 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 "Net-(U8-Pad10)"))
    (pad 9 smd roundrect (at -4.65 5.08 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at -4.65 3.81 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 CAN_CLK))
    (pad 7 smd roundrect (at -4.65 2.54 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(U8-Pad7)"))
    (pad 6 smd roundrect (at -4.65 1.27 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(U8-Pad6)"))
    (pad 5 smd roundrect (at -4.65 0 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(U8-Pad5)"))
    (pad 4 smd roundrect (at -4.65 -1.27 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(U8-Pad4)"))
    (pad 3 smd roundrect (at -4.65 -2.54 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(U8-Pad3)"))
    (pad 2 smd roundrect (at -4.65 -3.81 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 CAN_RX))
    (pad 1 smd roundrect (at -4.65 -5.08 135) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 CAN_TX))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Deutsch_DT:DT15-12PB (layer B.Cu) (tedit 5D822D66)
    (at 35 -61 45)
    (fp_text reference U7 (at 4.47 0 225) (layer B.SilkS))
    (fp_text value DT15-12PB (at -5.03 0 225) (layer B.Fab))
    (pad 1 thru_hole circle (at -11.1 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 49 /PWM1_OUT))
    (pad 2 thru_hole circle (at -6.66 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 50 /PWM2_OUT))
    (pad 3 thru_hole circle (at -2.22 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 130 /PWM3_OUT))
    (pad 4 thru_hole circle (at 2.22 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 132 /PWM4_OUT))
    (pad 5 thru_hole circle (at 6.66 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 131 /PWM5_OUT))
    (pad 6 thru_hole circle (at 11.1 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 133 /PWM6_OUT))
    (pad 7 thru_hole circle (at 11.1 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 31 DIAG6))
    (pad 8 thru_hole circle (at 6.66 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 25 DIAG5))
    (pad 9 thru_hole circle (at 2.22 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 29 DIAG4))
    (pad 10 thru_hole circle (at -2.22 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 23 DIAG3))
    (pad 11 thru_hole circle (at -6.66 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 27 DIAG2))
    (pad 12 thru_hole circle (at -11.1 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 21 DIAG1))
    (pad "" np_thru_hole circle (at -17.54 10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.54 10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.54 -10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -17.54 -10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${SL3DMODEL}/Deutsch_DT.3dshapes/DT15-12PB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Deutsch_DT:DT15-12PA (layer B.Cu) (tedit 5D822D46)
    (at 61 -36 45)
    (fp_text reference U6 (at 4.47 0 225) (layer B.SilkS))
    (fp_text value DT15-12PA (at -5.03 0 225) (layer B.Fab))
    (pad "" np_thru_hole circle (at -17.54 -10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.54 -10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.54 10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -17.54 10.67 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -11.1 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at -6.66 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 79 CAN_H))
    (pad 10 thru_hole circle (at -2.22 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 78 CAN_L))
    (pad 9 thru_hole circle (at 2.22 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 73 USART_RX))
    (pad 8 thru_hole circle (at 6.66 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 11.1 -4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 94 B))
    (pad 6 thru_hole circle (at 11.1 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 95 A))
    (pad 5 thru_hole circle (at 6.66 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 75 FAN_REVERSE))
    (pad 4 thru_hole circle (at 2.22 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 74 USART_TX))
    (pad 3 thru_hole circle (at -2.22 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 78 CAN_L))
    (pad 2 thru_hole circle (at -6.66 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 79 CAN_H))
    (pad 1 thru_hole circle (at -11.1 4.56 45) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 35 /KL30))
    (model ${SL3DMODEL}/Deutsch_DT.3dshapes/DT15-12PA.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Header_WE:61300621121 (layer B.Cu) (tedit 5D9F2B1B)
    (at 3.6 -52.4 180)
    (fp_text reference U5 (at 0 -4.5) (layer B.SilkS))
    (fp_text value AVR_ICP (at -0.7 4.8) (layer B.Fab))
    (pad 6 thru_hole circle (at 1.27 -2.54 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -1.27 -2.54 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 88 ~RESET))
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 96 MOSI))
    (pad 3 thru_hole circle (at -1.27 0 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 97 SCK))
    (pad 2 thru_hole circle (at 1.27 2.54 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at -1.27 2.54 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 98 MISO))
    (model ${SL3DMODEL}/Headers_WE.3dshapes/61300621121.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5CE06D78)
    (at 86 -26)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U4 (at -5.2 -0.1) (layer F.SilkS))
    (fp_text value LM2931AD2T−5R4G (at 0 6.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(C17-Pad1)"))
    (pad 1 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:WE-CNSW (layer F.Cu) (tedit 5D8B5A10)
    (at 57.4 -32.4 45)
    (fp_text reference U3 (at 0 0 45) (layer F.SilkS))
    (fp_text value CAN_CMC (at -2 -3 45) (layer F.Fab))
    (pad 4 smd rect (at -1.825 -1.125 45) (size 1.15 1.55) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U2-Pad7)"))
    (pad 3 smd rect (at 1.825 -1.125 45) (size 1.15 1.55) (layers F.Cu F.Paste F.Mask)
      (net 78 CAN_L))
    (pad 2 smd rect (at 1.825 1.125 45) (size 1.15 1.55) (layers F.Cu F.Paste F.Mask)
      (net 79 CAN_H))
    (pad 1 smd rect (at -1.825 1.125 45) (size 1.15 1.55) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U2-Pad6)"))
    (model ${SL3DMODEL}/CM_choke.3dshapes/STEP-WE-CNSW-1812-rev1.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 51.1 -26.2 45)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0.070711 -0.070711 45) (layer F.SilkS))
    (fp_text value "CAN(FD)" (at 0 3.4 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U2-Pad7)"))
    (pad 6 smd roundrect (at 2.475 0.635 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U2-Pad6)"))
    (pad 5 smd roundrect (at 2.475 1.905 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 4 smd roundrect (at -2.475 1.905 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(R68-Pad2)"))
    (pad 3 smd roundrect (at -2.475 0.635 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 2 smd roundrect (at -2.475 -0.635 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.475 -1.905 45) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 "Net-(R67-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:CFPX-218_AUTO (layer F.Cu) (tedit 5D8C8BF2)
    (at 3.552501 -36.210001 270)
    (fp_text reference U1 (at -0.089999 2.252501 90) (layer F.SilkS))
    (fp_text value 16MHz_3x2mm_125C (at -0.5 -3.5 90) (layer F.Fab))
    (pad 4 smd rect (at -0.825 -0.6125 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.825 -0.6125 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.825 0.6125 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.825 0.6125 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C2-Pad1)"))
    (model ${SL3DMODEL}/Crystals.3dshapes/IQXC-180.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5CE1174A)
    (at 60.3 -6 270)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference TVS1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 36V_3KW (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 86 VCC))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 36.5 -73)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R54 (at 0 1.5) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 DIAG6))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 µC_DIAG6))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 30.5 -67.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R53 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 DIAG4))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 µC_DIAG4))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 24.5 -62)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R52 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 DIAG2))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 µC_DIAG2))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 33 -70.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R51 (at 0.5 1.5) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 DIAG5))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 µC_DIAG5))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 27.5 -64.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R50 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 DIAG3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 µC_DIAG3))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 20.5 -58)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R49 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 DIAG1))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 µC_DIAG1))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 58.7 -87.7 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R48 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(Q17-Pad3)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 67.8 -78.8 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R47 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(Q16-Pad3)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 58.9 -76.7 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R46 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(Q15-Pad3)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 55.7 -90.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R45 (at 3.1 0) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(Q17-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 µC_PWM6))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 64.8 -81.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R44 (at 3.1 0.1) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(Q16-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 µC_PWM4))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 55.9 -79.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R43 (at 2.8 0.1) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(Q15-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 µC_PWM2))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 49.4 -87.5 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(Q13-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 65.6 -68 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(Q11-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 49.6 -76.8 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R40 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(Q10-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 46.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at 3.1 0) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(Q8-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 µC_PWM5))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 62.9 -70.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at 3 0.1) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(Q7-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 µC_PWM3))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 46.5 -79.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at 3.2 0) (layer F.SilkS))
    (fp_text value 1K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(Q6-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 µC_PWM1))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_1206 (layer F.Cu) (tedit 5CCCA5A3)
    (at 88.5 -86)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at -3.7 -0.1) (layer F.SilkS))
    (fp_text value 3.9R_1206_5%_660mW (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 41 "Net-(Q5-Pad3)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 82 -92.5 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(Q5-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 80 -92.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 37K_0603_1% (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(Q5-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D15-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 40.3 -19.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 ~RESET))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_2512 (layer F.Cu) (tedit 5CCCA639)
    (at 74 -92.7)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 0 0) (layer F.SilkS))
    (fp_text value 1.2k_2512_0.5W_1% (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 19 "Net-(D15-Pad1)"))
    (pad 1 smd roundrect (at -2.9 0) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 86 VCC))
    (model ${SL3DMODEL}/resistor.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_2512 (layer F.Cu) (tedit 5CCCA639)
    (at 75.8 -82.5 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 0 0) (layer F.SilkS))
    (fp_text value 1.2k_2512_0.5W_1% (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 180) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.9 0 180) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 11 "Net-(D8-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 42 -67.3 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at -2.192031 -0.777817 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 /PWM6_OUT))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 µC_FD6))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 44.4 -67.3 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 2.192031 1.484924 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 /PWM6_OUT))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 38.856847 -64.256847 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at -2.131003 -0.353553 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 /PWM5_OUT))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 µC_FD5))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 41.2 -64.3 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 2.192031 1.202082 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 /PWM5_OUT))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 36 -61.2 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at -2.333452 -0.636396 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 /PWM4_OUT))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 µC_FD4))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 38.2 -61.1 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 2.12132 0.989949 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 /PWM4_OUT))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 85 -74.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q3-Pad3)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 32.656847 -57.956847 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -2.413846 -0.636396 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /PWM3_OUT))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 µC_FD3))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 35 -58 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 2.05061 0.919239 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /PWM3_OUT))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 29.3 -54.8 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.262742 -0.565685 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /PWM2_OUT))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 µC_FD2))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 31.7 -54.8 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 2.333452 0.777817 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /PWM2_OUT))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_1206 (layer F.Cu) (tedit 5CCCA5A3)
    (at 82.3 -77.9 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 0) (layer F.SilkS))
    (fp_text value 3.9R_1206_5%_660mW (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(Q1-Pad3)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(C13-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 26.2 -51.6 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -1.555635 1.555635 45) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /PWM1_OUT))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 µC_FD1))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 28.4 -51.6 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 2.262742 0.989949 135) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 VCC))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /PWM1_OUT))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_1206 (layer F.Cu) (tedit 5CCCA5A3)
    (at 79.6 -50.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 1.7 90) (layer F.SilkS))
    (fp_text value 120_1206_5% (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 94 B))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 95 A))
    (model ${SL3DMODEL}/resistor.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 59.6 -36.3 225)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0.141421 1.272792 45) (layer F.SilkS))
    (fp_text value 68_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 CAN_L))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C18-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 80.8 -82.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.6 0.1 270) (layer F.SilkS))
    (fp_text value 37K_0603_1% (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D8-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q1-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 82.8 -82 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -1.5 2 270) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 61.3 -34.6 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0.141421 1.414214 45) (layer F.SilkS))
    (fp_text value 68_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C18-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 CAN_H))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0805 (layer F.Cu) (tedit 5CCCA387)
    (at 71.6 -14.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.2 0 90) (layer F.SilkS))
    (fp_text value 10K_0805_1% (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /µC_VCC_SENSE))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 67.6 -16.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.5 0 90) (layer F.SilkS))
    (fp_text value 100K_0603_1% (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /µC_VCC_SENSE))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /KL30))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 6.9 -8.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.2 0) (layer F.SilkS))
    (fp_text value 270_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 B3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 IO_3))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 6.9 -10.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.2 0.1) (layer F.SilkS))
    (fp_text value 270_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 B2))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 IO_2))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 6.9 -11.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.2 0.09) (layer F.SilkS))
    (fp_text value 180_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 B1))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 IO_1))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 6.9 -13.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.2 0) (layer F.SilkS))
    (fp_text value 270_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 B0))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 IO_0))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 39.5 -44.9 225)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.212132 1.626346 45) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(R2-Pad1)"))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:R_0603 (layer F.Cu) (tedit 5CCCA351)
    (at 3.2 -42.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.4 0) (layer F.SilkS))
    (fp_text value 10K_0603_1% (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 ~RESET))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/resistor.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 55 -84)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q23 (at 0 2.6) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 133 /PWM6_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q17-Pad3)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 58.7 -84)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q22 (at -0.3 2.6) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 133 /PWM6_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q17-Pad3)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 64.4 -75.2)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q21 (at 0 2.5) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 132 /PWM4_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q16-Pad3)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 68 -75.2)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q20 (at -0.1 2.5) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 132 /PWM4_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q16-Pad3)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 58 -73.1)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q19 (at -0.2 2.6) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 /PWM2_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q15-Pad3)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 54.3 -73.1)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q18 (at -0.3 2.6) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 /PWM2_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q15-Pad3)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 55.9 -87.7 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q17 (at 0 2.4 90) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q17-Pad3)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q17-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 64.9 -78.8 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q16 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q16-Pad3)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q16-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 56 -76.7 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q15 (at -0.1 2.7 90) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q15-Pad3)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Q15-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 49.6 -83.9)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q14 (at -0.3 2.5) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 131 /PWM5_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Q13-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 46 -83.9)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q13 (at 0 2.5) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 131 /PWM5_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Q13-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 65.5 -64.4)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q12 (at -0.2 2.6) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 130 /PWM3_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Q11-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 61.8 -64.4)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q11 (at -0.1 2.6) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 130 /PWM3_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Q11-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 46.2 -73.2)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q10 (at -0.1 2.4) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 /PWM1_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q10-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 49.8 -73.2)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q9 (at 0.4 2.5) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 /PWM1_OUT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q10-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 46.5 -87.5 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 2.4 90) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Q13-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q8-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 62.8 -68 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at -0.1 2.5 90) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Q11-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(Q7-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 46.6 -76.8 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 2.7 90) (layer F.SilkS))
    (fp_text value MMBT5550L (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q6-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer F.Cu) (tedit 5A70A390)
    (at 89 -91)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q5 (at -3.5 0) (layer F.SilkS))
    (fp_text value ZXT1053AKTC (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 40 "/Output Driver/L_RAIL"))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Q5-Pad3)"))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 81.5 -87.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 L_EN))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 89.3 -74.8 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -0.7 2.4 270) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 H_EN))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CEACB71)
    (at 79.1 -75.8 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value MMBT5401LT3G (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 VCC))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${SL3DMODEL}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer F.Cu) (tedit 5A70A390)
    (at 89.3 -80.5)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q1 (at -3 -0.5) (layer F.SilkS))
    (fp_text value MJD32CUQ (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q1-Pad3)"))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 33.5 -77.4 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D27 (at 1.1 2 90) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 µC_DIAG6))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 27 -74.5 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D26 (at 1 -2 90) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 µC_DIAG4))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 20.5 -66.5 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D25 (at 1.5 -2 90) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 µC_DIAG2))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 36.5 -75 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D24 (at -3.2 0.2) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 µC_DIAG6))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 DIAG6))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 29.5 -70.5 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D23 (at -0.5 1.5) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 µC_DIAG4))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 DIAG4))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 23.5 -65 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D22 (at 0 1.5) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 µC_DIAG2))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 DIAG2))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 31 -76.1 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D21 (at 0 -2 90) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 µC_DIAG5))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 24.5 -71.5 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D20 (at 0 -2 90) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 µC_DIAG3))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 17 -63.5 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D19 (at 0 -2 90) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 µC_DIAG1))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 33 -72.5 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D18 (at -0.5 1.7) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 µC_DIAG5))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 DIAG5))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 27 -67.5 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D17 (at 0 1.5) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 µC_DIAG3))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 DIAG3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 20 -61 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D16 (at 0 1.5) (layer F.SilkS))
    (fp_text value 100mA_100V (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 µC_DIAG1))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 DIAG1))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 77 -87.65 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D15 (at -0.15 2.1 270) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D15-Pad1)"))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 41.8 -70 45)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D14 (at -0.070711 -0.070711 45) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 45) (layer F.Fab))
    (fp_text user %R (at 0 -2 45) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 µC_FD6))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 38.2 -66.5 45)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D13 (at 0 0.08 45) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 45) (layer F.Fab))
    (fp_text user %R (at 0 -2 45) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 µC_FD5))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 34.8 -63 45)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D12 (at -0.1 0 45) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 45) (layer F.Fab))
    (fp_text user %R (at 0 -2 45) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 µC_FD4))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 31.3 -59.4 45)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D11 (at 0 0 45) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 45) (layer F.Fab))
    (fp_text user %R (at 0 -2 45) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 µC_FD3))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 27.9 -56.2 45)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D10 (at -0.049497 0.077782 45) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 45) (layer F.Fab))
    (fp_text user %R (at 0 -2 45) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 µC_FD2))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 24.5 -52.8 45)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D9 (at -0.07 0.03 45) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1 45) (layer F.Fab))
    (fp_text user %R (at 0 -2 45) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 45) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 µC_FD1))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 77.55 -79)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D8 (at 0 0) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D8-Pad1)"))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5CEA969C)
    (at 70.9 -17.2)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D7 (at 0 0) (layer F.SilkS))
    (fp_text value 4.7_0.5_5%_SOD-123 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /µC_VCC_SENSE))
    (model ${SL3DMODEL}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD_WE:WL-SMCD (layer F.Cu) (tedit 5DA07424)
    (at 2.3 -8.8)
    (fp_text reference D4 (at 2.14 0.040001) (layer F.SilkS))
    (fp_text value Yellow_0603 (at -2.54 -2.54) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 59 B3))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${SL3DMODEL}/LED_SMD_WE.3dshapes/STEP-WL-SMCD-0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD_WE:WL-SMCD (layer F.Cu) (tedit 5DA07424)
    (at 2.3 -10.3)
    (fp_text reference D3 (at 2.12 0.040001) (layer F.SilkS))
    (fp_text value Green_0603 (at -2.54 -2.54) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 60 B2))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${SL3DMODEL}/LED_SMD_WE.3dshapes/STEP-WL-SMCD-0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD_WE:WL-SMCD (layer F.Cu) (tedit 5DA07424)
    (at 2.3 -11.8)
    (fp_text reference D2 (at 2.1 0.060001) (layer F.SilkS))
    (fp_text value Blue_0603 (at -2.54 -2.54) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 B1))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${SL3DMODEL}/LED_SMD_WE.3dshapes/STEP-WL-SMCD-0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD_WE:WL-SMCD (layer F.Cu) (tedit 5DA07424)
    (at 2.3 -13.2)
    (fp_text reference D1 (at 2.07 0.010001) (layer F.SilkS))
    (fp_text value Red_0603 (at -2.54 -2.54) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 62 B0))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${SL3DMODEL}/LED_SMD_WE.3dshapes/STEP-WL-SMCD-0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:CP_Elec_4x5.7 (layer F.Cu) (tedit 5CE6F193)
    (at 49.3 -3.7 90)
    (descr "SMD capacitor, aluminum electrolytic, United Chemi-Con, 4.0x5.7mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C26 (at -0.2 -1.51 90) (layer F.SilkS))
    (fp_text value 10µ_25_2.1 (at 0 3.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 80.9 -30.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 45.2 -4 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at -2.757716 -0.070711 45) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 43.9 -18.6 315)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 -1.43 135) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 315) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 315) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 34.6 -18.3 45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 2.192031 0.070711 135) (layer F.SilkS))
    (fp_text value 1µ_25_0805_X7R (at 0 1.65 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 45) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 45) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(C21-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 36.1 -16.8 45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.12132 0 135) (layer F.SilkS))
    (fp_text value 100n_25_0805_X7R (at 0 1.65 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 45) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 45) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(C21-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 76.1 -54.1 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -0.1 1.4) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(C20-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:CP_Elec_16x17.5 (layer F.Cu) (tedit 5CE6F52F)
    (at 84.3 -9.9)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1616, 16.0x17.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C19 (at 0 0) (layer F.SilkS))
    (fp_text value 1000µ_50_0.072 (at 0 9.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 6.25 0) (size 7.8 9.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.032051)
      (net 2 GND))
    (pad 1 smd roundrect (at -6.25 0) (size 7.8 9.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.032051)
      (net 139 "Net-(C17-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/CP_Elec_16x17.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 63 -37.3)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100n_25_0805_X7R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C18-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 24.3 -14.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -0.1 1.5 90) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 19.6 -78.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.1 1.5) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 93 -86.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 330n_50_0805_X7R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "/Output Driver/L_RAIL"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 93.3 -76)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0.4 1.5) (layer F.SilkS))
    (fp_text value 330n_50_0805_X7R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "/Output Driver/H_RAIL"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:CP_Elec_4x5.7 (layer F.Cu) (tedit 5CE6F193)
    (at 80.7 -34.4)
    (descr "SMD capacitor, aluminum electrolytic, United Chemi-Con, 4.0x5.7mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C12 (at 0 -1.52) (layer F.SilkS))
    (fp_text value 10µ_25_2.1 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 70.4 -32.7)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 330n_50_0805_X7R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 38.6 -41.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0805 (layer F.Cu) (tedit 5CE03C65)
    (at 79.9 -21.3)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 2.6 -0.1 90) (layer F.SilkS))
    (fp_text value 330n_50_0805_X7R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 139 "Net-(C17-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 12.6 -29.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.1 1.3) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 47.7 -23 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.474874 0.070711 135) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 3.5 -33.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.3 0.2 90) (layer F.SilkS))
    (fp_text value 22p_50_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C6-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 4.1 -39.3 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.1 -1.4 90) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 19.6 -37.7 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C4-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 12.5 -45.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.1 1.3) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 1.3 -38 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.3 -0.2) (layer F.SilkS))
    (fp_text value 22p_50_0603_X7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C2-Pad1)"))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module capacitor:C_0603 (layer F.Cu) (tedit 5CE03C2F)
    (at 71.5 -13)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.5 0) (layer F.SilkS))
    (fp_text value 330n_25_0603_X7R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /µC_VCC_SENSE))
    (model ${SL3DMODEL}/capacitor.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 95 -95) (end 95 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 -95) (end 95 -95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0) (end 0 -95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95 0) (end 0 0) (layer Edge.Cuts) (width 0.05))
)
