(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 400)
    (zones 0)
    (modules 55)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 1.35)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 -153.67)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J2-Pad1)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(J2-Pad5)")
  (net 9 "Net-(J2-Pad7)")
  (net 10 "Net-(J2-Pad10)")
  (net 11 "Net-(J2-Pad11)")
  (net 12 "Net-(J2-Pad13)")
  (net 13 "Net-(J2-Pad15)")
  (net 14 "Net-(J2-Pad17)")
  (net 15 "Net-(J2-Pad19)")
  (net 16 "Net-(J2-Pad21)")
  (net 17 "Net-(J2-Pad23)")
  (net 18 "Net-(J2-Pad25)")
  (net 19 "Net-(J2-Pad27)")
  (net 20 "Net-(J2-Pad29)")
  (net 21 "Net-(J2-Pad31)")
  (net 22 "Net-(J3-Pad1)")
  (net 23 "Net-(J3-Pad3)")
  (net 24 "Net-(J3-Pad5)")
  (net 25 "Net-(J3-Pad7)")
  (net 26 "Net-(J3-Pad10)")
  (net 27 "Net-(J3-Pad11)")
  (net 28 "Net-(J3-Pad13)")
  (net 29 "Net-(J3-Pad15)")
  (net 30 "Net-(J3-Pad17)")
  (net 31 "Net-(J3-Pad19)")
  (net 32 "Net-(J3-Pad21)")
  (net 33 "Net-(J4-Pad3)")
  (net 34 "Net-(JP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad21)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(JP1-Pad1)")
  )
  (module Connector_PinSocket_2.00mm:PinSocket_2x02_P2.00mm_Vertical (layer F.Cu) (tedit 5E4C207B)
    (at 147.828 -121.412)
    (descr "Through hole straight socket strip, 2x02, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x02 2.00mm double row")
    (fp_text reference " " (at -1 -2.5) (layer F.SilkS))
    (fp_text value PinSocket_2x02_P2.00mm_Vertical (at -1 4.5) (layer F.Fab))
    (fp_text user %R (at -1 1 90) (layer F.Fab))
    (pad 4 thru_hole oval (at -2 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at -2 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_2x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5E4C1EF0)
    (at 147.828 -125.095 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "J1 dbg" (at -2.286 4.953) (layer F.SilkS))
    (fp_text value PinHeader_1x04_P2.54mm_Vertical (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23W_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 146.558 -113.792)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W for handsoldering")
    (attr smd)
    (fp_text reference TR3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SOT-23W_Handsoldering (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.7 0) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.7 0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.7 -0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23W_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23W_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 138.557 -113.284 90)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W for handsoldering")
    (attr smd)
    (fp_text reference TR4 (at -4.953 -0.127 90) (layer F.SilkS))
    (fp_text value SOT-23W_Handsoldering (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1.7 0 90) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.7 0.95 90) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.7 -0.95 90) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23W_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23W_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 161.798 -89.154)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W for handsoldering")
    (attr smd)
    (fp_text reference TR2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SOT-23W_Handsoldering (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.7 0) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.7 0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.7 -0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23W_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23W_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 150.749 -96.647)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W for handsoldering")
    (attr smd)
    (fp_text reference TR1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SOT-23W_Handsoldering (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.7 0) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.7 0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.7 -0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23W_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5E472BE3)
    (at 171.226 -112.776 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference "3.3V Sel" (at 0.03 2.413) (layer F.SilkS))
    (fp_text value SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 180) (size 1 1.5) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 1.3 0 180) (size 1 1.5) (layers F.Cu F.Mask))
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 170.942 -105.918)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference "ENBL REG" (at 0 -1.82) (layer F.SilkS))
    (fp_text value D_1206_3216Metric (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 177.038 -101.854)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference VIN (at 1.016 2.286) (layer F.SilkS))
    (fp_text value SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers F.Cu F.Mask))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer F.Cu) (tedit 5E4714B2)
    (at 180.086 -117.602 270)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference " " (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.725 0 270) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 -0.75) (xy 0.5 -0.75) (xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75)
) (width 0))
      ))
    (pad 2 smd custom (at 0.725 0 270) (size 0.3 0.3) (layers F.Cu F.Mask)
      (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0)
) (width 0))
      ))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 180.086 -111.746 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference " " (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (at 0 1.43 90) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 175.26 -104.14)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cp (at 2.794 0.127) (layer F.SilkS))
    (fp_text value C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 177.8 -106.68)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cin (at 2.921 0) (layer F.SilkS))
    (fp_text value C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 176.53 -114.3)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cout (at 0 -1.65) (layer F.SilkS))
    (fp_text value C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 176.53 -110.49 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Gnd (at -4.064 -3.81 90) (layer F.SilkS))
    (fp_text value SOT-23-6_Handsoldering (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -114.3)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -114.3)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 152.908 -115.316)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 152.908 -112.522)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 152.908 -112.522)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 152.908 -109.982)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 161.29 -106.68)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference " " (at 0 -1.75) (layer B.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -106.68)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -106.68)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 161.29 -104.14)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -104.14)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 157.48 -106.68)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference " " (at 0 -1.75) (layer B.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 157.48 -104.14)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 157.48 -109.22)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 161.29 -109.22)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -109.22)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -111.76)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 165.1 -111.76)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference "" (at 0 -1.75) (layer F.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 161.29 -111.76)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference " " (at 0 -1.75) (layer B.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_2x0603 (layer F.Cu) (tedit 58E0A851)
    (at 157.48 -111.76)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference " " (at 0 -1.75) (layer B.SilkS))
    (fp_text value R_Array_Concave_2x0603 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 177.8 -88.265)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P2 (at 0 2.33) (layer B.SilkS))
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 167.64 -88.265)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P1 (at 0 2.33) (layer B.SilkS))
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D1.8mm_W3.3mm_H2.4mm (layer B.Cu) (tedit 5880A862)
    (at 171.45 -88.265)
    (descr "LED, Round,  Rectangular size 3.3x2.4mm^2 diameter 1.8mm, 2 pins")
    (tags "LED Round  Rectangular size 3.3x2.4mm^2 diameter 1.8mm 2 pins")
    (fp_text reference LED (at 1.27 2.26) (layer B.SilkS))
    (fp_text value LED_D1.8mm_W3.3mm_H2.4mm (at 1.27 -2.26) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D1.8mm_W3.3mm_H2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 167.64 -91.44)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference REF** (at 3.81 2.37) (layer B.SilkS))
    (fp_text value R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 171.45 -92.71)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 2.54 0) (layer B.SilkS))
    (fp_text value R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (at 3.81 -2.37) (layer B.Fab))
    (fp_text user %R (at 3.81 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A434)
    (at 157.48 -101.6)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference P3 (at 0 2.77) (layer B.SilkS))
    (fp_text value PinSocket_1x01_P2.54mm_Vertical (at -0.254 -2.54) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A434)
    (at 173.99 -96.52)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference " " (at 0 2.77) (layer B.SilkS))
    (fp_text value PinSocket_1x01_P2.54mm_Vertical (at 0 -2.77) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H13mm (layer B.Cu) (tedit 5A02FE31)
    (at 161.29 -96.52)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=13mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 2) (layer B.SilkS))
    (fp_text value SW_PUSH_6mm_H13mm (at -2.54 -1.778) (layer B.Fab))
    (fp_text user %R (at 3.25 -2.25) (layer B.Fab))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 -4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H13mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:EFM8BB31F64G-QFP32 (layer B.Cu) (tedit 0)
    (at 146.05 -105.41 90)
    (fp_text reference U1 (at -2.3749 2.0828) (layer B.SilkS))
    (fp_text value EFM8BB31F64G-QFP32 (at -6.1214 0.5207 unlocked) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User))
    (fp_text user * (at -3.1242 3.2 270) (layer B.Fab))
    (fp_text user 0.031in/0.8mm (at 7.5438 2.4 270) (layer Dwgs.User))
    (fp_text user 0.02in/0.508mm (at 2.8 7.5438 270) (layer Dwgs.User))
    (fp_text user 0.058in/1.473mm (at 9.0932 4.1148 270) (layer Dwgs.User))
    (fp_text user 0.324in/8.23mm (at -9.0932 0 270) (layer Dwgs.User))
    (fp_text user 0.324in/8.23mm (at 0 -8.8138 270) (layer Dwgs.User))
    (fp_text user * (at -3.1242 3.2 270) (layer B.Fab))
    (pad 1 smd rect (at -4.1148 2.799999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -4.1148 2.000001) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -4.1148 1.2) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -4.1148 0.399999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -4.1148 -0.399999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at -4.1148 -1.2) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 7 smd rect (at -4.1148 -1.999999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 8 smd rect (at -4.1148 -2.799999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J3-Pad3)"))
    (pad 9 smd rect (at -2.799999 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 10 smd rect (at -2.000001 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 11 smd rect (at -1.2 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J3-Pad10)"))
    (pad 12 smd rect (at -0.399999 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J3-Pad11)"))
    (pad 13 smd rect (at 0.399999 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J3-Pad13)"))
    (pad 14 smd rect (at 1.2 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J3-Pad15)"))
    (pad 15 smd rect (at 1.999999 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J3-Pad17)"))
    (pad 16 smd rect (at 2.799999 -4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J3-Pad19)"))
    (pad 17 smd rect (at 4.1148 -2.799999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J3-Pad21)"))
    (pad 18 smd rect (at 4.1148 -2.000001) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J2-Pad31)"))
    (pad 19 smd rect (at 4.1148 -1.2) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J2-Pad29)"))
    (pad 20 smd rect (at 4.1148 -0.399999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J2-Pad27)"))
    (pad 21 smd rect (at 4.1148 0.399999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J2-Pad25)"))
    (pad 22 smd rect (at 4.1148 1.2) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J2-Pad23)"))
    (pad 23 smd rect (at 4.1148 1.999999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J2-Pad21)"))
    (pad 24 smd rect (at 4.1148 2.799999) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J2-Pad19)"))
    (pad 25 smd rect (at 2.799999 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J2-Pad17)"))
    (pad 26 smd rect (at 2.000001 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J2-Pad15)"))
    (pad 27 smd rect (at 1.2 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J2-Pad13)"))
    (pad 28 smd rect (at 0.399999 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J2-Pad11)"))
    (pad 29 smd rect (at -0.399999 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 30 smd rect (at -1.2 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 31 smd rect (at -1.999999 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 32 smd rect (at -2.799999 4.1148 90) (size 0.508 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad3)"))
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer B.Cu) (tedit 5AE50EF0)
    (at 158.75 -118.11 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C1 (at 3.75 2.67 270) (layer B.SilkS))
    (fp_text value 4.7uf (at 3.75 -2.67 270) (layer B.Fab))
    (fp_text user %R (at 3.75 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer B.Cu) (tedit 5AE50EF0)
    (at 154.94 -118.11 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C2 (at 3.75 2.67 270) (layer B.SilkS))
    (fp_text value .01uf (at 3.75 -2.67 270) (layer B.Fab))
    (fp_text user %R (at 3.75 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer B.Cu) (tedit 5AE50EF0)
    (at 151.13 -118.11 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C3 (at 3.75 2.67 270) (layer B.SilkS))
    (fp_text value "1 uf" (at 3.75 -2.67 270) (layer B.Fab))
    (fp_text user %R (at 3.75 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O6.35mm_Z8.2mm (layer B.Cu) (tedit 5880A863)
    (at 162.56 -118.11)
    (descr "LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins")
    (tags "LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins")
    (fp_text reference D1 (at 1.27 1.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -10.41) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O6.35mm_Z8.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x16_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 182.8419 -87.6554)
    (descr "Through hole straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x16 2.54mm double row")
    (fp_text reference J2 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value "Port 0 and 1" (at 1.27 -40.43) (layer B.Fab))
    (fp_text user %R (at 1.27 -19.05 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad11)"))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad13)"))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad15)"))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad17)"))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad19)"))
    (pad 21 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad21)"))
    (pad 23 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad23)"))
    (pad 25 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad25)"))
    (pad 27 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad27)"))
    (pad 29 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad29)"))
    (pad 31 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad31)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x12_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 130.81 -87.63)
    (descr "Through hole straight pin header, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x12 2.54mm double row")
    (fp_text reference J3 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value Conn_02x12_Odd_Even (at 1.27 -30.27) (layer B.Fab))
    (fp_text user %R (at 1.27 -13.97 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad3)"))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad10)"))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad11)"))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad13)"))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad15)"))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad17)"))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad19)"))
    (pad 21 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad21)"))
    (pad 23 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole oval (at 2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer B.Cu) (tedit 5E471B37)
    (at 171.45 -118.11 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J4 (at -8.45 -5.75 270) (layer B.SilkS))
    (fp_text value Power (at -6.2 5.5 270) (layer B.Fab))
    (fp_text user %R (at -3 2.95 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask))
    (pad 2 thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 thru_hole roundrect (at -3 -4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 142.24 -92.71 270)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J5 (at 5.655 2.27 270) (layer B.SilkS))
    (fp_text value "Ground and power" (at 5.655 -14.97 270) (layer B.Fab))
    (fp_text user %R (at 5.31 -6.35) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5B78013E)
    (at 130.81 -121.92)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference JP1 (at 1.27 4.12) (layer B.SilkS))
    (fp_text value Jumper (at 1.27 -4.08) (layer B.Fab))
    (fp_text user %R (at 1.27 2.22) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 34 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 137.16 -118.11 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 2.37 270) (layer B.SilkS))
    (fp_text value 1K (at 3.81 -2.37 270) (layer B.Fab))
    (fp_text user %R (at 3.81 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical (layer B.Cu) (tedit 5AE5139B)
    (at 161.29 -114.3 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=5.08mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 5.08mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 2.54 2.37) (layer B.SilkS))
    (fp_text value 470 (at 2.54 -2.37) (layer B.Fab))
    (fp_text user %R (at 2.54 2.37) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 190.5127 -129.413) (end 190.5 -85.09) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 -129.413) (end 190.5127 -129.413) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 -85.09) (end 127 -129.413) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 190.5 -85.09) (end 127 -85.09) (layer Edge.Cuts) (width 0.05))
)
